(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(uuid "4e49d584-f650-4a4e-ae26-e0322eda8233")
	(paper "A4")
	(lib_symbols
		(symbol "Connector_Generic:Conn_01x02"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "Conn_01x02"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "Conn_01x02_1_1"
				(rectangle
					(start -1.27 1.27)
					(end 1.27 -3.81)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(rectangle
					(start -1.27 0.127)
					(end 0 -0.127)
					(stroke
						(width 0.1524)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.27 -2.413)
					(end 0 -2.667)
					(stroke
						(width 0.1524)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 3.81)
					(name "Pin_1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 3.81)
					(name "Pin_2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "R"
				(at 0 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "MCU_ST_STM32C0:STM32C071GBUxN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 24.13 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "STM32C071GBUxN"
				(at 5.08 24.13 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
				(at -10.16 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify right)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071gb.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 25 GPIO, UFQFPN28_N"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "Arm Cortex-M0+ STM32C0 STM32C0x1"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "STM32C071GBUxN_0_1"
				(rectangle
					(start -10.16 -20.32)
					(end 10.16 22.86)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
			)
			(symbol "STM32C071GBUxN_1_1"
				(pin bidirectional line
					(at -12.7 17.78 0)
					(length 2.54)
					(name "PF2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "RCC_MCO" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "PC14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "RCC_OSCX_IN" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_BKIN2" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "PC15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "RCC_OSC32_EN" bidirectional line)
					(alternate "RCC_OSCX_OUT" bidirectional line)
					(alternate "RCC_OSC_EN" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "PB0"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN17" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "PB1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN18" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "PB3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "23"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "PB4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "24"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "PB5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "25"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "PWR_WKUP6" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM16_BKIN" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "PB6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "26"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "PWR_WKUP3" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM16_BKIN" bidirectional line)
					(alternate "TIM16_CH1N" bidirectional line)
					(alternate "TIM17_BKIN" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "PB7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "27"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "I2C1_SDA" bidirectional line)
					(alternate "RTC_REFIN" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "PB8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "28"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C1_SCL" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin power_in line
					(at 0 25.4 270)
					(length 2.54)
					(name "VDD"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -22.86 90)
					(length 2.54)
					(name "VSS"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 2.54 25.4 270)
					(length 2.54)
					(name "VDDIO2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "17"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 12.7 17.78 180)
					(length 2.54)
					(name "PA0"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN0" bidirectional line)
					(alternate "PWR_WKUP1" bidirectional line)
					(alternate "SPI2_SCK" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART1_TX" bidirectional line)
					(alternate "USART2_CTS" bidirectional line)
					(alternate "USART2_NSS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "PA1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN1" bidirectional line)
					(alternate "I2C1_SMBA" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH2" bidirectional line)
					(alternate "TIM2_CH2" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USART2_CK" bidirectional line)
					(alternate "USART2_DE" bidirectional line)
					(alternate "USART2_RTS" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 12.7 180)
					(length 2.54)
					(name "PA2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN2" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "PWR_WKUP4" bidirectional line)
					(alternate "RCC_LSCO" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM16_CH1N" bidirectional line)
					(alternate "TIM1_CH3" bidirectional line)
					(alternate "TIM2_CH3" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 10.16 180)
					(length 2.54)
					(name "PA3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "9"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN3" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "TIM2_CH4" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 7.62 180)
					(length 2.54)
					(name "PA4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "10"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN4" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "PWR_WKUP2" bidirectional line)
					(alternate "RTC_OUT1" bidirectional line)
					(alternate "RTC_TS" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI2_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM17_CH1N" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "PA5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "11"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN5" bidirectional line)
					(alternate "I2S1_CK" bidirectional line)
					(alternate "SPI1_SCK" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "PA6"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN6" bidirectional line)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM16_CH1" bidirectional line)
					(alternate "TIM1_BKIN" bidirectional line)
					(alternate "TIM3_CH1" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "PA7"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN7" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM17_CH1" bidirectional line)
					(alternate "TIM1_CH1N" bidirectional line)
					(alternate "TIM3_CH2" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "PA8"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "16"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN8" bidirectional line)
					(alternate "CRS_SYNC" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RCC_MCO" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "SPI2_MISO" bidirectional line)
					(alternate "SPI2_NSS" bidirectional line)
					(alternate "TIM14_CH1" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM1_CH2N" bidirectional line)
					(alternate "TIM1_CH3N" bidirectional line)
					(alternate "TIM3_CH3" bidirectional line)
					(alternate "TIM3_CH4" bidirectional line)
					(alternate "USART1_RX" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "PA11"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "18"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_EXTI11" bidirectional line)
					(alternate "I2C2_SCL" bidirectional line)
					(alternate "I2S1_MCK" bidirectional line)
					(alternate "SPI1_MISO" bidirectional line)
					(alternate "TIM1_BKIN2" bidirectional line)
					(alternate "TIM1_CH4" bidirectional line)
					(alternate "USART1_CTS" bidirectional line)
					(alternate "USART1_NSS" bidirectional line)
					(alternate "USB_DM" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "PA12"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "19"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2C2_SDA" bidirectional line)
					(alternate "I2S1_SD" bidirectional line)
					(alternate "I2S_CKIN" bidirectional line)
					(alternate "SPI1_MOSI" bidirectional line)
					(alternate "TIM1_ETR" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USB_DP" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "PA13"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "20"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN13" bidirectional line)
					(alternate "DEBUG_SWDIO" bidirectional line)
					(alternate "IR_OUT" bidirectional line)
					(alternate "TIM3_ETR" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "PA14"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "21"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "ADC1_IN14" bidirectional line)
					(alternate "DEBUG_SWCLK" bidirectional line)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USART2_TX" bidirectional line)
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "PA15"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "22"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(alternate "I2S1_WS" bidirectional line)
					(alternate "RCC_MCO2" bidirectional line)
					(alternate "SPI1_NSS" bidirectional line)
					(alternate "TIM1_CH1" bidirectional line)
					(alternate "TIM2_CH1" bidirectional line)
					(alternate "TIM2_ETR" bidirectional line)
					(alternate "USART1_CK" bidirectional line)
					(alternate "USART1_DE" bidirectional line)
					(alternate "USART1_RTS" bidirectional line)
					(alternate "USART2_RX" bidirectional line)
					(alternate "USB_NOE" bidirectional line)
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistor_FET:AO3400A"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "AO3400A"
				(at 5.08 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
				(at 5.08 -1.905 0)
				(effects
					(font
						(size 1.27 1.27)
						(italic yes)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf"
				(at 5.08 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Description" "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "N-Channel MOSFET"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "AO3400A_0_1"
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.778) (xy 3.302 -1.778) (xy 3.302 1.778) (xy 0.762 1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 0) (xy 2.032 0.381) (xy 2.032 -0.381) (xy 1.016 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.921 0.381) (xy 3.683 0.381)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 0.381) (xy 2.921 -0.254) (xy 3.683 -0.254) (xy 3.302 0.381)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "AO3400A_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "Transistor_FET:AO3401A"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "AO3401A"
				(at 5.08 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
				(at 5.08 -1.905 0)
				(effects
					(font
						(size 1.27 1.27)
						(italic yes)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
				(at 5.08 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "P-Channel MOSFET"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "AO3401A_0_1"
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 1.778) (xy 3.302 1.778) (xy 3.302 -1.778) (xy 0.762 -1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 0) (xy 1.27 0.381) (xy 1.27 -0.381) (xy 2.286 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 -0.508) (xy 2.921 -0.381) (xy 3.683 -0.381) (xy 3.81 -0.254)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 -0.381) (xy 2.921 0.254) (xy 3.683 0.254) (xy 3.302 -0.381)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "AO3401A_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Capacitors:C0402_1uF_35V_X5R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 5.08 3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "C0402_1uF_35V_X5R"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Footprint" "VL_Capacitors:C0402"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf?ref_disty=digikey"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Capacitor; Footprint 0402; 1uF/35V; X5R"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Capacitance" "1uF"
				(at 5.08 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Voltage" "35V"
				(at 5.08 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Dielectric" "X5R"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "TDK Corporation"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "C1005X5R1V105K050BE"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "445-175218-1-ND"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "810-C1005X5R1V105K"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "3416060"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "X"
				(at 0 -22.86 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "Kyocera International Inc. Electronic Components"
				(at 22.86 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "CM05X5R105K35AH"
				(at 22.86 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "C0402_1uF_35V_X5R_1_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(stroke
						(width 0.508)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(stroke
						(width 0.508)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Capacitors:C0603_100nF_50V_X7R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 5.08 3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "C0603_100nF_50V_X7R"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Footprint" "VL_Capacitors:C0603"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "http://www.samsungsem.com/kr/support/product-search/mlcc/CL10B104KB8NNNC.jsp"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Capacitor; Footprint 0603; 100nF/50V; X7R"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Capacitance" "100nF"
				(at 6.35 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Voltage" "50V"
				(at 5.08 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Dielectric" "X7R"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Samsung Electro-Mechanics"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "CL10B104KB8NNNC"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "1276-1000-1-ND"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "187-CL10B104KB8NNNC"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "1301804"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "CL10B104KB8NNNC"
				(at 0 -22.86 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "AVX Corporation"
				(at 24.13 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "06035C104KAT4A"
				(at 24.13 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "C0603_100nF_50V_X7R_1_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(stroke
						(width 0.508)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(stroke
						(width 0.508)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Capacitors:C0603_10uF_16V_X5R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 5.08 3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "C0603_10uF_16V_X5R"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Footprint" "VL_Capacitors:C0603"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Capacitor; Footprint 0603; 10uF/16V; X5R"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Capacitance" "10uF"
				(at 5.08 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Voltage" "16V"
				(at 5.08 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Dielectric" "X5R"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Taiyo Yuden"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "EMK107BBJ106MA-T"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "587-3238-1-ND"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "963-EMK107BBJ106MA-T"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "2779064"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "CL10A106MO8NQNC"
				(at 0 -22.86 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "Murata Electronics"
				(at 24.13 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "GRM188R61C106MA73D"
				(at 24.13 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "C0603_10uF_16V_X5R_1_1"
				(polyline
					(pts
						(xy -2.032 0.762) (xy 2.032 0.762)
					)
					(stroke
						(width 0.508)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.032 -0.762) (xy 2.032 -0.762)
					)
					(stroke
						(width 0.508)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Capacitors:CP2917_330uF_6.3V_Polymer"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.81 2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "CP2917_330uF_6.3V_Polymer"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Footprint" "VL_Capacitors:CP_EIA-7343-15_Kemet-W"
				(at 0.9652 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/ABE0000/ABE0000C106.pdf"
				(at -3.81 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "330 µF 6.3 V Aluminum - Polymer Capacitors 2917 (7343 Metric) 9mOhm 2000 Hrs @ 85°C"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Capacitance" "330uF"
				(at 6.35 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Voltage" "6.3V"
				(at 5.08 -2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Manufacturer" "Panasonic Electronic Components"
				(at -1.27 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "ECG-SY0J331R"
				(at 0 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "Panasonic Electronic Components"
				(at -1.27 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "ECG-CY0J331R"
				(at 0 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "P122483CT-ND"
				(at 0 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "667-ECG-SY0J331R"
				(at 0 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "2831753"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "X"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "cap capacitor"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "CP_*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "CP2917_330uF_6.3V_Polymer_0_1"
				(rectangle
					(start -2.286 0.508)
					(end 2.286 1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 2.286) (xy -0.762 2.286)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 2.794) (xy -1.27 1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.286 -0.508)
					(end -2.286 -1.016)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "CP2917_330uF_6.3V_Polymer_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.794)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Connectors:SWD_Connector"
			(pin_names
				(offset 0.0254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SWD"
				(at 2.54 7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "SWD_Connector"
				(at 1.27 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" "VL_Connectors:SWD_Connector_for_PogoHeader"
				(at 1.27 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" ""
				(at -11.43 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "SMD Connector for programming ARM MCUs using a spring-loaded header"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "X"
				(at 1.27 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "X"
				(at 1.27 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "X"
				(at 1.27 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "X"
				(at 1.27 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "SWD_Connector_0_1"
				(rectangle
					(start 0 6.35)
					(end 6.35 -6.35)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type background)
					)
				)
			)
			(symbol "SWD_Connector_1_1"
				(pin bidirectional line
					(at -2.54 5.08 0)
					(length 2.54)
					(name "3V3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at -2.54 2.54 0)
					(length 2.54)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -2.54 0 0)
					(length 2.54)
					(name "SWDIO"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -2.54 -2.54 0)
					(length 2.54)
					(name "SWCLK"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -2.54 -5.08 0)
					(length 2.54)
					(name "NRST"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Connectors:UE27AC54100"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -5.08 11.43 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "UE27AC54100"
				(at -5.08 8.89 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "VL_Connectors:AMPHENOL_UE27AC54100"
				(at 3.81 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/pue27acx4x0x.pdf"
				(at 3.81 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "USB Type A connector"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Amphenol ICC (Commercial Products)"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "UE27AC54100"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "UE27AC54100-ND"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "523-UE27-AC54-100"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "2709068"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "UE27AC54100"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "connector USB"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "USB*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "UE27AC54100_0_1"
				(rectangle
					(start -5.08 -7.62)
					(end 5.08 7.62)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(circle
					(center -3.81 2.159)
					(radius 0.635)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -3.175 2.159) (xy -2.54 2.159) (xy -1.27 3.429) (xy -0.635 3.429)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.159) (xy -1.905 2.159) (xy -1.27 0.889) (xy 0 0.889)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.524 4.826)
					(end -4.318 5.334)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 4.572)
					(end -4.572 5.842)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center -0.635 3.429)
					(radius 0.381)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -0.127 -7.62)
					(end 0.127 -6.858)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 0.254 1.27)
					(end -0.508 0.508)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0.635 2.794) (xy 0.635 1.524) (xy 1.905 2.159) (xy 0.635 2.794)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 5.08 4.953)
					(end 4.318 5.207)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 -0.127)
					(end 4.318 0.127)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 5.08 -2.667)
					(end 4.318 -2.413)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "UE27AC54100_1_1"
				(polyline
					(pts
						(xy -1.905 2.159) (xy 0.635 2.159)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -2.54 -10.16 90)
					(length 2.54)
					(name "Shield"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -10.16 90)
					(length 2.54)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 7.62 5.08 180)
					(length 2.54)
					(name "VBUS"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 7.62 0 180)
					(length 2.54)
					(name "D+"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin bidirectional line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "D-"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Diodes:PESD1CAN"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 6.35 2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "PESD1CAN"
				(at 12.065 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" "VL_SOT:SOT-23"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://4donline.ihs.com/images/VipMasterIC/IC/NEXP/NEXP-S-A0005722386/NEXP-S-A0005722386-1.pdf?hkey=6D3A4C79FDBF58556ACFDE234799DDF0"
				(at -1.27 15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "TVS DIODE 24VWM 70VC SOT-23-3"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Nexperia USA Inc."
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "PESD1CAN,215 "
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "EVVO"
				(at 25.4 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "PESD1CAN"
				(at 24.13 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "5272-PESD1CANCT-ND"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "771-PESD1CAN-T/R"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "1510703"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "PESD1CAN,215 "
				(at 0 -22.86 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "PESD1CAN_0_1"
				(polyline
					(pts
						(xy -1.27 2.54) (xy -3.81 2.54) (xy -2.54 1.27) (xy -1.27 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "PESD1CAN_1_1"
				(rectangle
					(start -5.08 3.81)
					(end 5.08 -2.54)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 1.524) (xy -3.556 1.27) (xy -1.524 1.27) (xy -1.27 1.016)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 0) (xy -1.27 0) (xy -2.54 1.27) (xy -3.81 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.54) (xy -2.54 3.81)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 0) (xy -2.54 -1.27) (xy 2.54 -1.27) (xy 2.54 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 0 -1.27)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.524) (xy 1.524 1.27) (xy 3.556 1.27) (xy 3.81 1.016)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 3.81 0) (xy 2.54 1.27) (xy 1.27 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 3.81)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 2.54) (xy 1.27 2.54) (xy 2.54 1.27) (xy 3.81 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(pin input line
					(at -2.54 6.35 270)
					(length 2.54)
					(name "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at 0 -5.08 90)
					(length 2.54)
					(name "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at 2.54 6.35 270)
					(length 2.54)
					(name "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Other:0ZCJ0050AF2E"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "F"
				(at 0 5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "0ZCJ0050AF2E"
				(at 0 -2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" "VL_Other:F1206"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://cz.mouser.com/datasheet/2/643/ds_CP_0zcj_series-1664160.pdf"
				(at 0 5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Polymeric PTC Resettable Fuse 24V 500mA Ih Surface Mount 1206 (3216 Metric)"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Bel Fuse Inc."
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "0ZCJ0050AF2E"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "Eaton - Electronics Division"
				(at 26.67 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "PTS120615V050"
				(at 27.94 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "507-1803-1-ND"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "530-0ZCJ0050AF2E"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "2834888"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" " 0ZCJ0050AF2E"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "0ZCJ0050AF2E_1_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 2.54 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.54 -0.762)
					(end -2.54 0.762)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Other:MF-PSML300/6-2"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "F"
				(at 0 2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "MF-PSML300{slash}6-2"
				(at 0 -2.54 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" "VL_Other:F0805"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.bourns.com/docs/product-datasheets/mf-nsml-x.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Polymeric PTC Resettable Fuse 6V 3 A Ih Surface Mount 0805 (2012 Metric), Concave"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Bourns Inc."
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "MF-PSML300/6-2"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "Littelfuse Inc."
				(at 26.67 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "0805L300SLWR"
				(at 27.94 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "118-MF-PSML300/6-2CT-ND"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "652-MF-PSML300/6-2"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "3131611"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "X"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "MF-PSML300/6-2_1_1"
				(polyline
					(pts
						(xy -2.54 0) (xy 2.54 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.54 -0.762)
					(end -2.54 0.762)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_PMICs:MIC5504-3.3YM5-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 0 7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "MIC5504-3.3YM5-TR"
				(at 0 5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" "VL_SOT:SOT-23-5"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC5501-02-03-04-300mA-Single-Output-LDO-in-Small-Packages-DS20006006B.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Linear Voltage Regulator IC Positive Fixed 3.3V Output 300mA SOT-23-5"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "MIC5504-3.3YM5-TR"
				(at 1.27 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "576-4764-1-ND"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "998-MIC5504-3.3YM5TR"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "2510377"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "MIC5504-3.3YM5-TR"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "MIC5504-3.3YM5-TR_1_1"
				(rectangle
					(start -6.35 3.81)
					(end 6.35 -3.81)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type background)
					)
				)
				(pin power_in line
					(at -8.89 2.54 0)
					(length 2.54)
					(name "VIN"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input input_low
					(at -8.89 -2.54 0)
					(length 2.54)
					(name "EN"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at 0 -6.35 90)
					(length 2.54)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_out line
					(at 8.89 2.54 180)
					(length 2.54)
					(name "VOUT"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin no_connect non_logic
					(at 8.89 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "NC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Resistors:R0402_10k_5%_1d16W"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "R0402_10k_5%_1d16W"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Footprint" "VL_Resistors:R0402"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Resistance" "10k"
				(at 3.81 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Power" "1/16W"
				(at 7.62 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Precision" "5%"
				(at 7.62 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Yageo"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "RC0402JR-0710KL"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "Stackpole Electronics Inc"
				(at 20.32 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "RMCF0402JT10K0"
				(at 20.32 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "311-10KJRCT-ND"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "603-RC0402JR-0710KL"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "*"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "SMD0402-10K"
				(at 0 -22.86 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "R0402_10k_5%_1d16W_1_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Resistors:R0402_1k_1%_1d16W"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "R0402_1k_1%_1d16W"
				(at 0 -5.08 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Footprint" "VL_Resistors:R0402"
				(at 0 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Resistance" "1k"
				(at 2.54 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Power" "1/16W"
				(at 7.62 1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Precision" "1%"
				(at 7.62 -1.27 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Yageo"
				(at 0 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "AC0402FR-071KL"
				(at 0 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Manufacturer" "TE Connectivity Passive Product"
				(at 20.32 -10.16 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Alt_Code" "CRGCQ0402F1K0"
				(at 20.32 -12.7 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "311-1KLBCT-ND"
				(at 0 -15.24 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "603-AC0402FR-071KL"
				(at 0 -17.78 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "3495181"
				(at 0 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "SMD0402-1K-1%"
				(at 0 -22.86 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "R0402_1k_1%_1d16W_1_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "VL_Transistors:2N7002NXAKR"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 5.08 1.905 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "2N7002NXAKR"
				(at 5.08 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Footprint" "VL_SOT:SOT-23"
				(at -6.35 -13.97 0)
				(effects
					(font
						(size 1.27 1.27)
						(italic yes)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/2N7002NXAK.pdf"
				(at -20.32 -7.62 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
					(hide yes)
				)
			)
			(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Manufacturer" "Nexperia USA Inc."
				(at 0 -8.89 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Code" "2N7002NXAKR"
				(at 0 -11.43 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Digikey" "1727-8643-1-ND"
				(at 0 -16.51 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Mouser" "771-2N7002NXAKR"
				(at 0 -19.05 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Farnell" "3226400"
				(at 0 -24.13 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "TME" "2N7002NXAKR"
				(at 0 -21.59 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "N-Channel Switching MOSFET"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_fp_filters" "SOT?23*"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "2N7002NXAKR_0_1"
				(polyline
					(pts
						(xy 0.254 1.905) (xy 0.254 -1.905)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.254 0) (xy -2.54 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 2.286) (xy 0.762 1.27)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 0.508) (xy 0.762 -0.508)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.27) (xy 0.762 -2.286)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.762 -1.778) (xy 3.302 -1.778) (xy 3.302 1.778) (xy 0.762 1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 0) (xy 2.032 0.381) (xy 2.032 -0.381) (xy 1.016 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 1.651 0)
					(radius 2.794)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 1.778)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.54 1.778)
					(radius 0.254)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(circle
					(center 2.54 -1.778)
					(radius 0.254)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 2.54 0) (xy 0.762 0)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 0.508) (xy 2.921 0.381) (xy 3.683 0.381) (xy 3.81 0.254)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.302 0.381) (xy 2.921 -0.254) (xy 3.683 -0.254) (xy 3.302 0.381)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "2N7002NXAKR_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "G"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 2.54 5.08 270)
					(length 2.54)
					(name "D"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 2.54 -5.08 90)
					(length 2.54)
					(name "S"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
				(effects
					(font
						(size 1.27 1.27)
					)
					(hide yes)
				)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
	)
	(text "3 A"
		(exclude_from_sim no)
		(at 62.23 48.006 0)
		(effects
			(font
				(size 1.27 1.27)
			)
		)
		(uuid "335bf0b8-8022-41f0-9e64-b9bc0abc5b74")
	)
	(junction
		(at 195.58 114.3)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "1c076050-528a-4abb-80cd-db09e34a27d6")
	)
	(junction
		(at 204.47 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "1ccc9e04-1783-4a59-8a4f-601c45858fb6")
	)
	(junction
		(at 217.17 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "22ac8084-bac5-472d-9b7d-ab7942b209f5")
	)
	(junction
		(at 240.03 114.3)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "23f921de-846e-4a12-ae99-1e778384f075")
	)
	(junction
		(at 256.54 100.33)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "25133076-ce85-497b-a510-847dcada30ab")
	)
	(junction
		(at 160.02 45.72)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "3a41e2d5-496a-4c70-9b1b-205b51440d13")
	)
	(junction
		(at 168.91 39.37)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "3e0787d4-21d5-4d4c-aeaa-c922fe948b89")
	)
	(junction
		(at 195.58 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "401abe20-d221-4491-bf85-039093d0cff4")
	)
	(junction
		(at 231.14 91.44)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "48fb40dd-0780-492f-ab99-46dc021741b5")
	)
	(junction
		(at 208.28 58.42)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "512a6622-863c-466d-a618-4d9ee9628792")
	)
	(junction
		(at 240.03 49.53)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "55a9e693-c545-4036-85fb-cb93cab66d68")
	)
	(junction
		(at 104.14 45.72)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "6713c232-0f1b-4de0-bb18-b6deae807723")
	)
	(junction
		(at 256.54 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "7a7df891-4c03-43c3-886c-0cf55be22ac7")
	)
	(junction
		(at 179.07 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "7c53f903-7157-4bac-9b72-7ab91d869d5a")
	)
	(junction
		(at 240.03 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "84141c0a-4f06-4e56-9d53-07370fb10d88")
	)
	(junction
		(at 218.44 58.42)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "8cfc6083-bf7d-48df-925d-15981f9fddba")
	)
	(junction
		(at 265.43 106.68)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "9ab1f803-8fa1-4931-9693-86e330dffe5f")
	)
	(junction
		(at 168.91 60.96)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "a1c5d8ef-1dd0-4354-835b-67b0f8a7ef14")
	)
	(junction
		(at 81.28 45.72)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "a821a7e7-38e2-4058-9d5d-579d5ee95cb3")
	)
	(junction
		(at 218.44 49.53)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "b8cd3d83-c978-4e65-8fd1-4d0fc9814176")
	)
	(junction
		(at 231.14 121.92)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "d307d396-e1dd-4fd4-a739-99d6d6ef3387")
	)
	(junction
		(at 208.28 49.53)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "d4ef6cdc-1b9a-4042-822e-62d389aa0a81")
	)
	(junction
		(at 109.22 111.76)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "dce8f8fb-8cb6-4098-b42a-e95b2b0c5401")
	)
	(junction
		(at 179.07 100.33)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "e1ecea07-8099-46fb-8bf8-b8824874d0e4")
	)
	(junction
		(at 204.47 91.44)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "e5c130f1-87cd-4ef7-8caa-965e37c5d6be")
	)
	(junction
		(at 217.17 91.44)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "eb34a3e8-66cd-470e-acb7-367179aeec58")
	)
	(junction
		(at 71.12 45.72)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "ec368908-a09b-4fce-a92d-5ad8201993ad")
	)
	(junction
		(at 170.18 106.68)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "eeb69b09-3aec-4303-98f2-f19c26ff5237")
	)
	(junction
		(at 43.18 62.23)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "f093aac9-e0e7-4763-84ba-8845b3c2a12f")
	)
	(junction
		(at 204.47 107.95)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "f5259012-1455-49c9-9c2b-734c18c88452")
	)
	(junction
		(at 231.14 107.95)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "f9150fc0-2282-420b-95ad-d285f19a9519")
	)
	(no_connect
		(at 120.65 124.46)
		(uuid "00513b0d-784d-444a-ba1f-218990155952")
	)
	(no_connect
		(at 95.25 149.86)
		(uuid "0b145e5e-bba1-45a4-85b1-f0b46238bede")
	)
	(no_connect
		(at 120.65 127)
		(uuid "0de86f6a-cef1-4cbc-93a8-fb75fde01509")
	)
	(no_connect
		(at 95.25 124.46)
		(uuid "292216ae-e141-4653-a395-5afab81da04b")
	)
	(no_connect
		(at 95.25 134.62)
		(uuid "2d2f94ab-a0fa-4258-9469-681e8255a09a")
	)
	(no_connect
		(at 95.25 127)
		(uuid "3df32a17-8de2-493f-ab6e-7350b5cbd7ab")
	)
	(no_connect
		(at 95.25 139.7)
		(uuid "5182f494-6a82-44b5-b0d3-9c5d2507f151")
	)
	(no_connect
		(at 120.65 152.4)
		(uuid "6084cd45-9731-4f03-8488-fb4eb2b68f90")
	)
	(no_connect
		(at 95.25 137.16)
		(uuid "617a576b-7581-496c-b5ea-50579fe281b6")
	)
	(no_connect
		(at 120.65 139.7)
		(uuid "d2bf2274-5c2f-4ae0-b598-0ef0593f54b4")
	)
	(no_connect
		(at 95.25 142.24)
		(uuid "d742cd77-6a58-40d8-a285-9954d60652fd")
	)
	(no_connect
		(at 95.25 144.78)
		(uuid "dac68ebc-f491-4032-88fd-c7e9e2d993a8")
	)
	(no_connect
		(at 95.25 147.32)
		(uuid "dbed9a4f-0054-431f-a9f6-c36395eacfee")
	)
	(wire
		(pts
			(xy 52.07 53.34) (xy 59.69 53.34)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "0350ad60-d66c-46cc-9acc-dbd92178ad89")
	)
	(wire
		(pts
			(xy 168.91 38.1) (xy 168.91 39.37)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "04badb4e-08a1-446c-a191-14b8acc47042")
	)
	(wire
		(pts
			(xy 273.05 106.68) (xy 278.13 106.68)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "08103bdc-f30c-40c3-8514-cecef0b993b8")
	)
	(wire
		(pts
			(xy 120.65 149.86) (xy 130.81 149.86)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "084a2318-9292-4131-aee7-b76f8b78e490")
	)
	(wire
		(pts
			(xy 43.18 62.23) (xy 44.45 62.23)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "0900838b-1c01-490e-a5d1-6718d6ca44d8")
	)
	(wire
		(pts
			(xy 248.92 114.3) (xy 254 114.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "09b6f3f9-11d0-4bd5-825e-7031812df07f")
	)
	(wire
		(pts
			(xy 170.18 106.68) (xy 171.45 106.68)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "0c9aca5a-eb9a-4bbe-b9e8-cca3da34f18e")
	)
	(wire
		(pts
			(xy 107.95 111.76) (xy 109.22 111.76)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "0d527eac-b998-4642-ab7d-a8bba3eebaa0")
	)
	(wire
		(pts
			(xy 204.47 121.92) (xy 217.17 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "11b804c9-3743-45f9-a2b7-a007df1036c2")
	)
	(wire
		(pts
			(xy 231.14 107.95) (xy 231.14 109.22)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "1268919c-9e84-43ac-912a-47b72755b524")
	)
	(wire
		(pts
			(xy 40.64 129.54) (xy 29.21 129.54)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "1286c177-1f19-4c0f-9222-980ba9707b8f")
	)
	(wire
		(pts
			(xy 184.15 39.37) (xy 186.69 39.37)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "1389fa13-4612-494e-bf0f-efc513f84272")
	)
	(wire
		(pts
			(xy 240.03 121.92) (xy 231.14 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "14e616f3-c01e-4c40-979f-94ce340c9604")
	)
	(wire
		(pts
			(xy 256.54 121.92) (xy 240.03 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "168d528c-9a3f-4129-b619-f9f326b85dbc")
	)
	(wire
		(pts
			(xy 168.91 60.96) (xy 168.91 62.23)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "178989ca-06a9-4c0e-bd34-15d7ded26bf9")
	)
	(wire
		(pts
			(xy 256.54 99.06) (xy 256.54 100.33)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "1b205f56-fc56-490f-a332-4b158c8e23b2")
	)
	(wire
		(pts
			(xy 29.21 129.54) (xy 29.21 132.08)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "22269c93-7812-45fc-b2bf-88e9bc8ac62f")
	)
	(wire
		(pts
			(xy 168.91 39.37) (xy 168.91 40.64)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "24305ceb-b268-40fd-b037-f69f426cba28")
	)
	(wire
		(pts
			(xy 64.77 50.8) (xy 64.77 57.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "25c11466-9d3a-43c4-a957-bf721cce574b")
	)
	(wire
		(pts
			(xy 168.91 50.8) (xy 168.91 60.96)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "27a1c8c3-9593-4084-b134-3f77f126509a")
	)
	(wire
		(pts
			(xy 194.31 100.33) (xy 196.85 100.33)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "2a2fb4ef-cc39-4690-b593-82b88a5477b0")
	)
	(wire
		(pts
			(xy 265.43 121.92) (xy 256.54 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "2c2044c2-fd86-40eb-b29c-77319600b5c4")
	)
	(wire
		(pts
			(xy 180.34 114.3) (xy 186.69 114.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "2f326a71-4495-4cb9-b078-12a37702d439")
	)
	(wire
		(pts
			(xy 194.31 34.29) (xy 194.31 30.48)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "30944a30-9633-4e92-b308-634a52b6659f")
	)
	(wire
		(pts
			(xy 120.65 119.38) (xy 135.89 119.38)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "360e6ba8-e4d1-4133-9b6e-b70b892ec456")
	)
	(wire
		(pts
			(xy 100.33 45.72) (xy 104.14 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "39615cd0-40ef-440e-862b-0759dea565f9")
	)
	(wire
		(pts
			(xy 66.04 45.72) (xy 71.12 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "3a1bf9fb-8a50-41fd-84b7-6a83c61a6607")
	)
	(wire
		(pts
			(xy 160.02 60.96) (xy 160.02 58.42)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "3dab111e-88ce-412d-a0b5-b96295735020")
	)
	(wire
		(pts
			(xy 120.65 142.24) (xy 130.81 142.24)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "3ec834a8-adc5-4db4-8c38-f73c9e48566c")
	)
	(wire
		(pts
			(xy 33.02 134.62) (xy 40.64 134.62)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "434d86b5-5ab6-44ae-ab08-250c8907a876")
	)
	(wire
		(pts
			(xy 33.02 132.08) (xy 40.64 132.08)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "44314319-a85d-485f-a4c6-01f67074fb64")
	)
	(wire
		(pts
			(xy 120.65 144.78) (xy 130.81 144.78)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "47c87b84-5d26-445e-899a-ef1f6dde0181")
	)
	(wire
		(pts
			(xy 109.22 107.95) (xy 109.22 111.76)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "47e29534-0d2b-4f0e-a5c9-8d584caba116")
	)
	(wire
		(pts
			(xy 31.75 127) (xy 40.64 127)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "49d209cb-1158-48a1-ada3-69922de0eee4")
	)
	(wire
		(pts
			(xy 179.07 121.92) (xy 170.18 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "4cb6c262-3aea-4160-8a4f-7e1c3574e625")
	)
	(wire
		(pts
			(xy 104.14 45.72) (xy 116.84 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "4ed11c16-ebdc-4b7d-a620-e05713ff718f")
	)
	(wire
		(pts
			(xy 52.07 50.8) (xy 64.77 50.8)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "4f5e5c56-1937-4007-857b-b40f3fafa18d")
	)
	(wire
		(pts
			(xy 194.31 44.45) (xy 194.31 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "51434d46-f6d4-4cbc-8370-bf901ca3113e")
	)
	(wire
		(pts
			(xy 217.17 121.92) (xy 217.17 123.19)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "53c27d57-25b1-4905-852d-e0f52326e112")
	)
	(wire
		(pts
			(xy 179.07 99.06) (xy 179.07 100.33)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "56348d4b-15d4-4998-8dfe-8b71ccaf6e32")
	)
	(wire
		(pts
			(xy 71.12 53.34) (xy 71.12 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "567c2f67-990f-41a6-81e2-7db6d8644d8c")
	)
	(wire
		(pts
			(xy 194.31 114.3) (xy 195.58 114.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "58404f54-c9fa-4991-9a27-4f6bf797ceea")
	)
	(wire
		(pts
			(xy 104.14 53.34) (xy 104.14 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "5a0c9c92-dcae-4cbb-9c1c-8a2633cb0a66")
	)
	(wire
		(pts
			(xy 76.2 119.38) (xy 95.25 119.38)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "5a30219e-90ad-4927-99bc-f23c97ee065b")
	)
	(wire
		(pts
			(xy 240.03 49.53) (xy 254 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "5fa5d86c-97b5-441d-a153-8c2c3f3dd05b")
	)
	(wire
		(pts
			(xy 170.18 121.92) (xy 170.18 119.38)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "64c88334-c96c-4d41-bd62-2b7d1dc627bf")
	)
	(wire
		(pts
			(xy 204.47 119.38) (xy 204.47 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "6a2416ab-21ef-464a-a2c8-89843a069bd7")
	)
	(wire
		(pts
			(xy 256.54 91.44) (xy 231.14 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "6cd9f876-454b-44e5-9eaa-8b3492c10904")
	)
	(wire
		(pts
			(xy 176.53 39.37) (xy 168.91 39.37)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "71f1ba25-134a-4240-ad2a-9341b10b731e")
	)
	(wire
		(pts
			(xy 41.91 60.96) (xy 41.91 62.23)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "744c5fe5-532f-466e-9d0d-08276a0c9c1d")
	)
	(wire
		(pts
			(xy 204.47 91.44) (xy 217.17 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "757f7e50-a3d4-438c-9b1c-6834492555b3")
	)
	(wire
		(pts
			(xy 44.45 62.23) (xy 44.45 60.96)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "76f6f182-c90d-4a5f-b013-2fb1859f2b4a")
	)
	(wire
		(pts
			(xy 231.14 121.92) (xy 231.14 119.38)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "77ac6aec-1983-4b0d-961b-62e38cb654c5")
	)
	(wire
		(pts
			(xy 81.28 50.8) (xy 81.28 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "7bf4f5ea-3b0f-4cc6-93e6-73c6868037c2")
	)
	(wire
		(pts
			(xy 132.08 129.54) (xy 120.65 129.54)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "7c032acc-3880-489c-8da0-727d0e4079b5")
	)
	(wire
		(pts
			(xy 204.47 105.41) (xy 204.47 107.95)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "7d18adc2-7d41-4fa3-b986-cdb725229460")
	)
	(wire
		(pts
			(xy 120.65 121.92) (xy 135.89 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "7d3c7913-644b-4ec7-a4ca-5fc8bc3d2c33")
	)
	(wire
		(pts
			(xy 76.2 119.38) (xy 76.2 120.65)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "8470cd66-b418-4883-928b-8aa7b57225d1")
	)
	(wire
		(pts
			(xy 179.07 100.33) (xy 179.07 101.6)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "852e5ac0-d70b-430b-b4c9-477b3c7d699b")
	)
	(wire
		(pts
			(xy 195.58 114.3) (xy 196.85 114.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "858647b8-5820-4dbf-8eb9-08cd5e5635da")
	)
	(wire
		(pts
			(xy 208.28 58.42) (xy 208.28 59.69)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "89237f20-9cff-48c0-9927-ed236ce57e3b")
	)
	(wire
		(pts
			(xy 71.12 45.72) (xy 81.28 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "8ad18b0d-0496-4d11-954e-e65bfa591a5b")
	)
	(wire
		(pts
			(xy 218.44 58.42) (xy 233.68 58.42)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "8c96d12c-866c-4aa9-8ae7-0f0499627226")
	)
	(wire
		(pts
			(xy 179.07 121.92) (xy 195.58 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "8ce8d0f5-e604-4797-99b5-89663cb6853a")
	)
	(wire
		(pts
			(xy 204.47 95.25) (xy 204.47 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "8cfa7f42-ffd0-4f59-9f23-ad142f713587")
	)
	(wire
		(pts
			(xy 160.02 45.72) (xy 161.29 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "8e141955-c619-4b36-8e0d-aa14c9b744a8")
	)
	(wire
		(pts
			(xy 179.07 111.76) (xy 179.07 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "93ef7968-8769-4d25-98a6-35f929c15d90")
	)
	(wire
		(pts
			(xy 132.08 132.08) (xy 120.65 132.08)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "99594ad1-d8ca-42da-a860-892824421db0")
	)
	(wire
		(pts
			(xy 231.14 91.44) (xy 231.14 95.25)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "9cac23b0-e07f-46e5-9df8-a68a8e084434")
	)
	(wire
		(pts
			(xy 265.43 106.68) (xy 265.43 111.76)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "9dad04e9-f12f-49f7-bab5-8dfa85813ba1")
	)
	(wire
		(pts
			(xy 238.76 100.33) (xy 241.3 100.33)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a010a389-eb1f-4f57-a156-7b39262edeed")
	)
	(wire
		(pts
			(xy 217.17 87.63) (xy 217.17 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a0251513-12f8-4581-8821-e32d9f8616bc")
	)
	(wire
		(pts
			(xy 157.48 106.68) (xy 162.56 106.68)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a1ae756a-5146-409a-8a92-776d1fc019f9")
	)
	(wire
		(pts
			(xy 204.47 107.95) (xy 204.47 109.22)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a51e66e9-3ca5-4053-947b-611d8043917b")
	)
	(wire
		(pts
			(xy 231.14 105.41) (xy 231.14 107.95)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a6ac2a2c-4656-42f5-9f93-79805833565f")
	)
	(wire
		(pts
			(xy 109.22 111.76) (xy 110.49 111.76)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a76b9350-409b-4f08-9af9-6c3ad49117e1")
	)
	(wire
		(pts
			(xy 168.91 30.48) (xy 194.31 30.48)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a7d5696d-0167-48a4-9278-08da70937040")
	)
	(wire
		(pts
			(xy 261.62 49.53) (xy 270.51 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "a9d4ac0d-4174-45bb-8f72-d3761cb4fc02")
	)
	(wire
		(pts
			(xy 59.69 53.34) (xy 59.69 57.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "aaa28676-6eab-4e23-9936-4142cca98e89")
	)
	(wire
		(pts
			(xy 194.31 49.53) (xy 208.28 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "abed7dd2-9477-4b10-a00b-69696a172c50")
	)
	(wire
		(pts
			(xy 248.92 100.33) (xy 256.54 100.33)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ac1ff02e-c9d1-4723-a638-9165f3a5eea7")
	)
	(wire
		(pts
			(xy 218.44 107.95) (xy 231.14 107.95)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ad6e7417-2e9e-437b-8c74-67b54736caa4")
	)
	(wire
		(pts
			(xy 81.28 45.72) (xy 82.55 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "aea9096b-171b-4fb6-8a7d-e64ff9e271c7")
	)
	(wire
		(pts
			(xy 256.54 100.33) (xy 256.54 101.6)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "b515ef61-18de-4cf6-ac04-fde02bec98ad")
	)
	(wire
		(pts
			(xy 132.08 137.16) (xy 120.65 137.16)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "b942eaee-d55b-409e-98f7-dc6133f0dcd0")
	)
	(wire
		(pts
			(xy 208.28 49.53) (xy 209.55 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "bbcb98fa-bc0b-4525-912f-f75eb5629490")
	)
	(wire
		(pts
			(xy 265.43 106.68) (xy 264.16 106.68)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "bbedf88c-8c00-462e-9601-e5a8f0f75ee0")
	)
	(wire
		(pts
			(xy 218.44 57.15) (xy 218.44 58.42)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "bd9df308-cd86-452e-a99d-4f19cb215766")
	)
	(wire
		(pts
			(xy 132.08 134.62) (xy 120.65 134.62)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "bf9ecdea-9395-4b0d-9573-4e9e06c1fc1c")
	)
	(wire
		(pts
			(xy 33.02 137.16) (xy 40.64 137.16)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c0d33045-a454-4bd4-8aa7-74a58c4b7cdd")
	)
	(wire
		(pts
			(xy 265.43 119.38) (xy 265.43 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c5acffc1-2e2b-4a84-a161-afe8830ac647")
	)
	(wire
		(pts
			(xy 52.07 45.72) (xy 58.42 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c5e1d78d-cd51-420b-8589-e22729c3731c")
	)
	(wire
		(pts
			(xy 179.07 91.44) (xy 204.47 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "c9a7f66e-bc0b-4ea2-ac73-2bde9ce461a8")
	)
	(wire
		(pts
			(xy 218.44 58.42) (xy 218.44 59.69)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "cb0072c1-cba6-4e52-8de0-87baaddaa059")
	)
	(wire
		(pts
			(xy 193.04 58.42) (xy 208.28 58.42)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ccaedab7-8309-45be-9199-92acdd19ce3c")
	)
	(wire
		(pts
			(xy 218.44 49.53) (xy 240.03 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ce837993-0b2c-4034-8274-a409f929d9b4")
	)
	(wire
		(pts
			(xy 240.03 49.53) (xy 240.03 53.34)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "cfd0c468-3804-48e9-adbd-904ee4cdc385")
	)
	(wire
		(pts
			(xy 170.18 106.68) (xy 170.18 111.76)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d2a2ce0a-5a1d-4292-97fe-9e13480418b9")
	)
	(wire
		(pts
			(xy 217.17 121.92) (xy 231.14 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d47ad5a6-d077-4318-91ae-f1cb3e64f050")
	)
	(wire
		(pts
			(xy 256.54 111.76) (xy 256.54 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d4b95f3f-2ff5-453d-ae22-fa23a0dc2b6e")
	)
	(wire
		(pts
			(xy 204.47 107.95) (xy 215.9 107.95)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d5843128-02d1-4acd-9d41-b7615e03993a")
	)
	(wire
		(pts
			(xy 116.84 53.34) (xy 116.84 54.61)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d6127d72-4dd6-424c-bfbb-5be47ac1d01b")
	)
	(wire
		(pts
			(xy 208.28 57.15) (xy 208.28 58.42)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d61ee1b7-61e6-49dc-91d4-33ceb273c70e")
	)
	(wire
		(pts
			(xy 139.7 45.72) (xy 152.4 45.72)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d719eadc-260b-441f-978e-531b7d26bb60")
	)
	(wire
		(pts
			(xy 160.02 45.72) (xy 160.02 50.8)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "d896983c-6d7c-44b5-b8d1-88f45da92820")
	)
	(wire
		(pts
			(xy 82.55 132.08) (xy 95.25 132.08)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "daa8337d-09bb-4d40-8a82-92c3b011dc83")
	)
	(wire
		(pts
			(xy 195.58 121.92) (xy 204.47 121.92)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "db16d58d-53a7-4f14-a5b2-5a5c06b61edf")
	)
	(wire
		(pts
			(xy 82.55 50.8) (xy 81.28 50.8)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "dd17caf1-2df6-4de8-b7aa-7406379b7753")
	)
	(wire
		(pts
			(xy 168.91 60.96) (xy 160.02 60.96)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "deb755c4-9541-45ab-970c-a43581759941")
	)
	(wire
		(pts
			(xy 238.76 114.3) (xy 240.03 114.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "e511b553-7c95-4790-86fb-5855196c1a8c")
	)
	(wire
		(pts
			(xy 217.17 49.53) (xy 218.44 49.53)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "e65a1e34-0eda-4a8d-82b4-9ff06ae010fe")
	)
	(wire
		(pts
			(xy 186.69 100.33) (xy 179.07 100.33)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "eaa2700f-d3e7-4b10-bec7-fece10170c76")
	)
	(wire
		(pts
			(xy 41.91 62.23) (xy 43.18 62.23)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "ef1de671-e9b4-4d67-8df0-bed9ac839dce")
	)
	(wire
		(pts
			(xy 240.03 114.3) (xy 241.3 114.3)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "f4cc0043-e1a8-4b6a-9c40-c0d6a6450e84")
	)
	(wire
		(pts
			(xy 120.65 147.32) (xy 130.81 147.32)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "faaafd50-c1d8-4863-b8af-103f75e77a34")
	)
	(wire
		(pts
			(xy 240.03 60.96) (xy 240.03 63.5)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "fc7f3baa-68ee-4c82-a5aa-095a0b67765a")
	)
	(wire
		(pts
			(xy 217.17 91.44) (xy 231.14 91.44)
		)
		(stroke
			(width 0)
			(type default)
		)
		(uuid "fe95c803-16b5-494e-9d2b-5cd981a0d32c")
	)
	(label "VDD_LED_EN"
		(at 82.55 132.08 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "00279635-4d5a-4f61-8800-97c69201878b")
	)
	(label "VDD_LED_EN"
		(at 139.7 45.72 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "105a2c70-1933-4083-bff6-b606403a4f61")
	)
	(label "LS_B"
		(at 132.08 132.08 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "16146db6-4974-4c22-bc97-45600d99f5ae")
	)
	(label "VDD_MCU"
		(at 115.57 45.72 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "18ef0a1a-e382-4276-9841-f87c04de7fb5")
	)
	(label "SWCLK"
		(at 130.81 149.86 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "18fc67fe-12bc-46d8-a074-1139d4b3f70e")
	)
	(label "CURR_SENSE_1"
		(at 135.89 119.38 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "24d4e0b7-a1ab-450f-930c-f5a1bb3828f6")
	)
	(label "HS_A"
		(at 157.48 106.68 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "2daa8da1-5c3a-4018-910c-fcd1ea1727b1")
	)
	(label "CURR_SENSE_2"
		(at 233.68 58.42 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "37cce2fc-a94f-4d98-ae61-e075ab26f765")
	)
	(label "HS_B"
		(at 132.08 129.54 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "4db21cd1-90e8-44db-a903-613100970ff4")
	)
	(label "HS_B"
		(at 278.13 106.68 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "5c4728e3-3c13-41ac-b2f2-ac577a0a987f")
	)
	(label "USB_D+"
		(at 130.81 144.78 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "5cc302fd-80da-4bcb-ac8b-ed2dc696ebb1")
	)
	(label "USB_D+"
		(at 53.34 50.8 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "6354dd90-af2b-4449-856a-2ccbbf3c92db")
	)
	(label "SWCLK"
		(at 33.02 134.62 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "76f2e54d-4b5d-4d48-9838-f2a2bcdeab67")
	)
	(label "SWDIO"
		(at 33.02 132.08 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "7a1384f8-ae11-4368-b135-50c99918b38e")
	)
	(label "HS_A"
		(at 132.08 137.16 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "7b43c180-0316-4e85-9ff1-6cab7215fab9")
	)
	(label "VDD_MCU"
		(at 31.75 127 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "7d54ce4b-5e09-4ec2-9337-0bdb50467e17")
	)
	(label "USB_D-"
		(at 130.81 142.24 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "7f1b0a59-e390-46eb-aed8-e8bdc4d9901f")
	)
	(label "VDD_LED"
		(at 270.51 49.53 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "8474965f-17f0-4c2f-8b56-90d163d4350c")
	)
	(label "USB_D-"
		(at 53.34 53.34 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "8831ba43-a618-47cb-a15a-c5eb8fb157a9")
	)
	(label "SWDIO"
		(at 130.81 147.32 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "92906f31-2e07-40d2-bd16-00514c5969a1")
	)
	(label "CURR_SENSE_1"
		(at 193.04 58.42 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "9b2ab672-a0b8-4c3f-b189-b1289e0e5116")
	)
	(label "VDD_LED"
		(at 217.17 87.63 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "ac8ccd4a-123b-436b-8f7e-d464288d5b64")
	)
	(label "CURR_SENSE_2"
		(at 135.89 121.92 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "b3967272-478b-4dc0-a806-eb48eeb1b9a1")
	)
	(label "NRST"
		(at 87.63 119.38 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "b8bad739-af1b-4111-ac37-733735ae6f45")
	)
	(label "VDD_MCU"
		(at 109.22 107.95 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "bf6c22b0-bf22-409c-8290-cd09f17271b4")
	)
	(label "NRST"
		(at 33.02 137.16 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "c167929a-ba91-4db0-8a60-ace98090c46c")
	)
	(label "LS_A"
		(at 132.08 134.62 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "c69d064f-6ac5-41f6-9cab-3b59545b4bf3")
	)
	(label "VBUS"
		(at 179.07 30.48 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "c9ae7903-3c18-4b6b-a16b-89c4ba3e4cf1")
	)
	(label "LS_A"
		(at 180.34 114.3 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "ca9329da-ae43-464d-ac8b-301bff5c5716")
	)
	(label "VBUS"
		(at 71.12 45.72 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left bottom)
		)
		(uuid "f6b5576e-9ef3-437b-9f9a-f85d99e49bed")
	)
	(label "LS_B"
		(at 254 114.3 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right bottom)
		)
		(uuid "fa05f2ad-a3ea-418b-9e54-2536ef27f6d9")
	)
	(symbol
		(lib_id "VL_PMICs:MIC5504-3.3YM5-TR")
		(at 91.44 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "08884ee4-b2a7-413b-98e7-824e37ffdfc1")
		(property "Reference" "U2"
			(at 91.44 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MIC5504-3.3YM5-TR"
			(at 91.44 41.91 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "VL_SOT:SOT-23-5"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MIC5501-02-03-04-300mA-Single-Output-LDO-in-Small-Packages-DS20006006B.pdf"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Linear Voltage Regulator IC Positive Fixed 3.3V Output 300mA SOT-23-5"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Microchip Technology"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "MIC5504-3.3YM5-TR"
			(at 92.71 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" ""
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" ""
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "576-4764-1-ND"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "998-MIC5504-3.3YM5TR"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "2510377"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "MIC5504-3.3YM5-TR"
			(at 91.44 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "3"
			(uuid "556d43a4-9c04-4d1c-aa2f-a9aeb1f89478")
		)
		(pin "1"
			(uuid "4d0b7d4e-8a3b-4b85-b64f-27308e5d82bb")
		)
		(pin "2"
			(uuid "7b07b2fa-34c2-47f8-8289-e9bc1630ad5f")
		)
		(pin "5"
			(uuid "3d4f9f8e-6285-49ae-90ff-d7e085b2804d")
		)
		(pin "4"
			(uuid "a8c06dee-b6ce-4fe8-abc7-874d0461abf5")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 160.02 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "0d6ec750-5f73-458c-8a69-87e5591d55fa")
		(property "Reference" "R19"
			(at 162.56 53.3399 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 160.02 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 160.02 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 160.02 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 160.02 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 162.56 55.8799 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 167.64 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 167.64 55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 160.02 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 160.02 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 180.34 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 180.34 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 160.02 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 160.02 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 160.02 74.93 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 160.02 77.47 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "c2bc5e5e-a519-428f-bf68-4f6622366805")
		)
		(pin "1"
			(uuid "34db343c-5090-4847-89ad-bf6746fe2559")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R19")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 213.36 49.53 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "11f8e0cb-cb35-4dcd-bb90-5333df573e35")
		(property "Reference" "R22"
			(at 213.36 43.18 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "10R"
			(at 213.36 45.72 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1225_3264Metric_Pad1.47x6.45mm_HandSolder"
			(at 213.36 47.752 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "~"
			(at 213.36 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor"
			(at 213.36 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "71-RCL122510R0FKEG "
			(at 213.36 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "40f6a144-74a3-4086-86bb-26eba48bb301")
		)
		(pin "1"
			(uuid "5f3a5ad7-f3ef-442d-9df5-7618fb7ef2cc")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R22")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 190.5 114.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "1722b27d-eba6-48d8-90fe-c85968d03053")
		(property "Reference" "R3"
			(at 190.754 116.586 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 195.58 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 198.12 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 190.5 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 190.5 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 190.754 118.364 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 189.23 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 191.77 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 200.66 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 203.2 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 200.66 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 203.2 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 205.74 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 208.28 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 210.82 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 213.36 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "22d9b5b6-68fa-4de2-9977-d01506a4c978")
		)
		(pin "1"
			(uuid "a51f8b43-d223-4cfe-9a76-5ae341b1bef4")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Capacitors:C0603_10uF_16V_X5R")
		(at 104.14 49.53 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "19a4edba-5b75-4b58-9375-c4b2b7f0cc77")
		(property "Reference" "C3"
			(at 109.728 46.99 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "C0603_10uF_16V_X5R"
			(at 104.14 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Capacitors:C0603"
			(at 104.14 41.91 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "*"
			(at 104.14 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Capacitor; Footprint 0603; 10uF/16V; X5R"
			(at 104.14 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Capacitance" "10uF"
			(at 109.728 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Voltage" "16V"
			(at 109.728 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Dielectric" "X5R"
			(at 104.14 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Taiyo Yuden"
			(at 104.14 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "EMK107BBJ106MA-T"
			(at 104.14 36.83 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "587-3238-1-ND"
			(at 104.14 34.29 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "963-EMK107BBJ106MA-T"
			(at 104.14 31.75 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "2779064"
			(at 104.14 29.21 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "CL10A106MO8NQNC"
			(at 104.14 26.67 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Murata Electronics"
			(at 80.01 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "GRM188R61C106MA73D"
			(at 80.01 36.83 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "ec1a973d-bc2e-40f2-8878-fbcca1a24538")
		)
		(pin "1"
			(uuid "97ecbcc3-5c4e-4ecf-9951-5371969215a8")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_ST_STM32C0:STM32C071GBUxN")
		(at 107.95 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "1c2e1b99-7849-44c9-9349-9cc6273abaf8")
		(property "Reference" "U1"
			(at 110.0933 160.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "STM32C071GBUxN"
			(at 110.0933 162.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28_4x4mm_P0.5mm"
			(at 97.79 157.48 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32c071gb.pdf"
			(at 107.95 137.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 128KB flash, 24KB RAM, 25 GPIO, UFQFPN28_N"
			(at 107.95 137.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "511-STM32C071GBU6N"
			(at 107.95 137.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "4"
			(uuid "18eb1773-8a38-4de8-81ed-694e57cf64f1")
		)
		(pin "7"
			(uuid "89e72f81-e477-4d8a-a313-e2373cfd9035")
		)
		(pin "6"
			(uuid "202c4e79-9393-4b4a-91da-8809792fb83b")
		)
		(pin "3"
			(uuid "d3d0f5f2-dff1-4750-85c5-2c34ac6cb164")
		)
		(pin "25"
			(uuid "33ea5805-4f6f-49f0-ae39-694a860c4c3f")
		)
		(pin "16"
			(uuid "5f7d61cc-9351-49f0-9474-793a36cd73fd")
		)
		(pin "28"
			(uuid "74698606-38b0-498b-b143-3e976dcb455b")
		)
		(pin "18"
			(uuid "13b50279-fbaf-4cf8-aafc-b24d686afa1d")
		)
		(pin "10"
			(uuid "f7b1fc16-8b5a-47a6-bae4-910139650c13")
		)
		(pin "17"
			(uuid "2a176666-1919-44d0-b3c7-bbf3c83fde71")
		)
		(pin "20"
			(uuid "6fa38a5d-8586-4e19-a6ff-9f864211fdd6")
		)
		(pin "9"
			(uuid "1ac0d440-dd42-4261-a46a-d04bdea4064d")
		)
		(pin "23"
			(uuid "22cbab9a-979c-40f8-8483-22a66a20c5cb")
		)
		(pin "8"
			(uuid "124fbaa9-1ed6-4dcc-9ef7-e4fbac25e43f")
		)
		(pin "21"
			(uuid "67579691-60d1-4c26-9bdb-74da3229366c")
		)
		(pin "22"
			(uuid "7437f587-6faa-4c5f-948e-5944f66d19f9")
		)
		(pin "19"
			(uuid "130017a9-8467-473b-b472-c23ee5412b1c")
		)
		(pin "26"
			(uuid "996ffea4-f4e5-4505-85dd-ca7a03fbed9e")
		)
		(pin "27"
			(uuid "9e801605-35dd-4990-b77c-619cccd43d7d")
		)
		(pin "12"
			(uuid "40480377-4ee4-413b-811a-893618d8cf60")
		)
		(pin "13"
			(uuid "f5217804-86c0-4d1f-b2f1-870b0623565c")
		)
		(pin "11"
			(uuid "6939187f-77a7-43fb-ba0f-f906d2a962d1")
		)
		(pin "2"
			(uuid "2b02480b-4510-4ca4-8e0f-9c9f2e3d47fe")
		)
		(pin "14"
			(uuid "3ba97b27-2d5a-4c71-9ad2-172fa11c56b2")
		)
		(pin "1"
			(uuid "63cdeff4-9d2c-49a3-b81d-76034e2f1a1b")
		)
		(pin "5"
			(uuid "cfd3f2fb-708b-4b3c-9520-92cc844cc242")
		)
		(pin "15"
			(uuid "022468b0-67f8-4a3f-bc17-ac85d4a8bb6b")
		)
		(pin "24"
			(uuid "238ad2dc-1803-451e-94c1-ef4a0a3a6b91")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 240.03 63.5 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "1edabd8f-f098-4cba-8bc0-660532c903ec")
		(property "Reference" "#PWR011"
			(at 240.03 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 240.03 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "c87bdf47-e6ab-45e8-b020-e78106150eff")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Transistors:2N7002NXAKR")
		(at 166.37 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "220e397b-41e6-475a-ad69-c6e3ef160cb2")
		(property "Reference" "Q7"
			(at 171.45 45.212 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "2N7002NXAKR"
			(at 171.45 47.244 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "VL_SOT:SOT-23"
			(at 160.02 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/2N7002NXAK.pdf"
			(at 146.05 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 166.37 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Nexperia USA Inc."
			(at 166.37 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "2N7002NXAKR"
			(at 166.37 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "1727-8643-1-ND"
			(at 166.37 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "771-2N7002NXAKR"
			(at 166.37 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3226400"
			(at 166.37 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "2N7002NXAKR"
			(at 166.37 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "e2f99fb9-fe8c-4202-8b9a-18db5b861b4b")
		)
		(pin "2"
			(uuid "27f7ee01-41f7-46c0-800b-706a1697d78c")
		)
		(pin "3"
			(uuid "3e578ae6-7429-48f3-8dbc-5a3a8760c90d")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 29.21 132.08 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "24b7e048-4652-4186-8bd3-130069f9ede5")
		(property "Reference" "#PWR012"
			(at 29.21 138.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 29.21 137.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 29.21 132.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 29.21 132.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 29.21 132.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "685748a7-2139-4cf1-8f64-47fe1054d4ac")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 245.11 114.3 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "2563c419-1f9c-4652-903e-6a744dfce738")
		(property "Reference" "R6"
			(at 245.11 116.586 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 250.19 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 252.73 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 245.11 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 245.11 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 245.11 118.618 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 243.84 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 246.38 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 255.27 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 257.81 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 255.27 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 257.81 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 260.35 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 262.89 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 265.43 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 267.97 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "defe991c-e9e7-405d-8f6e-c4720bf97fe2")
		)
		(pin "1"
			(uuid "d2074487-50eb-4fb6-a04b-69d5ccd6702c")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 179.07 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "2f6590ec-fbe1-47d8-b517-ee783ae27f47")
		(property "Reference" "R2"
			(at 181.61 93.9799 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 179.07 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 179.07 102.87 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 179.07 95.25 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 179.07 95.25 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 181.61 96.5199 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 186.69 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 186.69 96.52 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 179.07 105.41 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 179.07 107.95 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 199.39 105.41 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 199.39 107.95 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 179.07 110.49 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 179.07 113.03 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 179.07 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 179.07 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "415db5f7-b18c-4858-a002-569b374eb938")
		)
		(pin "1"
			(uuid "304eb70f-7a2c-4680-94ff-d13fb84431c7")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 218.44 67.31 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "32b49a59-814d-46ff-9dba-54fb779d85d6")
		(property "Reference" "#PWR09"
			(at 218.44 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 218.44 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 218.44 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 218.44 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 218.44 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "51584474-6cd9-452d-9d16-fcc628852616")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 116.84 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "389b5bda-9b95-422b-a74b-f6c08f9f05a0")
		(property "Reference" "#PWR07"
			(at 116.84 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 116.84 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 116.84 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 116.84 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 116.84 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "862adfcf-cee7-47f0-877f-dae89851d8e7")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 91.44 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "3b22f261-4a09-4c84-9453-35ecdad5a718")
		(property "Reference" "#PWR03"
			(at 91.44 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 91.44 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 91.44 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 91.44 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 91.44 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "68fadaa0-e223-46b2-a3f4-c47743a7ac39")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 76.2 128.27 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "3ccd80a1-05f5-43f9-83e9-e2c10ed0bf13")
		(property "Reference" "#PWR013"
			(at 76.2 134.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 76.2 133.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 76.2 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 76.2 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 76.2 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "5c3f832c-341d-4f34-a37e-27ae80049079")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Capacitors:CP2917_330uF_6.3V_Polymer")
		(at 240.03 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "3f4d195e-2e93-4123-8804-6ddda9cb564a")
		(property "Reference" "C4"
			(at 243.84 53.7209 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "CP2917_330uF_6.3V_Polymer"
			(at 240.03 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Capacitors:CP_EIA-7343-15_Kemet-W"
			(at 240.9952 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/ABE0000/ABE0000C106.pdf"
			(at 236.22 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "330 µF 6.3 V Aluminum - Polymer Capacitors 2917 (7343 Metric) 9mOhm 2000 Hrs @ 85°C"
			(at 240.03 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Capacitance" "330uF"
			(at 243.84 56.2609 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Voltage" "6.3V"
			(at 243.84 58.8009 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 238.76 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "ECG-SY0J331R"
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Panasonic Electronic Components"
			(at 238.76 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "ECG-CY0J331R"
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "P122483CT-ND"
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "667-ECG-SY0J331R"
			(at 240.03 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "2831753"
			(at 240.03 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "X"
			(at 240.03 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "8514b791-b0af-4932-afd0-01cc7bc3459e")
		)
		(pin "1"
			(uuid "2be54dbc-4c0e-4295-b9cd-e3d209b58fdd")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 156.21 45.72 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "4133f3ac-e087-49ac-95c0-c2c1ed2a9328")
		(property "Reference" "R18"
			(at 156.21 39.37 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 161.29 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 163.83 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 156.21 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 156.21 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 156.21 41.91 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 154.94 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 157.48 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 166.37 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 168.91 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 166.37 25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 168.91 25.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 171.45 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 173.99 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 176.53 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 179.07 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "b6131d60-ad5b-4929-8d45-6ef70f26f78f")
		)
		(pin "1"
			(uuid "a75db630-4010-476c-b66f-1fcb28caf056")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Transistors:2N7002NXAKR")
		(at 176.53 106.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "4d53b8cd-c044-4005-85e8-e626da1180ae")
		(property "Reference" "Q5"
			(at 181.61 106.172 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "2N7002NXAKR"
			(at 181.61 108.204 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "VL_SOT:SOT-23"
			(at 170.18 120.65 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/2N7002NXAK.pdf"
			(at 156.21 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 176.53 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Nexperia USA Inc."
			(at 176.53 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "2N7002NXAKR"
			(at 176.53 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "1727-8643-1-ND"
			(at 176.53 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "771-2N7002NXAKR"
			(at 176.53 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3226400"
			(at 176.53 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "2N7002NXAKR"
			(at 176.53 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "d028613c-651e-4d50-a6c6-fc469f361759")
		)
		(pin "2"
			(uuid "9f212248-f8ff-4f1c-a67a-de8969385d5f")
		)
		(pin "3"
			(uuid "2be3f491-852a-4a4e-93d8-ffd9dbbd3090")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 245.11 100.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "53082ae1-a5c5-4244-818b-3a44b57382c8")
		(property "Reference" "R5"
			(at 245.11 93.98 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 250.19 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 252.73 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 245.11 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 245.11 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 245.11 96.52 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 243.84 92.71 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 246.38 92.71 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 255.27 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 257.81 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 255.27 80.01 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 257.81 80.01 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 260.35 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 262.89 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 265.43 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 267.97 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "ac5ba818-2fef-488b-8754-66f540ee8a22")
		)
		(pin "1"
			(uuid "92fd2825-4f17-4638-8b64-b120c778e621")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Connectors:UE27AC54100")
		(at 44.45 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "53a9a0fe-d5f7-4235-8513-889ef7298328")
		(property "Reference" "J2"
			(at 44.45 38.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "48037-2200"
			(at 44.45 40.64 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "Connector_USB:USB_A_Molex_48037-2200_Horizontal"
			(at 48.26 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail-pdf/480372200?display=pdf"
			(at 48.26 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "USB Type A plug"
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Molex"
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "48037-2200"
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" ""
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" " 538-48037-2200"
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" ""
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" ""
			(at 44.45 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "341e1983-05a5-43b7-b05a-339023e76880")
		)
		(pin "5"
			(uuid "8a768f36-1cb0-4c58-bb23-a6849172ff9a")
		)
		(pin "4"
			(uuid "e83f3162-8706-40a9-8e20-88b9b295ba20")
		)
		(pin "3"
			(uuid "e5cef38a-a87c-443b-b1a4-36b6b53c3ba7")
		)
		(pin "1"
			(uuid "ee5b9866-73c9-4589-830d-d85833daa765")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Other:MF-PSML300/6-2")
		(at 62.23 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "54c37792-ae2f-4036-99dd-adbc618784c3")
		(property "Reference" "F2"
			(at 62.23 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "MF-PSML300/6-2"
			(at 62.23 41.91 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "VL_Other:F0805"
			(at 62.23 50.8 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.bourns.com/docs/product-datasheets/mf-nsml-x.pdf"
			(at 62.23 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Polymeric PTC Resettable Fuse 6V 3 A Ih Surface Mount 0805 (2012 Metric), Concave"
			(at 62.23 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Bourns Inc."
			(at 62.23 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "MF-PSML300/6-2"
			(at 62.23 55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Littelfuse Inc."
			(at 88.9 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "0805L300SLWR"
			(at 90.17 55.88 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "118-MF-PSML300/6-2CT-ND"
			(at 62.23 58.42 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "652-MF-PSML300/6-2"
			(at 62.23 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3131611"
			(at 62.23 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "X"
			(at 62.23 66.04 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "81f6e811-c311-4d4a-91f0-7ee5541d6125")
		)
		(pin "1"
			(uuid "51175a3b-1f4b-4039-8800-124287eb236b")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "F2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Diodes:PESD1CAN")
		(at 62.23 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "552b78bb-092b-4f3e-9e86-5066e0a2185f")
		(property "Reference" "D1"
			(at 68.58 61.5949 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "PESD1CAN"
			(at 68.58 64.1349 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "VL_SOT:SOT-23"
			(at 62.23 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://4donline.ihs.com/images/VipMasterIC/IC/NEXP/NEXP-S-A0005722386/NEXP-S-A0005722386-1.pdf?hkey=6D3A4C79FDBF58556ACFDE234799DDF0"
			(at 60.96 48.26 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "TVS DIODE 24VWM 70VC SOT-23-3"
			(at 62.23 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Nexperia USA Inc."
			(at 62.23 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "PESD1CAN,215 "
			(at 62.23 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "EVVO"
			(at 87.63 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "PESD1CAN"
			(at 86.36 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "5272-PESD1CANCT-ND"
			(at 62.23 78.74 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "771-PESD1CAN-T/R"
			(at 62.23 81.28 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "1510703"
			(at 62.23 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "PESD1CAN,215 "
			(at 62.23 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "3be9efce-d2d7-40f4-9ece-28357a0720e4")
		)
		(pin "3"
			(uuid "d661c34b-4054-4c13-a40a-299c8a298c20")
		)
		(pin "2"
			(uuid "5f94a9fe-d657-419a-bf8f-3c5cb7561049")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 62.23 68.58 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "58457afa-11e8-4586-81f2-c196569f146c")
		(property "Reference" "#PWR05"
			(at 62.23 74.93 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 62.23 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 62.23 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 62.23 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 62.23 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "6b22613d-d757-4f6f-8537-086e15b08e17")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:AO3401A")
		(at 191.77 39.37 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "63a985f1-eb58-48a2-a786-4c418b75b277")
		(property "Reference" "Q8"
			(at 197.104 38.608 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "AO3401A"
			(at 197.104 40.386 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 196.85 37.465 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 196.85 35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 191.77 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "621-DMP3130L-7"
			(at 191.77 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "d00ed6c6-395e-44a7-8b2f-309e648bce1e")
		)
		(pin "2"
			(uuid "3b9503b5-e548-427c-b85a-334f7db1230f")
		)
		(pin "3"
			(uuid "e274aa65-084e-479d-9b21-89de74070915")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 195.58 118.11 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "64638008-74da-4fd3-b487-cac7401bcdd8")
		(property "Reference" "R9"
			(at 198.12 116.8399 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 195.58 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 195.58 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 195.58 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 195.58 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 198.12 119.3799 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 203.2 116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 203.2 119.38 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 195.58 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 195.58 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 215.9 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 215.9 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 195.58 133.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 195.58 135.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 195.58 138.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 195.58 140.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "1cec8b89-04ab-45c7-81a4-086097923869")
		)
		(pin "1"
			(uuid "94cf5638-cb48-4205-845b-b71404316b18")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Capacitors:C0603_100nF_50V_X7R")
		(at 76.2 124.46 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "6662078a-a9fc-40ed-bd15-89c156ec952f")
		(property "Reference" "C6"
			(at 80.01 121.9199 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "C0603_100nF_50V_X7R"
			(at 76.2 129.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Capacitors:C0603"
			(at 76.2 132.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.samsungsem.com/kr/support/product-search/mlcc/CL10B104KB8NNNC.jsp"
			(at 76.2 124.46 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Capacitor; Footprint 0603; 100nF/50V; X7R"
			(at 76.2 124.46 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Capacitance" "100nF"
			(at 80.01 124.4599 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Voltage" "50V"
			(at 80.01 126.9999 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Dielectric" "X7R"
			(at 76.2 124.46 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 76.2 134.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "CL10B104KB8NNNC"
			(at 76.2 137.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "1276-1000-1-ND"
			(at 76.2 139.7 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "187-CL10B104KB8NNNC"
			(at 76.2 142.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "1301804"
			(at 76.2 144.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "CL10B104KB8NNNC"
			(at 76.2 147.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "AVX Corporation"
			(at 100.33 134.62 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "06035C104KAT4A"
			(at 100.33 137.16 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "baef1c68-db76-4a78-8cc2-c903ebe1e133")
		)
		(pin "2"
			(uuid "60442205-9415-428b-8776-7e82ff24b63a")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 208.28 53.34 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "6b6eb0ee-1c61-49ca-8601-8a4a21b8320b")
		(property "Reference" "R13"
			(at 205.74 52.0699 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 208.28 58.42 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 208.28 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 208.28 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 208.28 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 205.74 54.6099 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 200.66 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 200.66 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 208.28 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 208.28 66.04 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 187.96 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 187.96 66.04 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 208.28 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 208.28 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 208.28 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 208.28 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "d11ab1c1-b0b0-4096-95ae-707732d28736")
		)
		(pin "1"
			(uuid "43b701e2-dfa9-4a9a-97d7-f557100fa4e5")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:AO3401A")
		(at 233.68 100.33 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "6bf69b31-8360-4d2e-958d-52b9d165eddf")
		(property "Reference" "Q3"
			(at 228.6 99.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "AO3401A"
			(at 228.6 101.092 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 228.6 98.425 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 228.6 96.52 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 233.68 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "621-DMP3130L-7"
			(at 233.68 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "b6e690c6-686b-4bd5-babe-bd5c18585a56")
		)
		(pin "2"
			(uuid "b1b2a2cc-4bf8-433d-8683-5d43fdd6f309")
		)
		(pin "3"
			(uuid "30f4531b-74fe-4ae2-af3f-f178b8178941")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 240.03 118.11 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "72470202-6b0e-4a8b-ab5c-e3ae8d9ce6d3")
		(property "Reference" "R10"
			(at 234.95 116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 240.03 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 240.03 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 240.03 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 240.03 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 234.95 119.38 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 247.65 116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 247.65 119.38 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 240.03 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 240.03 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 260.35 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 260.35 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 240.03 133.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 240.03 135.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 240.03 138.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 240.03 140.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "aa7c8a60-5111-4e74-beb1-3ad6e0391613")
		)
		(pin "1"
			(uuid "42250142-8b3f-4e74-9f4a-b7731366d7f8")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 170.18 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "728f1127-6b90-4b46-8546-a2086f628ff9")
		(property "Reference" "R11"
			(at 172.72 114.2999 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 170.18 120.65 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 170.18 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 170.18 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 170.18 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 172.72 116.8399 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 177.8 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 177.8 116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 170.18 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 170.18 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 190.5 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 190.5 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 170.18 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 170.18 133.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 170.18 135.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 170.18 138.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "bcc9c936-2993-4c84-a1c4-4fd57c899862")
		)
		(pin "1"
			(uuid "21f0ce07-c35e-4c5a-a078-4acd29f356a2")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 190.5 100.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "74b30c3a-13e4-4dce-a0fd-2de7991f1c9a")
		(property "Reference" "R4"
			(at 190.5 93.98 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 195.58 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 198.12 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 190.5 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 190.5 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 190.5 96.52 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 189.23 92.71 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 191.77 92.71 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 200.66 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 203.2 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 200.66 80.01 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 203.2 80.01 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 205.74 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 208.28 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 210.82 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 213.36 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "779796df-122b-4c23-9be9-b8da8d451a61")
		)
		(pin "1"
			(uuid "23a9faee-cee3-476b-9927-adfb9a33f6c4")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Capacitors:C0603_100nF_50V_X7R")
		(at 116.84 49.53 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "7559fd36-5b9b-42e9-b05b-bc4d5d4c9aa0")
		(property "Reference" "C1"
			(at 120.65 46.9899 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Value" "C0603_100nF_50V_X7R"
			(at 116.84 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Capacitors:C0603"
			(at 116.84 41.91 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.samsungsem.com/kr/support/product-search/mlcc/CL10B104KB8NNNC.jsp"
			(at 116.84 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Capacitor; Footprint 0603; 100nF/50V; X7R"
			(at 116.84 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Capacitance" "100nF"
			(at 120.65 49.5299 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Voltage" "50V"
			(at 120.65 52.0699 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify right)
			)
		)
		(property "Dielectric" "X7R"
			(at 116.84 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Samsung Electro-Mechanics"
			(at 116.84 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "CL10B104KB8NNNC"
			(at 116.84 36.83 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "1276-1000-1-ND"
			(at 116.84 34.29 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "187-CL10B104KB8NNNC"
			(at 116.84 31.75 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "1301804"
			(at 116.84 29.21 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "CL10B104KB8NNNC"
			(at 116.84 26.67 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "AVX Corporation"
			(at 92.71 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "06035C104KAT4A"
			(at 92.71 36.83 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "aeec2b19-502a-4acf-9eff-e9f411de9c7b")
		)
		(pin "2"
			(uuid "4a2d73f5-e826-42b8-b934-dbca3d841201")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:AO3401A")
		(at 201.93 100.33 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "795126b3-a6fe-4130-8394-603c34f45059")
		(property "Reference" "Q2"
			(at 207.264 99.568 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "AO3401A"
			(at 207.264 101.346 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 207.01 98.425 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3401A.pdf"
			(at 207.01 96.52 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "-4.0A Id, -30V Vds, P-Channel MOSFET, SOT-23"
			(at 201.93 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "621-DMP3130L-7"
			(at 201.93 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "d29a7f80-20dc-4f11-8aad-d56e35a49fdc")
		)
		(pin "2"
			(uuid "5b5b1273-aa24-41c2-9653-753aeb03c5ac")
		)
		(pin "3"
			(uuid "d37be001-e1b4-4ef4-8c28-8ade7060ac2f")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 166.37 106.68 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "7b559ad2-89c6-4c5f-9a56-d70d11522c66")
		(property "Reference" "R1"
			(at 166.37 100.33 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 171.45 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 173.99 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 166.37 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 166.37 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 166.37 102.87 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 165.1 99.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 167.64 99.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 176.53 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 179.07 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 176.53 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 179.07 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 181.61 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 184.15 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 186.69 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 189.23 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "bf914828-7066-47d6-a18c-6d05b0f6cad5")
		)
		(pin "1"
			(uuid "54083685-2c4d-45fa-b7fe-4a5ca1efcd06")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 217.17 123.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "902f9bb0-c2ed-4e79-8e3d-2d5bc15d3e3d")
		(property "Reference" "#PWR02"
			(at 217.17 129.54 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 217.17 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 217.17 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 217.17 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 217.17 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "0bdac112-00e2-4199-a3db-7e2a3e3fd01d")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 208.28 63.5 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "94c452c1-d8f3-4e46-a2dd-3e7d53db5856")
		(property "Reference" "R15"
			(at 205.74 62.2299 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 208.28 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 208.28 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 208.28 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 208.28 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 205.74 64.7699 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 200.66 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 200.66 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 208.28 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 208.28 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 187.96 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 187.96 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 208.28 78.74 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 208.28 81.28 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 208.28 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 208.28 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "871207cd-375a-4b31-96ce-768271258c0b")
		)
		(pin "1"
			(uuid "eb685dd1-45da-4024-bc6a-5b9f0ad5961e")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Connectors:SWD_Connector")
		(at 43.18 132.08 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "96d465ab-3ae3-4492-b419-e16ba2190abc")
		(property "Reference" "SWD2"
			(at 50.8 130.8099 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "SWD_Connector"
			(at 50.8 133.3499 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "VL_Connectors:SWD_Connector_for_PogoHeader"
			(at 44.45 142.24 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 31.75 139.7 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "SMD Connector for programming ARM MCUs using a spring-loaded header"
			(at 43.18 132.08 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "X"
			(at 44.45 147.32 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "X"
			(at 44.45 149.86 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "X"
			(at 44.45 152.4 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "X"
			(at 44.45 144.78 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "35263cb4-52d3-40ca-acb2-0538cdc34679")
		)
		(pin "2"
			(uuid "e9bda9da-9588-4214-85c6-36e28d3fce08")
		)
		(pin "3"
			(uuid "daf2d7bd-2118-4a53-971e-8a600b6ba82f")
		)
		(pin "4"
			(uuid "9cada563-ca9b-4b24-82ff-5615155a76cd")
		)
		(pin "5"
			(uuid "3317fffc-3c55-4bc6-a468-e244fa5acfbc")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "SWD2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 180.34 39.37 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "9b2930ab-4297-400c-ad5a-7db291f14ef5")
		(property "Reference" "R21"
			(at 180.34 33.02 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 185.42 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 187.96 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 180.34 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 180.34 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 180.34 35.56 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 179.07 31.75 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 181.61 31.75 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 190.5 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 193.04 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 190.5 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 193.04 19.05 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 195.58 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 198.12 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 200.66 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 203.2 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "2899df86-093c-484b-a714-4e5ff4c464f7")
		)
		(pin "1"
			(uuid "becd3134-0d19-4ec9-ab08-b4de40eed50a")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R21")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 168.91 62.23 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "a276587b-f6bc-4735-9843-620c456b9c83")
		(property "Reference" "#PWR010"
			(at 168.91 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 168.91 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 168.91 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 168.91 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 168.91 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "b70c1ebe-f48b-4cd5-a2f0-c9df042787a6")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 269.24 106.68 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "a727ac8e-3bb2-4878-9ff5-191ff6d6f032")
		(property "Reference" "R7"
			(at 269.24 100.33 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 264.16 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 261.62 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 269.24 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 269.24 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 269.24 102.87 90)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power" "1/16W"
			(at 270.51 99.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 267.97 99.06 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 259.08 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 256.54 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 259.08 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 256.54 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 254 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 251.46 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 248.92 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 246.38 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "6464f6e4-025d-4ed6-ab99-064c9dc45a24")
		)
		(pin "1"
			(uuid "caa64d24-a004-42c7-a56e-4929c7625a20")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:AO3400A")
		(at 233.68 114.3 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "a796499e-29c7-495d-a347-bdf2f0aa4cdc")
		(property "Reference" "Q4"
			(at 228.854 114.046 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "AO3400A"
			(at 228.854 116.078 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 228.6 116.205 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf"
			(at 228.6 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"
			(at 233.68 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "522-ZXMN3B14FTA"
			(at 233.68 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "3b9e1f1a-400b-4dbd-9f98-7da3fcba98f1")
		)
		(pin "2"
			(uuid "64743766-d555-42a1-ac80-13ca3c9b099f")
		)
		(pin "3"
			(uuid "c7fd9a4d-1606-4bb2-a8f7-f360b931b01b")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Generic:Conn_01x02")
		(at 218.44 113.03 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "a9bb3e2f-94fa-4d83-bdd1-3568e5cf71c1")
		(property "Reference" "J3"
			(at 215.646 104.14 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "Conn_01x02"
			(at 211.074 105.918 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "VL_Connectors:Solder_Pads_Thin_1x2"
			(at 218.44 113.03 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "~"
			(at 218.44 113.03 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 218.44 113.03 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "817810f4-12da-486b-97f5-b6ab390da48a")
		)
		(pin "1"
			(uuid "a2358974-4710-4853-a29f-bf4c360bfa7c")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Transistor_FET:AO3400A")
		(at 201.93 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "ae5f522b-4f4a-4b86-b34e-74a286e1a100")
		(property "Reference" "Q1"
			(at 207.01 114.046 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "AO3400A"
			(at 207.01 116.078 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 207.01 116.205 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "http://www.aosmd.com/pdfs/datasheet/AO3400A.pdf"
			(at 207.01 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "30V Vds, 5.7A Id, N-Channel MOSFET, SOT-23"
			(at 201.93 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "522-ZXMN3B14FTA"
			(at 201.93 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "c4c16e50-c3ff-457b-bc6c-e8624aad16ab")
		)
		(pin "2"
			(uuid "5148892b-1ad4-4ba6-95ce-507b4bd9989f")
		)
		(pin "3"
			(uuid "f18c8711-3b90-48a7-ab30-da99ac468451")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 208.28 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "afefd5a0-4324-4136-9e6a-81f378d39a54")
		(property "Reference" "#PWR08"
			(at 208.28 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 208.28 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 208.28 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 208.28 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 208.28 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "7cd11313-a106-4aa5-b3f7-ababf7f34331")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 218.44 63.5 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "b6253409-e80d-4bc6-91ba-54c0179bdf90")
		(property "Reference" "R17"
			(at 220.98 62.2299 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 218.44 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 218.44 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 218.44 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 218.44 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 220.98 64.7699 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 226.06 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 226.06 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 218.44 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 218.44 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 238.76 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 238.76 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 218.44 78.74 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 218.44 81.28 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 218.44 83.82 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 218.44 86.36 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "c0ee7bc8-d2f9-4fe7-9919-3615bf2c7c46")
		)
		(pin "1"
			(uuid "44a99b12-da41-4cd4-9d14-36d84a054e3b")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 256.54 95.25 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "b730dfbe-bbc9-4486-988d-e610c6a29e45")
		(property "Reference" "R8"
			(at 254 93.9799 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 256.54 100.33 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 256.54 102.87 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 256.54 95.25 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 256.54 95.25 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 254 96.5199 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 248.92 93.98 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 248.92 96.52 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 256.54 105.41 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 256.54 107.95 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 236.22 105.41 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 236.22 107.95 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 256.54 110.49 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 256.54 113.03 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 256.54 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 256.54 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "6cb0315b-1585-40ed-bb37-bab1eec128eb")
		)
		(pin "1"
			(uuid "385c1a4b-a241-4b6b-8da0-dfc0ab83b76a")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 168.91 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "c1a6b862-098a-40cd-b2dd-4b4cd9ef428e")
		(property "Reference" "R20"
			(at 171.45 33.0199 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 168.91 39.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 168.91 41.91 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 168.91 34.29 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 168.91 34.29 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 171.45 35.5599 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 176.53 33.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 176.53 35.56 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 168.91 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 168.91 46.99 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 189.23 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 189.23 46.99 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 168.91 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 168.91 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 168.91 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 168.91 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "46d1aeb0-bacd-4ed6-92dc-04eb7ebf88fc")
		)
		(pin "1"
			(uuid "134610e5-115e-451e-8c13-7962727f9826")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R20")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 107.95 160.02 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "c7cffe84-1417-4c4b-b4ac-7b1ba84716d8")
		(property "Reference" "#PWR015"
			(at 107.95 166.37 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 107.95 165.1 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 107.95 160.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 107.95 160.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 107.95 160.02 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "38437dff-3ab4-4617-aa62-7c5b2f5a5241")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_1k_1%_1d16W")
		(at 218.44 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "c9328204-4663-49fb-8f1b-78ca8e703a0c")
		(property "Reference" "R16"
			(at 220.98 52.0699 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_1k_1%_1d16W"
			(at 218.44 58.42 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 218.44 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-AC_51_RoHS_L_7.pdf"
			(at 218.44 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 1 kOhm; 1%; 1/16W"
			(at 218.44 53.34 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "1k"
			(at 220.98 54.6099 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 226.06 52.07 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "1%"
			(at 226.06 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 218.44 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "AC0402FR-071KL"
			(at 218.44 66.04 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "TE Connectivity Passive Product"
			(at 238.76 63.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CRGCQ0402F1K0"
			(at 238.76 66.04 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-1KLBCT-ND"
			(at 218.44 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-AC0402FR-071KL"
			(at 218.44 71.12 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3495181"
			(at 218.44 73.66 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-1K-1%"
			(at 218.44 76.2 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "61ab4d14-f2f1-4316-bf45-279b77cc0085")
		)
		(pin "1"
			(uuid "e8acce2e-f5df-4401-85ae-6def20f1f0af")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 104.14 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "d76d995b-da0a-4134-a23c-14e9896752da")
		(property "Reference" "#PWR04"
			(at 104.14 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 104.14 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 104.14 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 104.14 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 104.14 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "884da80e-441c-40bf-90f4-a0c57bc62b4d")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 71.12 54.61 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "d77c7ccd-aade-4393-9610-abf518dff4ff")
		(property "Reference" "#PWR06"
			(at 71.12 60.96 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 71.12 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 71.12 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 71.12 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 71.12 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "1fdd7d5f-8d82-40d2-a5e2-128e6866d2d2")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Other:0ZCJ0050AF2E")
		(at 257.81 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "d7809ccb-9574-4beb-8e07-d8c3fe3712e3")
		(property "Reference" "F3"
			(at 257.81 43.18 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "0ZCJ0050AF2E"
			(at 257.81 45.72 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "VL_Other:F1206"
			(at 257.81 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://cz.mouser.com/datasheet/2/643/ds_CP_0zcj_series-1664160.pdf"
			(at 257.81 44.45 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Polymeric PTC Resettable Fuse 24V 500mA Ih Surface Mount 1206 (3216 Metric)"
			(at 257.81 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Bel Fuse Inc."
			(at 257.81 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "0ZCJ0050AF2E"
			(at 257.81 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Eaton - Electronics Division"
			(at 284.48 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "PTS120615V050"
			(at 285.75 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "507-1803-1-ND"
			(at 257.81 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "530-0ZCJ0050AF2E"
			(at 257.81 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "2834888"
			(at 257.81 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" " 0ZCJ0050AF2E"
			(at 257.81 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "a96e8f8c-a10d-4f5f-a9ef-8a1f317772d6")
		)
		(pin "2"
			(uuid "78276c1c-2448-41a0-a55d-aff555918c72")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "F3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 43.18 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "de8a96de-680e-4759-a8a4-d484ab10a2b7")
		(property "Reference" "#PWR01"
			(at 43.18 68.58 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "GND"
			(at 43.18 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 43.18 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 43.18 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 43.18 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "ab38a9ed-b79f-42f1-a319-6dd513d04f5c")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Capacitors:C0402_1uF_35V_X5R")
		(at 71.12 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "dfeeb10e-9715-46cb-9ffe-70580bc11b58")
		(property "Reference" "C5"
			(at 74.93 46.9899 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "C0402_1uF_35V_X5R"
			(at 71.12 54.61 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Capacitors:C0402"
			(at 71.12 57.15 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://product.tdk.com/info/en/catalog/datasheets/mlcc_commercial_soft_en.pdf?ref_disty=digikey"
			(at 71.12 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Capacitor; Footprint 0402; 1uF/35V; X5R"
			(at 71.12 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Capacitance" "1uF"
			(at 74.93 49.5299 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Voltage" "35V"
			(at 74.93 52.0699 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Dielectric" "X5R"
			(at 71.12 49.53 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "TDK Corporation"
			(at 71.12 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "C1005X5R1V105K050BE"
			(at 71.12 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "445-175218-1-ND"
			(at 71.12 64.77 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "810-C1005X5R1V105K"
			(at 71.12 67.31 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3416060"
			(at 71.12 69.85 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "X"
			(at 71.12 72.39 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Kyocera International Inc. Electronic Components"
			(at 93.98 59.69 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "CM05X5R105K35AH"
			(at 93.98 62.23 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "993b48ff-c67c-48b7-968a-a9fcd0421535")
		)
		(pin "1"
			(uuid "c2e3cf8c-d0c2-4034-b53b-b718403b6c7b")
		)
		(instances
			(project ""
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Transistors:2N7002NXAKR")
		(at 259.08 106.68 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(uuid "e13bc886-78c2-4dca-b28c-65fa4bccd316")
		(property "Reference" "Q6"
			(at 252.73 105.4099 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "2N7002NXAKR"
			(at 253.746 108.458 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Footprint" "VL_SOT:SOT-23"
			(at 265.43 120.65 0)
			(effects
				(font
					(size 1.27 1.27)
					(italic yes)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/2N7002NXAK.pdf"
			(at 279.4 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 259.08 106.68 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Nexperia USA Inc."
			(at 259.08 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "2N7002NXAKR"
			(at 259.08 118.11 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "1727-8643-1-ND"
			(at 259.08 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "771-2N7002NXAKR"
			(at 259.08 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "3226400"
			(at 259.08 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "2N7002NXAKR"
			(at 259.08 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "1"
			(uuid "f4631afb-7377-494b-88f1-6a5decc2efad")
		)
		(pin "2"
			(uuid "3315d879-661b-4a37-ad98-1312c47d3106")
		)
		(pin "3"
			(uuid "642edeae-7eeb-4529-8e52-064e2446959a")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "Q6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "VL_Resistors:R0402_10k_5%_1d16W")
		(at 265.43 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "f1c38f0b-7f66-4e65-ad46-205b1e3971ea")
		(property "Reference" "R12"
			(at 267.97 114.2999 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Value" "R0402_10k_5%_1d16W"
			(at 265.43 120.65 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" "VL_Resistors:R0402"
			(at 265.43 123.19 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/rchip/PYu-RC_Group_51_RoHS_L_11.pdf"
			(at 265.43 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" "Resistor; Footprint 0402; 10 kOhm; 5%; 1/16W"
			(at 265.43 115.57 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Resistance" "10k"
			(at 267.97 116.8399 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left)
			)
		)
		(property "Power" "1/16W"
			(at 273.05 114.3 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Precision" "5%"
			(at 273.05 116.84 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Manufacturer" "Yageo"
			(at 265.43 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Code" "RC0402JR-0710KL"
			(at 265.43 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Manufacturer" "Stackpole Electronics Inc"
			(at 285.75 125.73 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Alt_Code" "RMCF0402JT10K0"
			(at 285.75 128.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Digikey" "311-10KJRCT-ND"
			(at 265.43 130.81 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Mouser" "603-RC0402JR-0710KL"
			(at 265.43 133.35 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Farnell" "*"
			(at 265.43 135.89 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "TME" "SMD0402-10K"
			(at 265.43 138.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(pin "2"
			(uuid "3fb20428-d84a-426c-b0ff-7ae8661ead1e")
		)
		(pin "1"
			(uuid "21b84e25-3a1f-4591-b33c-d150e626f8fc")
		)
		(instances
			(project "led_driver"
				(path "/4e49d584-f650-4a4e-ae26-e0322eda8233"
					(reference "R12")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path "/"
			(page "1")
		)
	)
	(embedded_fonts no)
)
