#MicroXplorer Configuration settings - do not modify
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C1.IPParameters=Timing
I2C1.Timing=0x40000A0B
IWDG.IPParameters=Prescaler
IWDG.Prescaler=IWDG_PRESCALER_256
KeepUserPlacement=false
Mcu.Family=STM32L0
Mcu.IP0=I2C1
Mcu.IP1=IWDG
Mcu.IP2=NVIC
Mcu.IP3=RCC
Mcu.IP4=SYS
Mcu.IP5=TIM2
Mcu.IP6=TIM21
Mcu.IP7=TIM22
Mcu.IP8=USART2
Mcu.IPNb=9
Mcu.Name=STM32L031G(4-6)Ux
Mcu.Package=UFQFPN28
Mcu.Pin0=PA1
Mcu.Pin1=PA2
Mcu.Pin10=VP_IWDG_VS_IWDG
Mcu.Pin11=VP_SYS_VS_Systick
Mcu.Pin12=VP_TIM21_VS_ClockSourceINT
Mcu.Pin2=PA3
Mcu.Pin3=PA5
Mcu.Pin4=PA6
Mcu.Pin5=PA7
Mcu.Pin6=PA9
Mcu.Pin7=PA10
Mcu.Pin8=PA13
Mcu.Pin9=PA14
Mcu.PinsNb=13
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32L031G6Ux
MxCube.Version=6.3.0
MxDb.Version=DB.6.0.30
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SVC_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SysTick_IRQn=true\:3\:0\:false\:false\:true\:false\:true
NVIC.TIM21_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.USART2_IRQn=true\:0\:0\:false\:false\:true\:true\:true
PA1.Mode=Hardware Flow Control (RS485)
PA1.Signal=USART2_DE
PA10.GPIOParameters=GPIO_Pu
PA10.GPIO_Pu=GPIO_PULLUP
PA10.Mode=I2C
PA10.Signal=I2C1_SDA
PA13.Mode=Serial_Wire
PA13.Signal=SYS_SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_SWCLK
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.Mode=Asynchronous
PA3.Signal=USART2_RX
PA5.Locked=true
PA5.Signal=S_TIM2_CH1
PA6.Locked=true
PA6.Signal=S_TIM22_CH1
PA7.Locked=true
PA7.Signal=S_TIM22_CH2
PA9.GPIOParameters=GPIO_Pu
PA9.GPIO_Pu=GPIO_PULLUP
PA9.Mode=I2C
PA9.Signal=I2C1_SCL
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32L031G6Ux
ProjectManager.FirmwarePackage=STM32Cube FW_L0 V1.12.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=iaq_wired_sensor.ioc
ProjectManager.ProjectName=iaq_wired_sensor
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-LL-false,2-MX_GPIO_Init-GPIO-false-LL-true,3-MX_I2C1_Init-I2C1-false-LL-true,4-MX_USART2_UART_Init-USART2-false-LL-true,5-MX_TIM21_Init-TIM21-false-LL-true,6-MX_TIM2_Init-TIM2-false-LL-true,7-MX_TIM22_Init-TIM22-false-LL-true,8-MX_IWDG_Init-IWDG-false-LL-true
RCC.AHBFreq_Value=12000000
RCC.APB1Freq_Value=12000000
RCC.APB1TimFreq_Value=12000000
RCC.APB2Freq_Value=12000000
RCC.APB2TimFreq_Value=12000000
RCC.FCLKCortexFreq_Value=12000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=12000000
RCC.HSE_VALUE=8000000
RCC.HSI16_VALUE=16000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=12000000
RCC.IPParameters=AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI16_VALUE,HSI_VALUE,I2C1Freq_Value,LPTIMFreq_Value,LPUARTFreq_Value,LSE_VALUE,LSI_VALUE,MCOPinFreq_Value,MSI_VALUE,PLLCLKFreq_Value,PLLDIV,PWRFreq_Value,RTCFreq_Value,RTCHSEDivFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,TIMFreq_Value,TimerFreq_Value,USART2Freq_Value,VCOOutputFreq_Value,WatchDogFreq_Value
RCC.LPTIMFreq_Value=12000000
RCC.LPUARTFreq_Value=12000000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=37000
RCC.MCOPinFreq_Value=12000000
RCC.MSI_VALUE=2097000
RCC.PLLCLKFreq_Value=12000000
RCC.PLLDIV=RCC_PLLDIV_4
RCC.PWRFreq_Value=12000000
RCC.RTCFreq_Value=37000
RCC.RTCHSEDivFreq_Value=4000000
RCC.SYSCLKFreq_VALUE=12000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.TIMFreq_Value=12000000
RCC.TimerFreq_Value=12000000
RCC.USART2Freq_Value=12000000
RCC.VCOOutputFreq_Value=48000000
RCC.WatchDogFreq_Value=37000
SH.S_TIM22_CH1.0=TIM22_CH1,PWM Generation1 CH1
SH.S_TIM22_CH1.ConfNb=1
SH.S_TIM22_CH2.0=TIM22_CH2,PWM Generation2 CH2
SH.S_TIM22_CH2.ConfNb=1
SH.S_TIM2_CH1.0=TIM2_CH1,PWM Generation1 CH1
SH.S_TIM2_CH1.ConfNb=1
TIM2.Channel-PWM\ Generation1\ CH1=TIM_CHANNEL_1
TIM2.IPParameters=Channel-PWM Generation1 CH1,Prescaler,Period
TIM2.IPParametersWithoutCheck=Prescaler,Period
TIM2.Period=RGBLED_PERIOD
TIM2.Prescaler=RGBLED_PRESCALER
TIM21.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM21.IPParameters=Prescaler,Period,AutoReloadPreload
TIM21.IPParametersWithoutCheck=Prescaler,Period
TIM21.Period=tim21_period
TIM21.Prescaler=tim21_prescaler
TIM22.Channel-PWM\ Generation1\ CH1=TIM_CHANNEL_1
TIM22.Channel-PWM\ Generation2\ CH2=TIM_CHANNEL_2
TIM22.IPParameters=Channel-PWM Generation1 CH1,Channel-PWM Generation2 CH2,Pulse-PWM Generation1 CH1,Period,Prescaler
TIM22.IPParametersWithoutCheck=Prescaler,Period
TIM22.Period=RGBLED_PERIOD
TIM22.Prescaler=RGBLED_PRESCALER
TIM22.Pulse-PWM\ Generation1\ CH1=0
USART2.BaudRate=config_baudrates[sensor_config.baudrate_index]
USART2.IPParameters=VirtualMode-Asynchronous,VirtualMode-Hardware Flow Control (RS485),BaudRate,WordLength,Parity
USART2.IPParametersWithoutCheck=BaudRate
USART2.Parity=PARITY_EVEN
USART2.VirtualMode-Asynchronous=VM_ASYNC
USART2.VirtualMode-Hardware\ Flow\ Control\ (RS485)=VM_ASYNC
USART2.WordLength=WORDLENGTH_9B
VP_IWDG_VS_IWDG.Mode=IWDG_Activate
VP_IWDG_VS_IWDG.Signal=IWDG_VS_IWDG
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM21_VS_ClockSourceINT.Mode=Internal
VP_TIM21_VS_ClockSourceINT.Signal=TIM21_VS_ClockSourceINT
board=custom
isbadioc=false
