#MicroXplorer Configuration settings - do not modify
File.Version=6
GPIO.groupedBy=Group By Peripherals
I2C1.IPParameters=Timing
I2C1.Timing=0x40000A0B
KeepUserPlacement=false
LPUART1.BaudRate=115200
LPUART1.IPParameters=BaudRate,SwapParam,OneBitSampling,WordLength,Parity
LPUART1.OneBitSampling=UART_ONE_BIT_SAMPLE_ENABLE
LPUART1.Parity=UART_PARITY_EVEN
LPUART1.SwapParam=UART_ADVFEATURE_SWAP_ENABLE
LPUART1.WordLength=UART_WORDLENGTH_9B
Mcu.Family=STM32L0
Mcu.IP0=I2C1
Mcu.IP1=LPUART1
Mcu.IP2=NVIC
Mcu.IP3=RCC
Mcu.IP4=SYS
Mcu.IP5=TIM21
Mcu.IPNb=6
Mcu.Name=STM32L011F(3-4)Ux
Mcu.Package=UFQFPN20
Mcu.Pin0=PA0-CK_IN
Mcu.Pin1=PA1
Mcu.Pin10=VP_TIM21_VS_ClockSourceINT
Mcu.Pin2=PA5
Mcu.Pin3=PA6
Mcu.Pin4=PA7
Mcu.Pin5=PA9
Mcu.Pin6=PA10
Mcu.Pin7=PA13
Mcu.Pin8=PA14
Mcu.Pin9=VP_SYS_VS_Systick
Mcu.PinsNb=11
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32L011F4Ux
MxCube.Version=6.2.1
MxDb.Version=DB.6.0.21
NVIC.ForceEnableDMAVector=true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.LPUART1_IRQn=true\:0\:0\:false\:false\:true\:true\:true
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SVC_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.SysTick_IRQn=true\:0\:0\:false\:false\:true\:false\:true
NVIC.TIM21_IRQn=true\:0\:0\:false\:false\:true\:true\:true
PA0-CK_IN.GPIOParameters=GPIO_PuPd
PA0-CK_IN.GPIO_PuPd=GPIO_PULLUP
PA0-CK_IN.Mode=Asynchronous
PA0-CK_IN.Signal=LPUART1_RX
PA1.GPIOParameters=GPIO_PuPd
PA1.GPIO_PuPd=GPIO_PULLUP
PA1.Mode=Asynchronous
PA1.Signal=LPUART1_TX
PA10.Mode=I2C
PA10.Signal=I2C1_SDA
PA13.Mode=Serial_Wire
PA13.Signal=SYS_SWDIO
PA14.Mode=Serial_Wire
PA14.Signal=SYS_SWCLK
PA5.GPIOParameters=PinState,GPIO_Label
PA5.GPIO_Label=LED_B
PA5.Locked=true
PA5.PinState=GPIO_PIN_SET
PA5.Signal=GPIO_Output
PA6.GPIOParameters=PinState,GPIO_Label
PA6.GPIO_Label=LED_G
PA6.Locked=true
PA6.PinState=GPIO_PIN_SET
PA6.Signal=GPIO_Output
PA7.GPIOParameters=PinState,GPIO_Label
PA7.GPIO_Label=LED_R
PA7.Locked=true
PA7.PinState=GPIO_PIN_SET
PA7.Signal=GPIO_Output
PA9.Locked=true
PA9.Mode=I2C
PA9.Signal=I2C1_SCL
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32L011F4Ux
ProjectManager.FirmwarePackage=STM32Cube FW_L0 V1.12.0
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=iaq_wired_sensor.ioc
ProjectManager.ProjectName=iaq_wired_sensor
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-LL-true,2-SystemClock_Config-RCC-false-LL-false,3-MX_I2C1_Init-I2C1-false-LL-true,4-MX_LPUART1_UART_Init-LPUART1-false-LL-true,5-MX_TIM21_Init-TIM21-false-LL-true
RCC.AHBFreq_Value=12000000
RCC.APB1Freq_Value=12000000
RCC.APB1TimFreq_Value=12000000
RCC.APB2Freq_Value=12000000
RCC.APB2TimFreq_Value=12000000
RCC.FCLKCortexFreq_Value=12000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=12000000
RCC.HSE_VALUE=8000000
RCC.HSI16_VALUE=16000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=12000000
RCC.IPParameters=AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI16_VALUE,HSI_VALUE,I2C1Freq_Value,LPTIMFreq_Value,LPUARTFreq_Value,LSE_VALUE,LSI_VALUE,MCOPinFreq_Value,MSI_VALUE,PLLCLKFreq_Value,PLLDIV,PWRFreq_Value,RTCFreq_Value,RTCHSEDivFreq_Value,SYSCLKFreq_VALUE,SYSCLKSource,TIMFreq_Value,TimerFreq_Value,USART2Freq_Value,VCOOutputFreq_Value,WatchDogFreq_Value
RCC.LPTIMFreq_Value=12000000
RCC.LPUARTFreq_Value=12000000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=37000
RCC.MCOPinFreq_Value=12000000
RCC.MSI_VALUE=2097000
RCC.PLLCLKFreq_Value=12000000
RCC.PLLDIV=RCC_PLLDIV_4
RCC.PWRFreq_Value=12000000
RCC.RTCFreq_Value=37000
RCC.RTCHSEDivFreq_Value=4000000
RCC.SYSCLKFreq_VALUE=12000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.TIMFreq_Value=12000000
RCC.TimerFreq_Value=12000000
RCC.USART2Freq_Value=12000000
RCC.VCOOutputFreq_Value=48000000
RCC.WatchDogFreq_Value=37000
TIM21.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_ENABLE
TIM21.ClockDivision=TIM_CLOCKDIVISION_DIV1
TIM21.IPParameters=Prescaler,Period,AutoReloadPreload,ClockDivision
TIM21.IPParametersWithoutCheck=Prescaler,Period
TIM21.Period=tim21_period
TIM21.Prescaler=tim21_prescaler
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM21_VS_ClockSourceINT.Mode=Internal
VP_TIM21_VS_ClockSourceINT.Signal=TIM21_VS_ClockSourceINT
board=custom
