3751000657887794
Connector_PinHeader_2.00mm
PinHeader_1x01_P2.00mm_Horizontal
Through hole angled pin header, 1x01, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x01 2.00mm single row
0
1
1
Connector_PinHeader_2.00mm
PinHeader_1x01_P2.00mm_Vertical
Through hole straight pin header, 1x01, 2.00mm pitch, single row
Through hole pin header THT 1x01 2.00mm single row
0
1
1
Connector_PinHeader_2.00mm
PinHeader_1x02_P2.00mm_Horizontal
Through hole angled pin header, 1x02, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x02 2.00mm single row
0
2
2
Connector_PinHeader_2.00mm
PinHeader_1x02_P2.00mm_Vertical
Through hole straight pin header, 1x02, 2.00mm pitch, single row
Through hole pin header THT 1x02 2.00mm single row
0
2
2
Connector_PinHeader_2.00mm
PinHeader_1x02_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x02, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x02 2.00mm single row style1 pin1 left
0
2
2
Connector_PinHeader_2.00mm
PinHeader_1x02_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x02, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x02 2.00mm single row style2 pin1 right
0
2
2
Connector_PinHeader_2.00mm
PinHeader_1x03_P2.00mm_Horizontal
Through hole angled pin header, 1x03, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x03 2.00mm single row
0
3
3
Connector_PinHeader_2.00mm
PinHeader_1x03_P2.00mm_Vertical
Through hole straight pin header, 1x03, 2.00mm pitch, single row
Through hole pin header THT 1x03 2.00mm single row
0
3
3
Connector_PinHeader_2.00mm
PinHeader_1x03_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x03, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x03 2.00mm single row style1 pin1 left
0
3
3
Connector_PinHeader_2.00mm
PinHeader_1x03_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x03, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x03 2.00mm single row style2 pin1 right
0
3
3
Connector_PinHeader_2.00mm
PinHeader_1x04_P2.00mm_Horizontal
Through hole angled pin header, 1x04, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x04 2.00mm single row
0
4
4
Connector_PinHeader_2.00mm
PinHeader_1x04_P2.00mm_Vertical
Through hole straight pin header, 1x04, 2.00mm pitch, single row
Through hole pin header THT 1x04 2.00mm single row
0
4
4
Connector_PinHeader_2.00mm
PinHeader_1x04_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x04, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x04 2.00mm single row style1 pin1 left
0
4
4
Connector_PinHeader_2.00mm
PinHeader_1x04_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x04, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x04 2.00mm single row style2 pin1 right
0
4
4
Connector_PinHeader_2.00mm
PinHeader_1x05_P2.00mm_Horizontal
Through hole angled pin header, 1x05, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x05 2.00mm single row
0
5
5
Connector_PinHeader_2.00mm
PinHeader_1x05_P2.00mm_Vertical
Through hole straight pin header, 1x05, 2.00mm pitch, single row
Through hole pin header THT 1x05 2.00mm single row
0
5
5
Connector_PinHeader_2.00mm
PinHeader_1x05_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x05, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x05 2.00mm single row style1 pin1 left
0
5
5
Connector_PinHeader_2.00mm
PinHeader_1x05_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x05, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x05 2.00mm single row style2 pin1 right
0
5
5
Connector_PinHeader_2.00mm
PinHeader_1x06_P2.00mm_Horizontal
Through hole angled pin header, 1x06, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x06 2.00mm single row
0
6
6
Connector_PinHeader_2.00mm
PinHeader_1x06_P2.00mm_Vertical
Through hole straight pin header, 1x06, 2.00mm pitch, single row
Through hole pin header THT 1x06 2.00mm single row
0
6
6
Connector_PinHeader_2.00mm
PinHeader_1x06_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x06, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x06 2.00mm single row style1 pin1 left
0
6
6
Connector_PinHeader_2.00mm
PinHeader_1x06_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x06, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x06 2.00mm single row style2 pin1 right
0
6
6
Connector_PinHeader_2.00mm
PinHeader_1x07_P2.00mm_Horizontal
Through hole angled pin header, 1x07, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x07 2.00mm single row
0
7
7
Connector_PinHeader_2.00mm
PinHeader_1x07_P2.00mm_Vertical
Through hole straight pin header, 1x07, 2.00mm pitch, single row
Through hole pin header THT 1x07 2.00mm single row
0
7
7
Connector_PinHeader_2.00mm
PinHeader_1x07_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x07, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x07 2.00mm single row style1 pin1 left
0
7
7
Connector_PinHeader_2.00mm
PinHeader_1x07_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x07, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x07 2.00mm single row style2 pin1 right
0
7
7
Connector_PinHeader_2.00mm
PinHeader_1x08_P2.00mm_Horizontal
Through hole angled pin header, 1x08, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x08 2.00mm single row
0
8
8
Connector_PinHeader_2.00mm
PinHeader_1x08_P2.00mm_Vertical
Through hole straight pin header, 1x08, 2.00mm pitch, single row
Through hole pin header THT 1x08 2.00mm single row
0
8
8
Connector_PinHeader_2.00mm
PinHeader_1x08_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x08, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x08 2.00mm single row style1 pin1 left
0
8
8
Connector_PinHeader_2.00mm
PinHeader_1x08_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x08, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x08 2.00mm single row style2 pin1 right
0
8
8
Connector_PinHeader_2.00mm
PinHeader_1x09_P2.00mm_Horizontal
Through hole angled pin header, 1x09, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x09 2.00mm single row
0
9
9
Connector_PinHeader_2.00mm
PinHeader_1x09_P2.00mm_Vertical
Through hole straight pin header, 1x09, 2.00mm pitch, single row
Through hole pin header THT 1x09 2.00mm single row
0
9
9
Connector_PinHeader_2.00mm
PinHeader_1x09_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x09, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x09 2.00mm single row style1 pin1 left
0
9
9
Connector_PinHeader_2.00mm
PinHeader_1x09_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x09, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x09 2.00mm single row style2 pin1 right
0
9
9
Connector_PinHeader_2.00mm
PinHeader_1x10_P2.00mm_Horizontal
Through hole angled pin header, 1x10, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x10 2.00mm single row
0
10
10
Connector_PinHeader_2.00mm
PinHeader_1x10_P2.00mm_Vertical
Through hole straight pin header, 1x10, 2.00mm pitch, single row
Through hole pin header THT 1x10 2.00mm single row
0
10
10
Connector_PinHeader_2.00mm
PinHeader_1x10_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x10, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x10 2.00mm single row style1 pin1 left
0
10
10
Connector_PinHeader_2.00mm
PinHeader_1x10_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x10, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x10 2.00mm single row style2 pin1 right
0
10
10
Connector_PinHeader_2.00mm
PinHeader_1x11_P2.00mm_Horizontal
Through hole angled pin header, 1x11, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x11 2.00mm single row
0
11
11
Connector_PinHeader_2.00mm
PinHeader_1x11_P2.00mm_Vertical
Through hole straight pin header, 1x11, 2.00mm pitch, single row
Through hole pin header THT 1x11 2.00mm single row
0
11
11
Connector_PinHeader_2.00mm
PinHeader_1x11_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x11, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x11 2.00mm single row style1 pin1 left
0
11
11
Connector_PinHeader_2.00mm
PinHeader_1x11_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x11, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x11 2.00mm single row style2 pin1 right
0
11
11
Connector_PinHeader_2.00mm
PinHeader_1x12_P2.00mm_Horizontal
Through hole angled pin header, 1x12, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x12 2.00mm single row
0
12
12
Connector_PinHeader_2.00mm
PinHeader_1x12_P2.00mm_Vertical
Through hole straight pin header, 1x12, 2.00mm pitch, single row
Through hole pin header THT 1x12 2.00mm single row
0
12
12
Connector_PinHeader_2.00mm
PinHeader_1x12_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x12, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x12 2.00mm single row style1 pin1 left
0
12
12
Connector_PinHeader_2.00mm
PinHeader_1x12_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x12, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x12 2.00mm single row style2 pin1 right
0
12
12
Connector_PinHeader_2.00mm
PinHeader_1x13_P2.00mm_Horizontal
Through hole angled pin header, 1x13, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x13 2.00mm single row
0
13
13
Connector_PinHeader_2.00mm
PinHeader_1x13_P2.00mm_Vertical
Through hole straight pin header, 1x13, 2.00mm pitch, single row
Through hole pin header THT 1x13 2.00mm single row
0
13
13
Connector_PinHeader_2.00mm
PinHeader_1x13_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x13, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x13 2.00mm single row style1 pin1 left
0
13
13
Connector_PinHeader_2.00mm
PinHeader_1x13_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x13, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x13 2.00mm single row style2 pin1 right
0
13
13
Connector_PinHeader_2.00mm
PinHeader_1x14_P2.00mm_Horizontal
Through hole angled pin header, 1x14, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x14 2.00mm single row
0
14
14
Connector_PinHeader_2.00mm
PinHeader_1x14_P2.00mm_Vertical
Through hole straight pin header, 1x14, 2.00mm pitch, single row
Through hole pin header THT 1x14 2.00mm single row
0
14
14
Connector_PinHeader_2.00mm
PinHeader_1x14_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x14, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x14 2.00mm single row style1 pin1 left
0
14
14
Connector_PinHeader_2.00mm
PinHeader_1x14_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x14, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x14 2.00mm single row style2 pin1 right
0
14
14
Connector_PinHeader_2.00mm
PinHeader_1x15_P2.00mm_Horizontal
Through hole angled pin header, 1x15, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x15 2.00mm single row
0
15
15
Connector_PinHeader_2.00mm
PinHeader_1x15_P2.00mm_Vertical
Through hole straight pin header, 1x15, 2.00mm pitch, single row
Through hole pin header THT 1x15 2.00mm single row
0
15
15
Connector_PinHeader_2.00mm
PinHeader_1x15_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x15, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x15 2.00mm single row style1 pin1 left
0
15
15
Connector_PinHeader_2.00mm
PinHeader_1x15_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x15, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x15 2.00mm single row style2 pin1 right
0
15
15
Connector_PinHeader_2.00mm
PinHeader_1x16_P2.00mm_Horizontal
Through hole angled pin header, 1x16, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x16 2.00mm single row
0
16
16
Connector_PinHeader_2.00mm
PinHeader_1x16_P2.00mm_Vertical
Through hole straight pin header, 1x16, 2.00mm pitch, single row
Through hole pin header THT 1x16 2.00mm single row
0
16
16
Connector_PinHeader_2.00mm
PinHeader_1x16_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x16, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x16 2.00mm single row style1 pin1 left
0
16
16
Connector_PinHeader_2.00mm
PinHeader_1x16_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x16, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x16 2.00mm single row style2 pin1 right
0
16
16
Connector_PinHeader_2.00mm
PinHeader_1x17_P2.00mm_Horizontal
Through hole angled pin header, 1x17, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x17 2.00mm single row
0
17
17
Connector_PinHeader_2.00mm
PinHeader_1x17_P2.00mm_Vertical
Through hole straight pin header, 1x17, 2.00mm pitch, single row
Through hole pin header THT 1x17 2.00mm single row
0
17
17
Connector_PinHeader_2.00mm
PinHeader_1x17_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x17, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x17 2.00mm single row style1 pin1 left
0
17
17
Connector_PinHeader_2.00mm
PinHeader_1x17_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x17, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x17 2.00mm single row style2 pin1 right
0
17
17
Connector_PinHeader_2.00mm
PinHeader_1x18_P2.00mm_Horizontal
Through hole angled pin header, 1x18, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x18 2.00mm single row
0
18
18
Connector_PinHeader_2.00mm
PinHeader_1x18_P2.00mm_Vertical
Through hole straight pin header, 1x18, 2.00mm pitch, single row
Through hole pin header THT 1x18 2.00mm single row
0
18
18
Connector_PinHeader_2.00mm
PinHeader_1x18_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x18, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x18 2.00mm single row style1 pin1 left
0
18
18
Connector_PinHeader_2.00mm
PinHeader_1x18_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x18, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x18 2.00mm single row style2 pin1 right
0
18
18
Connector_PinHeader_2.00mm
PinHeader_1x19_P2.00mm_Horizontal
Through hole angled pin header, 1x19, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x19 2.00mm single row
0
19
19
Connector_PinHeader_2.00mm
PinHeader_1x19_P2.00mm_Vertical
Through hole straight pin header, 1x19, 2.00mm pitch, single row
Through hole pin header THT 1x19 2.00mm single row
0
19
19
Connector_PinHeader_2.00mm
PinHeader_1x19_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x19, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x19 2.00mm single row style1 pin1 left
0
19
19
Connector_PinHeader_2.00mm
PinHeader_1x19_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x19, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x19 2.00mm single row style2 pin1 right
0
19
19
Connector_PinHeader_2.00mm
PinHeader_1x20_P2.00mm_Horizontal
Through hole angled pin header, 1x20, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x20 2.00mm single row
0
20
20
Connector_PinHeader_2.00mm
PinHeader_1x20_P2.00mm_Vertical
Through hole straight pin header, 1x20, 2.00mm pitch, single row
Through hole pin header THT 1x20 2.00mm single row
0
20
20
Connector_PinHeader_2.00mm
PinHeader_1x20_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x20, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x20 2.00mm single row style1 pin1 left
0
20
20
Connector_PinHeader_2.00mm
PinHeader_1x20_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x20, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x20 2.00mm single row style2 pin1 right
0
20
20
Connector_PinHeader_2.00mm
PinHeader_1x21_P2.00mm_Horizontal
Through hole angled pin header, 1x21, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x21 2.00mm single row
0
21
21
Connector_PinHeader_2.00mm
PinHeader_1x21_P2.00mm_Vertical
Through hole straight pin header, 1x21, 2.00mm pitch, single row
Through hole pin header THT 1x21 2.00mm single row
0
21
21
Connector_PinHeader_2.00mm
PinHeader_1x21_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x21, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x21 2.00mm single row style1 pin1 left
0
21
21
Connector_PinHeader_2.00mm
PinHeader_1x21_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x21, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x21 2.00mm single row style2 pin1 right
0
21
21
Connector_PinHeader_2.00mm
PinHeader_1x22_P2.00mm_Horizontal
Through hole angled pin header, 1x22, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x22 2.00mm single row
0
22
22
Connector_PinHeader_2.00mm
PinHeader_1x22_P2.00mm_Vertical
Through hole straight pin header, 1x22, 2.00mm pitch, single row
Through hole pin header THT 1x22 2.00mm single row
0
22
22
Connector_PinHeader_2.00mm
PinHeader_1x22_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x22, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x22 2.00mm single row style1 pin1 left
0
22
22
Connector_PinHeader_2.00mm
PinHeader_1x22_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x22, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x22 2.00mm single row style2 pin1 right
0
22
22
Connector_PinHeader_2.00mm
PinHeader_1x23_P2.00mm_Horizontal
Through hole angled pin header, 1x23, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x23 2.00mm single row
0
23
23
Connector_PinHeader_2.00mm
PinHeader_1x23_P2.00mm_Vertical
Through hole straight pin header, 1x23, 2.00mm pitch, single row
Through hole pin header THT 1x23 2.00mm single row
0
23
23
Connector_PinHeader_2.00mm
PinHeader_1x23_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x23, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x23 2.00mm single row style1 pin1 left
0
23
23
Connector_PinHeader_2.00mm
PinHeader_1x23_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x23, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x23 2.00mm single row style2 pin1 right
0
23
23
Connector_PinHeader_2.00mm
PinHeader_1x24_P2.00mm_Horizontal
Through hole angled pin header, 1x24, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x24 2.00mm single row
0
24
24
Connector_PinHeader_2.00mm
PinHeader_1x24_P2.00mm_Vertical
Through hole straight pin header, 1x24, 2.00mm pitch, single row
Through hole pin header THT 1x24 2.00mm single row
0
24
24
Connector_PinHeader_2.00mm
PinHeader_1x24_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x24, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x24 2.00mm single row style1 pin1 left
0
24
24
Connector_PinHeader_2.00mm
PinHeader_1x24_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x24, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x24 2.00mm single row style2 pin1 right
0
24
24
Connector_PinHeader_2.00mm
PinHeader_1x25_P2.00mm_Horizontal
Through hole angled pin header, 1x25, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x25 2.00mm single row
0
25
25
Connector_PinHeader_2.00mm
PinHeader_1x25_P2.00mm_Vertical
Through hole straight pin header, 1x25, 2.00mm pitch, single row
Through hole pin header THT 1x25 2.00mm single row
0
25
25
Connector_PinHeader_2.00mm
PinHeader_1x25_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x25, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x25 2.00mm single row style1 pin1 left
0
25
25
Connector_PinHeader_2.00mm
PinHeader_1x25_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x25, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x25 2.00mm single row style2 pin1 right
0
25
25
Connector_PinHeader_2.00mm
PinHeader_1x26_P2.00mm_Horizontal
Through hole angled pin header, 1x26, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x26 2.00mm single row
0
26
26
Connector_PinHeader_2.00mm
PinHeader_1x26_P2.00mm_Vertical
Through hole straight pin header, 1x26, 2.00mm pitch, single row
Through hole pin header THT 1x26 2.00mm single row
0
26
26
Connector_PinHeader_2.00mm
PinHeader_1x26_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x26, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x26 2.00mm single row style1 pin1 left
0
26
26
Connector_PinHeader_2.00mm
PinHeader_1x26_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x26, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x26 2.00mm single row style2 pin1 right
0
26
26
Connector_PinHeader_2.00mm
PinHeader_1x27_P2.00mm_Horizontal
Through hole angled pin header, 1x27, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x27 2.00mm single row
0
27
27
Connector_PinHeader_2.00mm
PinHeader_1x27_P2.00mm_Vertical
Through hole straight pin header, 1x27, 2.00mm pitch, single row
Through hole pin header THT 1x27 2.00mm single row
0
27
27
Connector_PinHeader_2.00mm
PinHeader_1x27_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x27, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x27 2.00mm single row style1 pin1 left
0
27
27
Connector_PinHeader_2.00mm
PinHeader_1x27_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x27, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x27 2.00mm single row style2 pin1 right
0
27
27
Connector_PinHeader_2.00mm
PinHeader_1x28_P2.00mm_Horizontal
Through hole angled pin header, 1x28, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x28 2.00mm single row
0
28
28
Connector_PinHeader_2.00mm
PinHeader_1x28_P2.00mm_Vertical
Through hole straight pin header, 1x28, 2.00mm pitch, single row
Through hole pin header THT 1x28 2.00mm single row
0
28
28
Connector_PinHeader_2.00mm
PinHeader_1x28_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x28, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x28 2.00mm single row style1 pin1 left
0
28
28
Connector_PinHeader_2.00mm
PinHeader_1x28_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x28, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x28 2.00mm single row style2 pin1 right
0
28
28
Connector_PinHeader_2.00mm
PinHeader_1x29_P2.00mm_Horizontal
Through hole angled pin header, 1x29, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x29 2.00mm single row
0
29
29
Connector_PinHeader_2.00mm
PinHeader_1x29_P2.00mm_Vertical
Through hole straight pin header, 1x29, 2.00mm pitch, single row
Through hole pin header THT 1x29 2.00mm single row
0
29
29
Connector_PinHeader_2.00mm
PinHeader_1x29_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x29, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x29 2.00mm single row style1 pin1 left
0
29
29
Connector_PinHeader_2.00mm
PinHeader_1x29_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x29, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x29 2.00mm single row style2 pin1 right
0
29
29
Connector_PinHeader_2.00mm
PinHeader_1x30_P2.00mm_Horizontal
Through hole angled pin header, 1x30, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x30 2.00mm single row
0
30
30
Connector_PinHeader_2.00mm
PinHeader_1x30_P2.00mm_Vertical
Through hole straight pin header, 1x30, 2.00mm pitch, single row
Through hole pin header THT 1x30 2.00mm single row
0
30
30
Connector_PinHeader_2.00mm
PinHeader_1x30_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x30, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x30 2.00mm single row style1 pin1 left
0
30
30
Connector_PinHeader_2.00mm
PinHeader_1x30_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x30, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x30 2.00mm single row style2 pin1 right
0
30
30
Connector_PinHeader_2.00mm
PinHeader_1x31_P2.00mm_Horizontal
Through hole angled pin header, 1x31, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x31 2.00mm single row
0
31
31
Connector_PinHeader_2.00mm
PinHeader_1x31_P2.00mm_Vertical
Through hole straight pin header, 1x31, 2.00mm pitch, single row
Through hole pin header THT 1x31 2.00mm single row
0
31
31
Connector_PinHeader_2.00mm
PinHeader_1x31_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x31, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x31 2.00mm single row style1 pin1 left
0
31
31
Connector_PinHeader_2.00mm
PinHeader_1x31_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x31, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x31 2.00mm single row style2 pin1 right
0
31
31
Connector_PinHeader_2.00mm
PinHeader_1x32_P2.00mm_Horizontal
Through hole angled pin header, 1x32, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x32 2.00mm single row
0
32
32
Connector_PinHeader_2.00mm
PinHeader_1x32_P2.00mm_Vertical
Through hole straight pin header, 1x32, 2.00mm pitch, single row
Through hole pin header THT 1x32 2.00mm single row
0
32
32
Connector_PinHeader_2.00mm
PinHeader_1x32_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x32, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x32 2.00mm single row style1 pin1 left
0
32
32
Connector_PinHeader_2.00mm
PinHeader_1x32_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x32, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x32 2.00mm single row style2 pin1 right
0
32
32
Connector_PinHeader_2.00mm
PinHeader_1x33_P2.00mm_Horizontal
Through hole angled pin header, 1x33, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x33 2.00mm single row
0
33
33
Connector_PinHeader_2.00mm
PinHeader_1x33_P2.00mm_Vertical
Through hole straight pin header, 1x33, 2.00mm pitch, single row
Through hole pin header THT 1x33 2.00mm single row
0
33
33
Connector_PinHeader_2.00mm
PinHeader_1x33_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x33, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x33 2.00mm single row style1 pin1 left
0
33
33
Connector_PinHeader_2.00mm
PinHeader_1x33_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x33, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x33 2.00mm single row style2 pin1 right
0
33
33
Connector_PinHeader_2.00mm
PinHeader_1x34_P2.00mm_Horizontal
Through hole angled pin header, 1x34, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x34 2.00mm single row
0
34
34
Connector_PinHeader_2.00mm
PinHeader_1x34_P2.00mm_Vertical
Through hole straight pin header, 1x34, 2.00mm pitch, single row
Through hole pin header THT 1x34 2.00mm single row
0
34
34
Connector_PinHeader_2.00mm
PinHeader_1x34_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x34, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x34 2.00mm single row style1 pin1 left
0
34
34
Connector_PinHeader_2.00mm
PinHeader_1x34_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x34, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x34 2.00mm single row style2 pin1 right
0
34
34
Connector_PinHeader_2.00mm
PinHeader_1x35_P2.00mm_Horizontal
Through hole angled pin header, 1x35, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x35 2.00mm single row
0
35
35
Connector_PinHeader_2.00mm
PinHeader_1x35_P2.00mm_Vertical
Through hole straight pin header, 1x35, 2.00mm pitch, single row
Through hole pin header THT 1x35 2.00mm single row
0
35
35
Connector_PinHeader_2.00mm
PinHeader_1x35_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x35, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x35 2.00mm single row style1 pin1 left
0
35
35
Connector_PinHeader_2.00mm
PinHeader_1x35_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x35, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x35 2.00mm single row style2 pin1 right
0
35
35
Connector_PinHeader_2.00mm
PinHeader_1x36_P2.00mm_Horizontal
Through hole angled pin header, 1x36, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x36 2.00mm single row
0
36
36
Connector_PinHeader_2.00mm
PinHeader_1x36_P2.00mm_Vertical
Through hole straight pin header, 1x36, 2.00mm pitch, single row
Through hole pin header THT 1x36 2.00mm single row
0
36
36
Connector_PinHeader_2.00mm
PinHeader_1x36_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x36, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x36 2.00mm single row style1 pin1 left
0
36
36
Connector_PinHeader_2.00mm
PinHeader_1x36_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x36, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x36 2.00mm single row style2 pin1 right
0
36
36
Connector_PinHeader_2.00mm
PinHeader_1x37_P2.00mm_Horizontal
Through hole angled pin header, 1x37, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x37 2.00mm single row
0
37
37
Connector_PinHeader_2.00mm
PinHeader_1x37_P2.00mm_Vertical
Through hole straight pin header, 1x37, 2.00mm pitch, single row
Through hole pin header THT 1x37 2.00mm single row
0
37
37
Connector_PinHeader_2.00mm
PinHeader_1x37_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x37, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x37 2.00mm single row style1 pin1 left
0
37
37
Connector_PinHeader_2.00mm
PinHeader_1x37_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x37, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x37 2.00mm single row style2 pin1 right
0
37
37
Connector_PinHeader_2.00mm
PinHeader_1x38_P2.00mm_Horizontal
Through hole angled pin header, 1x38, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x38 2.00mm single row
0
38
38
Connector_PinHeader_2.00mm
PinHeader_1x38_P2.00mm_Vertical
Through hole straight pin header, 1x38, 2.00mm pitch, single row
Through hole pin header THT 1x38 2.00mm single row
0
38
38
Connector_PinHeader_2.00mm
PinHeader_1x38_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x38, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x38 2.00mm single row style1 pin1 left
0
38
38
Connector_PinHeader_2.00mm
PinHeader_1x38_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x38, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x38 2.00mm single row style2 pin1 right
0
38
38
Connector_PinHeader_2.00mm
PinHeader_1x39_P2.00mm_Horizontal
Through hole angled pin header, 1x39, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x39 2.00mm single row
0
39
39
Connector_PinHeader_2.00mm
PinHeader_1x39_P2.00mm_Vertical
Through hole straight pin header, 1x39, 2.00mm pitch, single row
Through hole pin header THT 1x39 2.00mm single row
0
39
39
Connector_PinHeader_2.00mm
PinHeader_1x39_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x39, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x39 2.00mm single row style1 pin1 left
0
39
39
Connector_PinHeader_2.00mm
PinHeader_1x39_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x39, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x39 2.00mm single row style2 pin1 right
0
39
39
Connector_PinHeader_2.00mm
PinHeader_1x40_P2.00mm_Horizontal
Through hole angled pin header, 1x40, 2.00mm pitch, 4.2mm pin length, single row
Through hole angled pin header THT 1x40 2.00mm single row
0
40
40
Connector_PinHeader_2.00mm
PinHeader_1x40_P2.00mm_Vertical
Through hole straight pin header, 1x40, 2.00mm pitch, single row
Through hole pin header THT 1x40 2.00mm single row
0
40
40
Connector_PinHeader_2.00mm
PinHeader_1x40_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x40, 2.00mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x40 2.00mm single row style1 pin1 left
0
40
40
Connector_PinHeader_2.00mm
PinHeader_1x40_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x40, 2.00mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x40 2.00mm single row style2 pin1 right
0
40
40
Connector_PinHeader_2.00mm
PinHeader_2x01_P2.00mm_Horizontal
Through hole angled pin header, 2x01, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x01 2.00mm double row
0
2
2
Connector_PinHeader_2.00mm
PinHeader_2x01_P2.00mm_Vertical
Through hole straight pin header, 2x01, 2.00mm pitch, double rows
Through hole pin header THT 2x01 2.00mm double row
0
2
2
Connector_PinHeader_2.00mm
PinHeader_2x01_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x01, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x01 2.00mm double row
0
2
2
Connector_PinHeader_2.00mm
PinHeader_2x02_P2.00mm_Horizontal
Through hole angled pin header, 2x02, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x02 2.00mm double row
0
4
4
Connector_PinHeader_2.00mm
PinHeader_2x02_P2.00mm_Vertical
Through hole straight pin header, 2x02, 2.00mm pitch, double rows
Through hole pin header THT 2x02 2.00mm double row
0
4
4
Connector_PinHeader_2.00mm
PinHeader_2x02_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x02, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x02 2.00mm double row
0
4
4
Connector_PinHeader_2.00mm
PinHeader_2x03_P2.00mm_Horizontal
Through hole angled pin header, 2x03, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x03 2.00mm double row
0
6
6
Connector_PinHeader_2.00mm
PinHeader_2x03_P2.00mm_Vertical
Through hole straight pin header, 2x03, 2.00mm pitch, double rows
Through hole pin header THT 2x03 2.00mm double row
0
6
6
Connector_PinHeader_2.00mm
PinHeader_2x03_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x03, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x03 2.00mm double row
0
6
6
Connector_PinHeader_2.00mm
PinHeader_2x04_P2.00mm_Horizontal
Through hole angled pin header, 2x04, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x04 2.00mm double row
0
8
8
Connector_PinHeader_2.00mm
PinHeader_2x04_P2.00mm_Vertical
Through hole straight pin header, 2x04, 2.00mm pitch, double rows
Through hole pin header THT 2x04 2.00mm double row
0
8
8
Connector_PinHeader_2.00mm
PinHeader_2x04_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x04 2.00mm double row
0
8
8
Connector_PinHeader_2.00mm
PinHeader_2x05_P2.00mm_Horizontal
Through hole angled pin header, 2x05, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x05 2.00mm double row
0
10
10
Connector_PinHeader_2.00mm
PinHeader_2x05_P2.00mm_Vertical
Through hole straight pin header, 2x05, 2.00mm pitch, double rows
Through hole pin header THT 2x05 2.00mm double row
0
10
10
Connector_PinHeader_2.00mm
PinHeader_2x05_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x05, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x05 2.00mm double row
0
10
10
Connector_PinHeader_2.00mm
PinHeader_2x06_P2.00mm_Horizontal
Through hole angled pin header, 2x06, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x06 2.00mm double row
0
12
12
Connector_PinHeader_2.00mm
PinHeader_2x06_P2.00mm_Vertical
Through hole straight pin header, 2x06, 2.00mm pitch, double rows
Through hole pin header THT 2x06 2.00mm double row
0
12
12
Connector_PinHeader_2.00mm
PinHeader_2x06_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x06, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x06 2.00mm double row
0
12
12
Connector_PinHeader_2.00mm
PinHeader_2x07_P2.00mm_Horizontal
Through hole angled pin header, 2x07, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x07 2.00mm double row
0
14
14
Connector_PinHeader_2.00mm
PinHeader_2x07_P2.00mm_Vertical
Through hole straight pin header, 2x07, 2.00mm pitch, double rows
Through hole pin header THT 2x07 2.00mm double row
0
14
14
Connector_PinHeader_2.00mm
PinHeader_2x07_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x07 2.00mm double row
0
14
14
Connector_PinHeader_2.00mm
PinHeader_2x08_P2.00mm_Horizontal
Through hole angled pin header, 2x08, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x08 2.00mm double row
0
16
16
Connector_PinHeader_2.00mm
PinHeader_2x08_P2.00mm_Vertical
Through hole straight pin header, 2x08, 2.00mm pitch, double rows
Through hole pin header THT 2x08 2.00mm double row
0
16
16
Connector_PinHeader_2.00mm
PinHeader_2x08_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x08, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x08 2.00mm double row
0
16
16
Connector_PinHeader_2.00mm
PinHeader_2x09_P2.00mm_Horizontal
Through hole angled pin header, 2x09, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x09 2.00mm double row
0
18
18
Connector_PinHeader_2.00mm
PinHeader_2x09_P2.00mm_Vertical
Through hole straight pin header, 2x09, 2.00mm pitch, double rows
Through hole pin header THT 2x09 2.00mm double row
0
18
18
Connector_PinHeader_2.00mm
PinHeader_2x09_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x09, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x09 2.00mm double row
0
18
18
Connector_PinHeader_2.00mm
PinHeader_2x10_P2.00mm_Horizontal
Through hole angled pin header, 2x10, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x10 2.00mm double row
0
20
20
Connector_PinHeader_2.00mm
PinHeader_2x10_P2.00mm_Vertical
Through hole straight pin header, 2x10, 2.00mm pitch, double rows
Through hole pin header THT 2x10 2.00mm double row
0
20
20
Connector_PinHeader_2.00mm
PinHeader_2x10_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x10, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x10 2.00mm double row
0
20
20
Connector_PinHeader_2.00mm
PinHeader_2x11_P2.00mm_Horizontal
Through hole angled pin header, 2x11, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x11 2.00mm double row
0
22
22
Connector_PinHeader_2.00mm
PinHeader_2x11_P2.00mm_Vertical
Through hole straight pin header, 2x11, 2.00mm pitch, double rows
Through hole pin header THT 2x11 2.00mm double row
0
22
22
Connector_PinHeader_2.00mm
PinHeader_2x11_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x11, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x11 2.00mm double row
0
22
22
Connector_PinHeader_2.00mm
PinHeader_2x12_P2.00mm_Horizontal
Through hole angled pin header, 2x12, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x12 2.00mm double row
0
24
24
Connector_PinHeader_2.00mm
PinHeader_2x12_P2.00mm_Vertical
Through hole straight pin header, 2x12, 2.00mm pitch, double rows
Through hole pin header THT 2x12 2.00mm double row
0
24
24
Connector_PinHeader_2.00mm
PinHeader_2x12_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x12, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x12 2.00mm double row
0
24
24
Connector_PinHeader_2.00mm
PinHeader_2x13_P2.00mm_Horizontal
Through hole angled pin header, 2x13, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x13 2.00mm double row
0
26
26
Connector_PinHeader_2.00mm
PinHeader_2x13_P2.00mm_Vertical
Through hole straight pin header, 2x13, 2.00mm pitch, double rows
Through hole pin header THT 2x13 2.00mm double row
0
26
26
Connector_PinHeader_2.00mm
PinHeader_2x13_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x13, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x13 2.00mm double row
0
26
26
Connector_PinHeader_2.00mm
PinHeader_2x14_P2.00mm_Horizontal
Through hole angled pin header, 2x14, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x14 2.00mm double row
0
28
28
Connector_PinHeader_2.00mm
PinHeader_2x14_P2.00mm_Vertical
Through hole straight pin header, 2x14, 2.00mm pitch, double rows
Through hole pin header THT 2x14 2.00mm double row
0
28
28
Connector_PinHeader_2.00mm
PinHeader_2x14_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x14, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x14 2.00mm double row
0
28
28
Connector_PinHeader_2.00mm
PinHeader_2x15_P2.00mm_Horizontal
Through hole angled pin header, 2x15, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x15 2.00mm double row
0
30
30
Connector_PinHeader_2.00mm
PinHeader_2x15_P2.00mm_Vertical
Through hole straight pin header, 2x15, 2.00mm pitch, double rows
Through hole pin header THT 2x15 2.00mm double row
0
30
30
Connector_PinHeader_2.00mm
PinHeader_2x15_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x15, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x15 2.00mm double row
0
30
30
Connector_PinHeader_2.00mm
PinHeader_2x16_P2.00mm_Horizontal
Through hole angled pin header, 2x16, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x16 2.00mm double row
0
32
32
Connector_PinHeader_2.00mm
PinHeader_2x16_P2.00mm_Vertical
Through hole straight pin header, 2x16, 2.00mm pitch, double rows
Through hole pin header THT 2x16 2.00mm double row
0
32
32
Connector_PinHeader_2.00mm
PinHeader_2x16_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x16, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x16 2.00mm double row
0
32
32
Connector_PinHeader_2.00mm
PinHeader_2x17_P2.00mm_Horizontal
Through hole angled pin header, 2x17, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x17 2.00mm double row
0
34
34
Connector_PinHeader_2.00mm
PinHeader_2x17_P2.00mm_Vertical
Through hole straight pin header, 2x17, 2.00mm pitch, double rows
Through hole pin header THT 2x17 2.00mm double row
0
34
34
Connector_PinHeader_2.00mm
PinHeader_2x17_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x17, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x17 2.00mm double row
0
34
34
Connector_PinHeader_2.00mm
PinHeader_2x18_P2.00mm_Horizontal
Through hole angled pin header, 2x18, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x18 2.00mm double row
0
36
36
Connector_PinHeader_2.00mm
PinHeader_2x18_P2.00mm_Vertical
Through hole straight pin header, 2x18, 2.00mm pitch, double rows
Through hole pin header THT 2x18 2.00mm double row
0
36
36
Connector_PinHeader_2.00mm
PinHeader_2x18_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x18, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x18 2.00mm double row
0
36
36
Connector_PinHeader_2.00mm
PinHeader_2x19_P2.00mm_Horizontal
Through hole angled pin header, 2x19, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x19 2.00mm double row
0
38
38
Connector_PinHeader_2.00mm
PinHeader_2x19_P2.00mm_Vertical
Through hole straight pin header, 2x19, 2.00mm pitch, double rows
Through hole pin header THT 2x19 2.00mm double row
0
38
38
Connector_PinHeader_2.00mm
PinHeader_2x19_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x19, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x19 2.00mm double row
0
38
38
Connector_PinHeader_2.00mm
PinHeader_2x20_P2.00mm_Horizontal
Through hole angled pin header, 2x20, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x20 2.00mm double row
0
40
40
Connector_PinHeader_2.00mm
PinHeader_2x20_P2.00mm_Vertical
Through hole straight pin header, 2x20, 2.00mm pitch, double rows
Through hole pin header THT 2x20 2.00mm double row
0
40
40
Connector_PinHeader_2.00mm
PinHeader_2x20_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x20, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x20 2.00mm double row
0
40
40
Connector_PinHeader_2.00mm
PinHeader_2x21_P2.00mm_Horizontal
Through hole angled pin header, 2x21, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x21 2.00mm double row
0
42
42
Connector_PinHeader_2.00mm
PinHeader_2x21_P2.00mm_Vertical
Through hole straight pin header, 2x21, 2.00mm pitch, double rows
Through hole pin header THT 2x21 2.00mm double row
0
42
42
Connector_PinHeader_2.00mm
PinHeader_2x21_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x21, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x21 2.00mm double row
0
42
42
Connector_PinHeader_2.00mm
PinHeader_2x22_P2.00mm_Horizontal
Through hole angled pin header, 2x22, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x22 2.00mm double row
0
44
44
Connector_PinHeader_2.00mm
PinHeader_2x22_P2.00mm_Vertical
Through hole straight pin header, 2x22, 2.00mm pitch, double rows
Through hole pin header THT 2x22 2.00mm double row
0
44
44
Connector_PinHeader_2.00mm
PinHeader_2x22_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x22, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x22 2.00mm double row
0
44
44
Connector_PinHeader_2.00mm
PinHeader_2x23_P2.00mm_Horizontal
Through hole angled pin header, 2x23, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x23 2.00mm double row
0
46
46
Connector_PinHeader_2.00mm
PinHeader_2x23_P2.00mm_Vertical
Through hole straight pin header, 2x23, 2.00mm pitch, double rows
Through hole pin header THT 2x23 2.00mm double row
0
46
46
Connector_PinHeader_2.00mm
PinHeader_2x23_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x23, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x23 2.00mm double row
0
46
46
Connector_PinHeader_2.00mm
PinHeader_2x24_P2.00mm_Horizontal
Through hole angled pin header, 2x24, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x24 2.00mm double row
0
48
48
Connector_PinHeader_2.00mm
PinHeader_2x24_P2.00mm_Vertical
Through hole straight pin header, 2x24, 2.00mm pitch, double rows
Through hole pin header THT 2x24 2.00mm double row
0
48
48
Connector_PinHeader_2.00mm
PinHeader_2x24_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x24, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x24 2.00mm double row
0
48
48
Connector_PinHeader_2.00mm
PinHeader_2x25_P2.00mm_Horizontal
Through hole angled pin header, 2x25, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x25 2.00mm double row
0
50
50
Connector_PinHeader_2.00mm
PinHeader_2x25_P2.00mm_Vertical
Through hole straight pin header, 2x25, 2.00mm pitch, double rows
Through hole pin header THT 2x25 2.00mm double row
0
50
50
Connector_PinHeader_2.00mm
PinHeader_2x25_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x25, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x25 2.00mm double row
0
50
50
Connector_PinHeader_2.00mm
PinHeader_2x26_P2.00mm_Horizontal
Through hole angled pin header, 2x26, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x26 2.00mm double row
0
52
52
Connector_PinHeader_2.00mm
PinHeader_2x26_P2.00mm_Vertical
Through hole straight pin header, 2x26, 2.00mm pitch, double rows
Through hole pin header THT 2x26 2.00mm double row
0
52
52
Connector_PinHeader_2.00mm
PinHeader_2x26_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x26, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x26 2.00mm double row
0
52
52
Connector_PinHeader_2.00mm
PinHeader_2x27_P2.00mm_Horizontal
Through hole angled pin header, 2x27, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x27 2.00mm double row
0
54
54
Connector_PinHeader_2.00mm
PinHeader_2x27_P2.00mm_Vertical
Through hole straight pin header, 2x27, 2.00mm pitch, double rows
Through hole pin header THT 2x27 2.00mm double row
0
54
54
Connector_PinHeader_2.00mm
PinHeader_2x27_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x27, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x27 2.00mm double row
0
54
54
Connector_PinHeader_2.00mm
PinHeader_2x28_P2.00mm_Horizontal
Through hole angled pin header, 2x28, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x28 2.00mm double row
0
56
56
Connector_PinHeader_2.00mm
PinHeader_2x28_P2.00mm_Vertical
Through hole straight pin header, 2x28, 2.00mm pitch, double rows
Through hole pin header THT 2x28 2.00mm double row
0
56
56
Connector_PinHeader_2.00mm
PinHeader_2x28_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x28, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x28 2.00mm double row
0
56
56
Connector_PinHeader_2.00mm
PinHeader_2x29_P2.00mm_Horizontal
Through hole angled pin header, 2x29, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x29 2.00mm double row
0
58
58
Connector_PinHeader_2.00mm
PinHeader_2x29_P2.00mm_Vertical
Through hole straight pin header, 2x29, 2.00mm pitch, double rows
Through hole pin header THT 2x29 2.00mm double row
0
58
58
Connector_PinHeader_2.00mm
PinHeader_2x29_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x29, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x29 2.00mm double row
0
58
58
Connector_PinHeader_2.00mm
PinHeader_2x30_P2.00mm_Horizontal
Through hole angled pin header, 2x30, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x30 2.00mm double row
0
60
60
Connector_PinHeader_2.00mm
PinHeader_2x30_P2.00mm_Vertical
Through hole straight pin header, 2x30, 2.00mm pitch, double rows
Through hole pin header THT 2x30 2.00mm double row
0
60
60
Connector_PinHeader_2.00mm
PinHeader_2x30_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x30, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x30 2.00mm double row
0
60
60
Connector_PinHeader_2.00mm
PinHeader_2x31_P2.00mm_Horizontal
Through hole angled pin header, 2x31, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x31 2.00mm double row
0
62
62
Connector_PinHeader_2.00mm
PinHeader_2x31_P2.00mm_Vertical
Through hole straight pin header, 2x31, 2.00mm pitch, double rows
Through hole pin header THT 2x31 2.00mm double row
0
62
62
Connector_PinHeader_2.00mm
PinHeader_2x31_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x31, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x31 2.00mm double row
0
62
62
Connector_PinHeader_2.00mm
PinHeader_2x32_P2.00mm_Horizontal
Through hole angled pin header, 2x32, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x32 2.00mm double row
0
64
64
Connector_PinHeader_2.00mm
PinHeader_2x32_P2.00mm_Vertical
Through hole straight pin header, 2x32, 2.00mm pitch, double rows
Through hole pin header THT 2x32 2.00mm double row
0
64
64
Connector_PinHeader_2.00mm
PinHeader_2x32_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x32, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x32 2.00mm double row
0
64
64
Connector_PinHeader_2.00mm
PinHeader_2x33_P2.00mm_Horizontal
Through hole angled pin header, 2x33, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x33 2.00mm double row
0
66
66
Connector_PinHeader_2.00mm
PinHeader_2x33_P2.00mm_Vertical
Through hole straight pin header, 2x33, 2.00mm pitch, double rows
Through hole pin header THT 2x33 2.00mm double row
0
66
66
Connector_PinHeader_2.00mm
PinHeader_2x33_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x33, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x33 2.00mm double row
0
66
66
Connector_PinHeader_2.00mm
PinHeader_2x34_P2.00mm_Horizontal
Through hole angled pin header, 2x34, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x34 2.00mm double row
0
68
68
Connector_PinHeader_2.00mm
PinHeader_2x34_P2.00mm_Vertical
Through hole straight pin header, 2x34, 2.00mm pitch, double rows
Through hole pin header THT 2x34 2.00mm double row
0
68
68
Connector_PinHeader_2.00mm
PinHeader_2x34_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x34, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x34 2.00mm double row
0
68
68
Connector_PinHeader_2.00mm
PinHeader_2x35_P2.00mm_Horizontal
Through hole angled pin header, 2x35, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x35 2.00mm double row
0
70
70
Connector_PinHeader_2.00mm
PinHeader_2x35_P2.00mm_Vertical
Through hole straight pin header, 2x35, 2.00mm pitch, double rows
Through hole pin header THT 2x35 2.00mm double row
0
70
70
Connector_PinHeader_2.00mm
PinHeader_2x35_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x35, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x35 2.00mm double row
0
70
70
Connector_PinHeader_2.00mm
PinHeader_2x36_P2.00mm_Horizontal
Through hole angled pin header, 2x36, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x36 2.00mm double row
0
72
72
Connector_PinHeader_2.00mm
PinHeader_2x36_P2.00mm_Vertical
Through hole straight pin header, 2x36, 2.00mm pitch, double rows
Through hole pin header THT 2x36 2.00mm double row
0
72
72
Connector_PinHeader_2.00mm
PinHeader_2x36_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x36, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x36 2.00mm double row
0
72
72
Connector_PinHeader_2.00mm
PinHeader_2x37_P2.00mm_Horizontal
Through hole angled pin header, 2x37, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x37 2.00mm double row
0
74
74
Connector_PinHeader_2.00mm
PinHeader_2x37_P2.00mm_Vertical
Through hole straight pin header, 2x37, 2.00mm pitch, double rows
Through hole pin header THT 2x37 2.00mm double row
0
74
74
Connector_PinHeader_2.00mm
PinHeader_2x37_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x37, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x37 2.00mm double row
0
74
74
Connector_PinHeader_2.00mm
PinHeader_2x38_P2.00mm_Horizontal
Through hole angled pin header, 2x38, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x38 2.00mm double row
0
76
76
Connector_PinHeader_2.00mm
PinHeader_2x38_P2.00mm_Vertical
Through hole straight pin header, 2x38, 2.00mm pitch, double rows
Through hole pin header THT 2x38 2.00mm double row
0
76
76
Connector_PinHeader_2.00mm
PinHeader_2x38_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x38, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x38 2.00mm double row
0
76
76
Connector_PinHeader_2.00mm
PinHeader_2x39_P2.00mm_Horizontal
Through hole angled pin header, 2x39, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x39 2.00mm double row
0
78
78
Connector_PinHeader_2.00mm
PinHeader_2x39_P2.00mm_Vertical
Through hole straight pin header, 2x39, 2.00mm pitch, double rows
Through hole pin header THT 2x39 2.00mm double row
0
78
78
Connector_PinHeader_2.00mm
PinHeader_2x39_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x39, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x39 2.00mm double row
0
78
78
Connector_PinHeader_2.00mm
PinHeader_2x40_P2.00mm_Horizontal
Through hole angled pin header, 2x40, 2.00mm pitch, 4.2mm pin length, double rows
Through hole angled pin header THT 2x40 2.00mm double row
0
80
80
Connector_PinHeader_2.00mm
PinHeader_2x40_P2.00mm_Vertical
Through hole straight pin header, 2x40, 2.00mm pitch, double rows
Through hole pin header THT 2x40 2.00mm double row
0
80
80
Connector_PinHeader_2.00mm
PinHeader_2x40_P2.00mm_Vertical_SMD
surface-mounted straight pin header, 2x40, 2.00mm pitch, double rows
Surface mounted pin header SMD 2x40 2.00mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_1x01_P2.54mm_Horizontal
Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x01 2.54mm single row
0
1
1
Connector_PinHeader_2.54mm
PinHeader_1x01_P2.54mm_Vertical
Through hole straight pin header, 1x01, 2.54mm pitch, single row
Through hole pin header THT 1x01 2.54mm single row
0
1
1
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Horizontal
Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x02 2.54mm single row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x02 2.54mm single row style1 pin1 left
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x02_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x02 2.54mm single row style2 pin1 right
0
2
2
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Horizontal
Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x03 2.54mm single row
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical
Through hole straight pin header, 1x03, 2.54mm pitch, single row
Through hole pin header THT 1x03 2.54mm single row
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x03 2.54mm single row style1 pin1 left
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x03 2.54mm single row style2 pin1 right
0
3
3
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Horizontal
Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x04 2.54mm single row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical
Through hole straight pin header, 1x04, 2.54mm pitch, single row
Through hole pin header THT 1x04 2.54mm single row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x04 2.54mm single row style1 pin1 left
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right
0
4
4
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Horizontal
Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x05 2.54mm single row
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical
Through hole straight pin header, 1x05, 2.54mm pitch, single row
Through hole pin header THT 1x05 2.54mm single row
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x05 2.54mm single row style2 pin1 right
0
5
5
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Horizontal
Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x06 2.54mm single row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical
Through hole straight pin header, 1x06, 2.54mm pitch, single row
Through hole pin header THT 1x06 2.54mm single row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x06 2.54mm single row style1 pin1 left
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x06_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x06 2.54mm single row style2 pin1 right
0
6
6
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Horizontal
Through hole angled pin header, 1x07, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x07 2.54mm single row
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical
Through hole straight pin header, 1x07, 2.54mm pitch, single row
Through hole pin header THT 1x07 2.54mm single row
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x07, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x07 2.54mm single row style1 pin1 left
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x07_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x07, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x07 2.54mm single row style2 pin1 right
0
7
7
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Horizontal
Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x08 2.54mm single row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical
Through hole straight pin header, 1x08, 2.54mm pitch, single row
Through hole pin header THT 1x08 2.54mm single row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x08 2.54mm single row style1 pin1 left
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x08_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x08 2.54mm single row style2 pin1 right
0
8
8
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Horizontal
Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x09 2.54mm single row
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical
Through hole straight pin header, 1x09, 2.54mm pitch, single row
Through hole pin header THT 1x09 2.54mm single row
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x09, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x09 2.54mm single row style1 pin1 left
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x09_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x09, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x09 2.54mm single row style2 pin1 right
0
9
9
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Horizontal
Through hole angled pin header, 1x10, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x10 2.54mm single row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical
Through hole straight pin header, 1x10, 2.54mm pitch, single row
Through hole pin header THT 1x10 2.54mm single row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x10, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x10 2.54mm single row style1 pin1 left
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x10_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x10, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x10 2.54mm single row style2 pin1 right
0
10
10
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Horizontal
Through hole angled pin header, 1x11, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x11 2.54mm single row
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical
Through hole straight pin header, 1x11, 2.54mm pitch, single row
Through hole pin header THT 1x11 2.54mm single row
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x11, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x11 2.54mm single row style1 pin1 left
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x11_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x11, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x11 2.54mm single row style2 pin1 right
0
11
11
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Horizontal
Through hole angled pin header, 1x12, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x12 2.54mm single row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical
Through hole straight pin header, 1x12, 2.54mm pitch, single row
Through hole pin header THT 1x12 2.54mm single row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x12 2.54mm single row style1 pin1 left
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x12_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x12, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x12 2.54mm single row style2 pin1 right
0
12
12
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Horizontal
Through hole angled pin header, 1x13, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x13 2.54mm single row
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical
Through hole straight pin header, 1x13, 2.54mm pitch, single row
Through hole pin header THT 1x13 2.54mm single row
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x13, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x13 2.54mm single row style1 pin1 left
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x13_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x13, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x13 2.54mm single row style2 pin1 right
0
13
13
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Horizontal
Through hole angled pin header, 1x14, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x14 2.54mm single row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical
Through hole straight pin header, 1x14, 2.54mm pitch, single row
Through hole pin header THT 1x14 2.54mm single row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x14 2.54mm single row style2 pin1 right
0
14
14
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Horizontal
Through hole angled pin header, 1x15, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x15 2.54mm single row
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical
Through hole straight pin header, 1x15, 2.54mm pitch, single row
Through hole pin header THT 1x15 2.54mm single row
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x15, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x15 2.54mm single row style1 pin1 left
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x15_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x15, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x15 2.54mm single row style2 pin1 right
0
15
15
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Horizontal
Through hole angled pin header, 1x16, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x16 2.54mm single row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical
Through hole straight pin header, 1x16, 2.54mm pitch, single row
Through hole pin header THT 1x16 2.54mm single row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x16, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x16 2.54mm single row style1 pin1 left
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x16_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x16, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x16 2.54mm single row style2 pin1 right
0
16
16
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Horizontal
Through hole angled pin header, 1x17, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x17 2.54mm single row
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical
Through hole straight pin header, 1x17, 2.54mm pitch, single row
Through hole pin header THT 1x17 2.54mm single row
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x17, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x17 2.54mm single row style1 pin1 left
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x17_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x17, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x17 2.54mm single row style2 pin1 right
0
17
17
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Horizontal
Through hole angled pin header, 1x18, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x18 2.54mm single row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical
Through hole straight pin header, 1x18, 2.54mm pitch, single row
Through hole pin header THT 1x18 2.54mm single row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x18, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x18 2.54mm single row style1 pin1 left
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x18_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x18, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x18 2.54mm single row style2 pin1 right
0
18
18
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Horizontal
Through hole angled pin header, 1x19, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x19 2.54mm single row
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical
Through hole straight pin header, 1x19, 2.54mm pitch, single row
Through hole pin header THT 1x19 2.54mm single row
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x19, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x19 2.54mm single row style1 pin1 left
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x19_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x19, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x19 2.54mm single row style2 pin1 right
0
19
19
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Horizontal
Through hole angled pin header, 1x20, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x20 2.54mm single row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical
Through hole straight pin header, 1x20, 2.54mm pitch, single row
Through hole pin header THT 1x20 2.54mm single row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x20, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x20 2.54mm single row style1 pin1 left
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x20_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x20, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x20 2.54mm single row style2 pin1 right
0
20
20
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Horizontal
Through hole angled pin header, 1x21, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x21 2.54mm single row
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical
Through hole straight pin header, 1x21, 2.54mm pitch, single row
Through hole pin header THT 1x21 2.54mm single row
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x21, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x21 2.54mm single row style1 pin1 left
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x21_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x21, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x21 2.54mm single row style2 pin1 right
0
21
21
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Horizontal
Through hole angled pin header, 1x22, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x22 2.54mm single row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical
Through hole straight pin header, 1x22, 2.54mm pitch, single row
Through hole pin header THT 1x22 2.54mm single row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x22, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x22 2.54mm single row style1 pin1 left
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x22_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x22, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x22 2.54mm single row style2 pin1 right
0
22
22
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Horizontal
Through hole angled pin header, 1x23, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x23 2.54mm single row
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical
Through hole straight pin header, 1x23, 2.54mm pitch, single row
Through hole pin header THT 1x23 2.54mm single row
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x23, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x23 2.54mm single row style1 pin1 left
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x23_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x23, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x23 2.54mm single row style2 pin1 right
0
23
23
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Horizontal
Through hole angled pin header, 1x24, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x24 2.54mm single row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical
Through hole straight pin header, 1x24, 2.54mm pitch, single row
Through hole pin header THT 1x24 2.54mm single row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x24, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x24 2.54mm single row style1 pin1 left
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x24_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x24, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x24 2.54mm single row style2 pin1 right
0
24
24
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Horizontal
Through hole angled pin header, 1x25, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x25 2.54mm single row
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical
Through hole straight pin header, 1x25, 2.54mm pitch, single row
Through hole pin header THT 1x25 2.54mm single row
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x25, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x25 2.54mm single row style1 pin1 left
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x25_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x25, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x25 2.54mm single row style2 pin1 right
0
25
25
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Horizontal
Through hole angled pin header, 1x26, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x26 2.54mm single row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical
Through hole straight pin header, 1x26, 2.54mm pitch, single row
Through hole pin header THT 1x26 2.54mm single row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x26, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x26 2.54mm single row style1 pin1 left
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x26_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x26, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x26 2.54mm single row style2 pin1 right
0
26
26
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Horizontal
Through hole angled pin header, 1x27, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x27 2.54mm single row
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical
Through hole straight pin header, 1x27, 2.54mm pitch, single row
Through hole pin header THT 1x27 2.54mm single row
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x27, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x27 2.54mm single row style1 pin1 left
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x27_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x27, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x27 2.54mm single row style2 pin1 right
0
27
27
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Horizontal
Through hole angled pin header, 1x28, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x28 2.54mm single row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical
Through hole straight pin header, 1x28, 2.54mm pitch, single row
Through hole pin header THT 1x28 2.54mm single row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x28, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x28 2.54mm single row style1 pin1 left
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x28_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x28, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x28 2.54mm single row style2 pin1 right
0
28
28
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Horizontal
Through hole angled pin header, 1x29, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x29 2.54mm single row
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical
Through hole straight pin header, 1x29, 2.54mm pitch, single row
Through hole pin header THT 1x29 2.54mm single row
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x29, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x29 2.54mm single row style1 pin1 left
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x29_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x29, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x29 2.54mm single row style2 pin1 right
0
29
29
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Horizontal
Through hole angled pin header, 1x30, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x30 2.54mm single row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical
Through hole straight pin header, 1x30, 2.54mm pitch, single row
Through hole pin header THT 1x30 2.54mm single row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x30, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x30 2.54mm single row style1 pin1 left
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x30_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x30, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x30 2.54mm single row style2 pin1 right
0
30
30
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Horizontal
Through hole angled pin header, 1x31, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x31 2.54mm single row
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical
Through hole straight pin header, 1x31, 2.54mm pitch, single row
Through hole pin header THT 1x31 2.54mm single row
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x31, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x31 2.54mm single row style1 pin1 left
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x31_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x31, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x31 2.54mm single row style2 pin1 right
0
31
31
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Horizontal
Through hole angled pin header, 1x32, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x32 2.54mm single row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical
Through hole straight pin header, 1x32, 2.54mm pitch, single row
Through hole pin header THT 1x32 2.54mm single row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x32, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x32 2.54mm single row style1 pin1 left
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x32_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x32, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x32 2.54mm single row style2 pin1 right
0
32
32
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Horizontal
Through hole angled pin header, 1x33, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x33 2.54mm single row
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical
Through hole straight pin header, 1x33, 2.54mm pitch, single row
Through hole pin header THT 1x33 2.54mm single row
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x33, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x33 2.54mm single row style1 pin1 left
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x33_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x33, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x33 2.54mm single row style2 pin1 right
0
33
33
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Horizontal
Through hole angled pin header, 1x34, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x34 2.54mm single row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical
Through hole straight pin header, 1x34, 2.54mm pitch, single row
Through hole pin header THT 1x34 2.54mm single row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x34, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x34 2.54mm single row style1 pin1 left
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x34_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x34, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x34 2.54mm single row style2 pin1 right
0
34
34
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Horizontal
Through hole angled pin header, 1x35, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x35 2.54mm single row
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical
Through hole straight pin header, 1x35, 2.54mm pitch, single row
Through hole pin header THT 1x35 2.54mm single row
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x35, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x35 2.54mm single row style1 pin1 left
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x35_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x35, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x35 2.54mm single row style2 pin1 right
0
35
35
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Horizontal
Through hole angled pin header, 1x36, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x36 2.54mm single row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical
Through hole straight pin header, 1x36, 2.54mm pitch, single row
Through hole pin header THT 1x36 2.54mm single row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x36, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x36 2.54mm single row style1 pin1 left
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x36_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x36, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x36 2.54mm single row style2 pin1 right
0
36
36
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Horizontal
Through hole angled pin header, 1x37, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x37 2.54mm single row
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical
Through hole straight pin header, 1x37, 2.54mm pitch, single row
Through hole pin header THT 1x37 2.54mm single row
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x37, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x37 2.54mm single row style1 pin1 left
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x37_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x37, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x37 2.54mm single row style2 pin1 right
0
37
37
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Horizontal
Through hole angled pin header, 1x38, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x38 2.54mm single row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical
Through hole straight pin header, 1x38, 2.54mm pitch, single row
Through hole pin header THT 1x38 2.54mm single row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x38, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x38 2.54mm single row style1 pin1 left
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x38_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x38, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x38 2.54mm single row style2 pin1 right
0
38
38
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Horizontal
Through hole angled pin header, 1x39, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x39 2.54mm single row
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical
Through hole straight pin header, 1x39, 2.54mm pitch, single row
Through hole pin header THT 1x39 2.54mm single row
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x39, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x39 2.54mm single row style1 pin1 left
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x39_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x39, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x39 2.54mm single row style2 pin1 right
0
39
39
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Horizontal
Through hole angled pin header, 1x40, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x40 2.54mm single row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical
Through hole straight pin header, 1x40, 2.54mm pitch, single row
Through hole pin header THT 1x40 2.54mm single row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight pin header, 1x40, 2.54mm pitch, single row, style 1 (pin 1 left)
Surface mounted pin header SMD 1x40 2.54mm single row style1 pin1 left
0
40
40
Connector_PinHeader_2.54mm
PinHeader_1x40_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight pin header, 1x40, 2.54mm pitch, single row, style 2 (pin 1 right)
Surface mounted pin header SMD 1x40 2.54mm single row style2 pin1 right
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Horizontal
Through hole angled pin header, 2x01, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Vertical
Through hole straight pin header, 2x01, 2.54mm pitch, double rows
Through hole pin header THT 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x01_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x01, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x01 2.54mm double row
0
2
2
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Horizontal
Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Vertical
Through hole straight pin header, 2x02, 2.54mm pitch, double rows
Through hole pin header THT 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x02_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x02 2.54mm double row
0
4
4
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Horizontal
Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Vertical
Through hole straight pin header, 2x03, 2.54mm pitch, double rows
Through hole pin header THT 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x03_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x03 2.54mm double row
0
6
6
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Horizontal
Through hole angled pin header, 2x04, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Vertical
Through hole straight pin header, 2x04, 2.54mm pitch, double rows
Through hole pin header THT 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x04_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x04 2.54mm double row
0
8
8
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Horizontal
Through hole angled pin header, 2x05, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Vertical
Through hole straight pin header, 2x05, 2.54mm pitch, double rows
Through hole pin header THT 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x05_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x05, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x05 2.54mm double row
0
10
10
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Horizontal
Through hole angled pin header, 2x06, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Vertical
Through hole straight pin header, 2x06, 2.54mm pitch, double rows
Through hole pin header THT 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x06_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x06, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x06 2.54mm double row
0
12
12
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Horizontal
Through hole angled pin header, 2x07, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Vertical
Through hole straight pin header, 2x07, 2.54mm pitch, double rows
Through hole pin header THT 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x07_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x07 2.54mm double row
0
14
14
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Horizontal
Through hole angled pin header, 2x08, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Vertical
Through hole straight pin header, 2x08, 2.54mm pitch, double rows
Through hole pin header THT 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x08_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x08, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x08 2.54mm double row
0
16
16
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Horizontal
Through hole angled pin header, 2x09, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Vertical
Through hole straight pin header, 2x09, 2.54mm pitch, double rows
Through hole pin header THT 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x09_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x09, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x09 2.54mm double row
0
18
18
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Horizontal
Through hole angled pin header, 2x10, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Vertical
Through hole straight pin header, 2x10, 2.54mm pitch, double rows
Through hole pin header THT 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x10_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x10, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x10 2.54mm double row
0
20
20
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Horizontal
Through hole angled pin header, 2x11, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Vertical
Through hole straight pin header, 2x11, 2.54mm pitch, double rows
Through hole pin header THT 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x11_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x11, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x11 2.54mm double row
0
22
22
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Horizontal
Through hole angled pin header, 2x12, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Vertical
Through hole straight pin header, 2x12, 2.54mm pitch, double rows
Through hole pin header THT 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x12_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x12, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x12 2.54mm double row
0
24
24
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Horizontal
Through hole angled pin header, 2x13, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Vertical
Through hole straight pin header, 2x13, 2.54mm pitch, double rows
Through hole pin header THT 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x13_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x13, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x13 2.54mm double row
0
26
26
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Horizontal
Through hole angled pin header, 2x14, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Vertical
Through hole straight pin header, 2x14, 2.54mm pitch, double rows
Through hole pin header THT 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x14_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x14, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x14 2.54mm double row
0
28
28
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Horizontal
Through hole angled pin header, 2x15, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Vertical
Through hole straight pin header, 2x15, 2.54mm pitch, double rows
Through hole pin header THT 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x15_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x15, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x15 2.54mm double row
0
30
30
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Horizontal
Through hole angled pin header, 2x16, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Vertical
Through hole straight pin header, 2x16, 2.54mm pitch, double rows
Through hole pin header THT 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x16_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x16, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x16 2.54mm double row
0
32
32
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Horizontal
Through hole angled pin header, 2x17, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Vertical
Through hole straight pin header, 2x17, 2.54mm pitch, double rows
Through hole pin header THT 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x17_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x17, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x17 2.54mm double row
0
34
34
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Horizontal
Through hole angled pin header, 2x18, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Vertical
Through hole straight pin header, 2x18, 2.54mm pitch, double rows
Through hole pin header THT 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x18_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x18, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x18 2.54mm double row
0
36
36
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Horizontal
Through hole angled pin header, 2x19, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Vertical
Through hole straight pin header, 2x19, 2.54mm pitch, double rows
Through hole pin header THT 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x19_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x19, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x19 2.54mm double row
0
38
38
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Horizontal
Through hole angled pin header, 2x20, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Vertical
Through hole straight pin header, 2x20, 2.54mm pitch, double rows
Through hole pin header THT 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x20_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x20, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x20 2.54mm double row
0
40
40
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Horizontal
Through hole angled pin header, 2x21, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Vertical
Through hole straight pin header, 2x21, 2.54mm pitch, double rows
Through hole pin header THT 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x21_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x21, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x21 2.54mm double row
0
42
42
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Horizontal
Through hole angled pin header, 2x22, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Vertical
Through hole straight pin header, 2x22, 2.54mm pitch, double rows
Through hole pin header THT 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x22_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x22, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x22 2.54mm double row
0
44
44
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Horizontal
Through hole angled pin header, 2x23, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Vertical
Through hole straight pin header, 2x23, 2.54mm pitch, double rows
Through hole pin header THT 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x23_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x23, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x23 2.54mm double row
0
46
46
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Horizontal
Through hole angled pin header, 2x24, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Vertical
Through hole straight pin header, 2x24, 2.54mm pitch, double rows
Through hole pin header THT 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x24_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x24, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x24 2.54mm double row
0
48
48
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Horizontal
Through hole angled pin header, 2x25, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Vertical
Through hole straight pin header, 2x25, 2.54mm pitch, double rows
Through hole pin header THT 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x25_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x25, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x25 2.54mm double row
0
50
50
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Horizontal
Through hole angled pin header, 2x26, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Vertical
Through hole straight pin header, 2x26, 2.54mm pitch, double rows
Through hole pin header THT 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x26_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x26, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x26 2.54mm double row
0
52
52
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Horizontal
Through hole angled pin header, 2x27, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Vertical
Through hole straight pin header, 2x27, 2.54mm pitch, double rows
Through hole pin header THT 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x27_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x27, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x27 2.54mm double row
0
54
54
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Horizontal
Through hole angled pin header, 2x28, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Vertical
Through hole straight pin header, 2x28, 2.54mm pitch, double rows
Through hole pin header THT 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x28_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x28, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x28 2.54mm double row
0
56
56
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Horizontal
Through hole angled pin header, 2x29, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Vertical
Through hole straight pin header, 2x29, 2.54mm pitch, double rows
Through hole pin header THT 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x29_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x29, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x29 2.54mm double row
0
58
58
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Horizontal
Through hole angled pin header, 2x30, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Vertical
Through hole straight pin header, 2x30, 2.54mm pitch, double rows
Through hole pin header THT 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x30_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x30, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x30 2.54mm double row
0
60
60
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Horizontal
Through hole angled pin header, 2x31, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Vertical
Through hole straight pin header, 2x31, 2.54mm pitch, double rows
Through hole pin header THT 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x31_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x31, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x31 2.54mm double row
0
62
62
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Horizontal
Through hole angled pin header, 2x32, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Vertical
Through hole straight pin header, 2x32, 2.54mm pitch, double rows
Through hole pin header THT 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x32_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x32, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x32 2.54mm double row
0
64
64
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Horizontal
Through hole angled pin header, 2x33, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Vertical
Through hole straight pin header, 2x33, 2.54mm pitch, double rows
Through hole pin header THT 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x33_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x33, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x33 2.54mm double row
0
66
66
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Horizontal
Through hole angled pin header, 2x34, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Vertical
Through hole straight pin header, 2x34, 2.54mm pitch, double rows
Through hole pin header THT 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x34_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x34, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x34 2.54mm double row
0
68
68
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Horizontal
Through hole angled pin header, 2x35, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Vertical
Through hole straight pin header, 2x35, 2.54mm pitch, double rows
Through hole pin header THT 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x35_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x35, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x35 2.54mm double row
0
70
70
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Horizontal
Through hole angled pin header, 2x36, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Vertical
Through hole straight pin header, 2x36, 2.54mm pitch, double rows
Through hole pin header THT 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x36_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x36, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x36 2.54mm double row
0
72
72
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Horizontal
Through hole angled pin header, 2x37, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Vertical
Through hole straight pin header, 2x37, 2.54mm pitch, double rows
Through hole pin header THT 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x37_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x37, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x37 2.54mm double row
0
74
74
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Horizontal
Through hole angled pin header, 2x38, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Vertical
Through hole straight pin header, 2x38, 2.54mm pitch, double rows
Through hole pin header THT 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x38_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x38, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x38 2.54mm double row
0
76
76
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Horizontal
Through hole angled pin header, 2x39, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Vertical
Through hole straight pin header, 2x39, 2.54mm pitch, double rows
Through hole pin header THT 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x39_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x39, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x39 2.54mm double row
0
78
78
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Horizontal
Through hole angled pin header, 2x40, 2.54mm pitch, 6mm pin length, double rows
Through hole angled pin header THT 2x40 2.54mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Vertical
Through hole straight pin header, 2x40, 2.54mm pitch, double rows
Through hole pin header THT 2x40 2.54mm double row
0
80
80
Connector_PinHeader_2.54mm
PinHeader_2x40_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x40, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x40 2.54mm double row
0
80
80
Connector_PinSocket_2.00mm
PinSocket_1x01_P2.00mm_Horizontal
Through hole angled socket strip, 1x01, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x01 2.00mm single row
0
1
1
Connector_PinSocket_2.00mm
PinSocket_1x01_P2.00mm_Vertical
Through hole straight socket strip, 1x01, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x01 2.00mm single row
0
1
1
Connector_PinSocket_2.00mm
PinSocket_1x02_P2.00mm_Horizontal
Through hole angled socket strip, 1x02, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x02 2.00mm single row
0
2
2
Connector_PinSocket_2.00mm
PinSocket_1x02_P2.00mm_Vertical
Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x02 2.00mm single row
0
2
2
Connector_PinSocket_2.00mm
PinSocket_1x02_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x02, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x02 2.00mm single row style1 pin1 left
0
2
2
Connector_PinSocket_2.00mm
PinSocket_1x02_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x02, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x02 2.00mm single row style2 pin1 right
0
2
2
Connector_PinSocket_2.00mm
PinSocket_1x03_P2.00mm_Horizontal
Through hole angled socket strip, 1x03, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x03 2.00mm single row
0
3
3
Connector_PinSocket_2.00mm
PinSocket_1x03_P2.00mm_Vertical
Through hole straight socket strip, 1x03, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x03 2.00mm single row
0
3
3
Connector_PinSocket_2.00mm
PinSocket_1x03_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x03, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x03 2.00mm single row style1 pin1 left
0
3
3
Connector_PinSocket_2.00mm
PinSocket_1x03_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x03, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x03 2.00mm single row style2 pin1 right
0
3
3
Connector_PinSocket_2.00mm
PinSocket_1x04_P2.00mm_Horizontal
Through hole angled socket strip, 1x04, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x04 2.00mm single row
0
4
4
Connector_PinSocket_2.00mm
PinSocket_1x04_P2.00mm_Vertical
Through hole straight socket strip, 1x04, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.00mm single row
0
4
4
Connector_PinSocket_2.00mm
PinSocket_1x04_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x04, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x04 2.00mm single row style1 pin1 left
0
4
4
Connector_PinSocket_2.00mm
PinSocket_1x04_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x04, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x04 2.00mm single row style2 pin1 right
0
4
4
Connector_PinSocket_2.00mm
PinSocket_1x05_P2.00mm_Horizontal
Through hole angled socket strip, 1x05, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x05 2.00mm single row
0
5
5
Connector_PinSocket_2.00mm
PinSocket_1x05_P2.00mm_Vertical
Through hole straight socket strip, 1x05, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x05 2.00mm single row
0
5
5
Connector_PinSocket_2.00mm
PinSocket_1x05_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x05, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x05 2.00mm single row style1 pin1 left
0
5
5
Connector_PinSocket_2.00mm
PinSocket_1x05_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x05, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x05 2.00mm single row style2 pin1 right
0
5
5
Connector_PinSocket_2.00mm
PinSocket_1x06_P2.00mm_Horizontal
Through hole angled socket strip, 1x06, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x06 2.00mm single row
0
6
6
Connector_PinSocket_2.00mm
PinSocket_1x06_P2.00mm_Vertical
Through hole straight socket strip, 1x06, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x06 2.00mm single row
0
6
6
Connector_PinSocket_2.00mm
PinSocket_1x06_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x06, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x06 2.00mm single row style1 pin1 left
0
6
6
Connector_PinSocket_2.00mm
PinSocket_1x06_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x06, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x06 2.00mm single row style2 pin1 right
0
6
6
Connector_PinSocket_2.00mm
PinSocket_1x07_P2.00mm_Horizontal
Through hole angled socket strip, 1x07, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x07 2.00mm single row
0
7
7
Connector_PinSocket_2.00mm
PinSocket_1x07_P2.00mm_Vertical
Through hole straight socket strip, 1x07, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x07 2.00mm single row
0
7
7
Connector_PinSocket_2.00mm
PinSocket_1x07_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x07, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x07 2.00mm single row style1 pin1 left
0
7
7
Connector_PinSocket_2.00mm
PinSocket_1x07_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x07, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x07 2.00mm single row style2 pin1 right
0
7
7
Connector_PinSocket_2.00mm
PinSocket_1x08_P2.00mm_Horizontal
Through hole angled socket strip, 1x08, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x08 2.00mm single row
0
8
8
Connector_PinSocket_2.00mm
PinSocket_1x08_P2.00mm_Vertical
Through hole straight socket strip, 1x08, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x08 2.00mm single row
0
8
8
Connector_PinSocket_2.00mm
PinSocket_1x08_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x08, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x08 2.00mm single row style1 pin1 left
0
8
8
Connector_PinSocket_2.00mm
PinSocket_1x08_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x08, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x08 2.00mm single row style2 pin1 right
0
8
8
Connector_PinSocket_2.00mm
PinSocket_1x09_P2.00mm_Horizontal
Through hole angled socket strip, 1x09, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x09 2.00mm single row
0
9
9
Connector_PinSocket_2.00mm
PinSocket_1x09_P2.00mm_Vertical
Through hole straight socket strip, 1x09, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x09 2.00mm single row
0
9
9
Connector_PinSocket_2.00mm
PinSocket_1x09_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x09, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x09 2.00mm single row style1 pin1 left
0
9
9
Connector_PinSocket_2.00mm
PinSocket_1x09_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x09, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x09 2.00mm single row style2 pin1 right
0
9
9
Connector_PinSocket_2.00mm
PinSocket_1x10_P2.00mm_Horizontal
Through hole angled socket strip, 1x10, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x10 2.00mm single row
0
10
10
Connector_PinSocket_2.00mm
PinSocket_1x10_P2.00mm_Vertical
Through hole straight socket strip, 1x10, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x10 2.00mm single row
0
10
10
Connector_PinSocket_2.00mm
PinSocket_1x10_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x10, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x10 2.00mm single row style1 pin1 left
0
10
10
Connector_PinSocket_2.00mm
PinSocket_1x10_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x10, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x10 2.00mm single row style2 pin1 right
0
10
10
Connector_PinSocket_2.00mm
PinSocket_1x11_P2.00mm_Horizontal
Through hole angled socket strip, 1x11, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x11 2.00mm single row
0
11
11
Connector_PinSocket_2.00mm
PinSocket_1x11_P2.00mm_Vertical
Through hole straight socket strip, 1x11, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x11 2.00mm single row
0
11
11
Connector_PinSocket_2.00mm
PinSocket_1x11_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x11, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x11 2.00mm single row style1 pin1 left
0
11
11
Connector_PinSocket_2.00mm
PinSocket_1x11_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x11, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x11 2.00mm single row style2 pin1 right
0
11
11
Connector_PinSocket_2.00mm
PinSocket_1x12_P2.00mm_Horizontal
Through hole angled socket strip, 1x12, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x12 2.00mm single row
0
12
12
Connector_PinSocket_2.00mm
PinSocket_1x12_P2.00mm_Vertical
Through hole straight socket strip, 1x12, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x12 2.00mm single row
0
12
12
Connector_PinSocket_2.00mm
PinSocket_1x12_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x12, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x12 2.00mm single row style1 pin1 left
0
12
12
Connector_PinSocket_2.00mm
PinSocket_1x12_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x12, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x12 2.00mm single row style2 pin1 right
0
12
12
Connector_PinSocket_2.00mm
PinSocket_1x13_P2.00mm_Horizontal
Through hole angled socket strip, 1x13, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x13 2.00mm single row
0
13
13
Connector_PinSocket_2.00mm
PinSocket_1x13_P2.00mm_Vertical
Through hole straight socket strip, 1x13, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x13 2.00mm single row
0
13
13
Connector_PinSocket_2.00mm
PinSocket_1x13_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x13, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x13 2.00mm single row style1 pin1 left
0
13
13
Connector_PinSocket_2.00mm
PinSocket_1x13_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x13, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x13 2.00mm single row style2 pin1 right
0
13
13
Connector_PinSocket_2.00mm
PinSocket_1x14_P2.00mm_Horizontal
Through hole angled socket strip, 1x14, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x14 2.00mm single row
0
14
14
Connector_PinSocket_2.00mm
PinSocket_1x14_P2.00mm_Vertical
Through hole straight socket strip, 1x14, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x14 2.00mm single row
0
14
14
Connector_PinSocket_2.00mm
PinSocket_1x14_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x14, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x14 2.00mm single row style1 pin1 left
0
14
14
Connector_PinSocket_2.00mm
PinSocket_1x14_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x14, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x14 2.00mm single row style2 pin1 right
0
14
14
Connector_PinSocket_2.00mm
PinSocket_1x15_P2.00mm_Horizontal
Through hole angled socket strip, 1x15, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x15 2.00mm single row
0
15
15
Connector_PinSocket_2.00mm
PinSocket_1x15_P2.00mm_Vertical
Through hole straight socket strip, 1x15, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x15 2.00mm single row
0
15
15
Connector_PinSocket_2.00mm
PinSocket_1x15_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x15, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x15 2.00mm single row style1 pin1 left
0
15
15
Connector_PinSocket_2.00mm
PinSocket_1x15_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x15, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x15 2.00mm single row style2 pin1 right
0
15
15
Connector_PinSocket_2.00mm
PinSocket_1x16_P2.00mm_Horizontal
Through hole angled socket strip, 1x16, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x16 2.00mm single row
0
16
16
Connector_PinSocket_2.00mm
PinSocket_1x16_P2.00mm_Vertical
Through hole straight socket strip, 1x16, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x16 2.00mm single row
0
16
16
Connector_PinSocket_2.00mm
PinSocket_1x16_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x16, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x16 2.00mm single row style1 pin1 left
0
16
16
Connector_PinSocket_2.00mm
PinSocket_1x16_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x16, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x16 2.00mm single row style2 pin1 right
0
16
16
Connector_PinSocket_2.00mm
PinSocket_1x17_P2.00mm_Horizontal
Through hole angled socket strip, 1x17, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x17 2.00mm single row
0
17
17
Connector_PinSocket_2.00mm
PinSocket_1x17_P2.00mm_Vertical
Through hole straight socket strip, 1x17, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x17 2.00mm single row
0
17
17
Connector_PinSocket_2.00mm
PinSocket_1x17_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x17, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x17 2.00mm single row style1 pin1 left
0
17
17
Connector_PinSocket_2.00mm
PinSocket_1x17_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x17, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x17 2.00mm single row style2 pin1 right
0
17
17
Connector_PinSocket_2.00mm
PinSocket_1x18_P2.00mm_Horizontal
Through hole angled socket strip, 1x18, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x18 2.00mm single row
0
18
18
Connector_PinSocket_2.00mm
PinSocket_1x18_P2.00mm_Vertical
Through hole straight socket strip, 1x18, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x18 2.00mm single row
0
18
18
Connector_PinSocket_2.00mm
PinSocket_1x18_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x18, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x18 2.00mm single row style1 pin1 left
0
18
18
Connector_PinSocket_2.00mm
PinSocket_1x18_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x18, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x18 2.00mm single row style2 pin1 right
0
18
18
Connector_PinSocket_2.00mm
PinSocket_1x19_P2.00mm_Horizontal
Through hole angled socket strip, 1x19, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x19 2.00mm single row
0
19
19
Connector_PinSocket_2.00mm
PinSocket_1x19_P2.00mm_Vertical
Through hole straight socket strip, 1x19, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x19 2.00mm single row
0
19
19
Connector_PinSocket_2.00mm
PinSocket_1x19_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x19, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x19 2.00mm single row style1 pin1 left
0
19
19
Connector_PinSocket_2.00mm
PinSocket_1x19_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x19, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x19 2.00mm single row style2 pin1 right
0
19
19
Connector_PinSocket_2.00mm
PinSocket_1x20_P2.00mm_Horizontal
Through hole angled socket strip, 1x20, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x20 2.00mm single row
0
20
20
Connector_PinSocket_2.00mm
PinSocket_1x20_P2.00mm_Vertical
Through hole straight socket strip, 1x20, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x20 2.00mm single row
0
20
20
Connector_PinSocket_2.00mm
PinSocket_1x20_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x20, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x20 2.00mm single row style1 pin1 left
0
20
20
Connector_PinSocket_2.00mm
PinSocket_1x20_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x20, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x20 2.00mm single row style2 pin1 right
0
20
20
Connector_PinSocket_2.00mm
PinSocket_1x21_P2.00mm_Horizontal
Through hole angled socket strip, 1x21, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x21 2.00mm single row
0
21
21
Connector_PinSocket_2.00mm
PinSocket_1x21_P2.00mm_Vertical
Through hole straight socket strip, 1x21, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x21 2.00mm single row
0
21
21
Connector_PinSocket_2.00mm
PinSocket_1x21_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x21, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x21 2.00mm single row style1 pin1 left
0
21
21
Connector_PinSocket_2.00mm
PinSocket_1x21_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x21, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x21 2.00mm single row style2 pin1 right
0
21
21
Connector_PinSocket_2.00mm
PinSocket_1x22_P2.00mm_Horizontal
Through hole angled socket strip, 1x22, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x22 2.00mm single row
0
22
22
Connector_PinSocket_2.00mm
PinSocket_1x22_P2.00mm_Vertical
Through hole straight socket strip, 1x22, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x22 2.00mm single row
0
22
22
Connector_PinSocket_2.00mm
PinSocket_1x22_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x22, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x22 2.00mm single row style1 pin1 left
0
22
22
Connector_PinSocket_2.00mm
PinSocket_1x22_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x22, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x22 2.00mm single row style2 pin1 right
0
22
22
Connector_PinSocket_2.00mm
PinSocket_1x23_P2.00mm_Horizontal
Through hole angled socket strip, 1x23, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x23 2.00mm single row
0
23
23
Connector_PinSocket_2.00mm
PinSocket_1x23_P2.00mm_Vertical
Through hole straight socket strip, 1x23, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x23 2.00mm single row
0
23
23
Connector_PinSocket_2.00mm
PinSocket_1x23_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x23, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x23 2.00mm single row style1 pin1 left
0
23
23
Connector_PinSocket_2.00mm
PinSocket_1x23_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x23, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x23 2.00mm single row style2 pin1 right
0
23
23
Connector_PinSocket_2.00mm
PinSocket_1x24_P2.00mm_Horizontal
Through hole angled socket strip, 1x24, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x24 2.00mm single row
0
24
24
Connector_PinSocket_2.00mm
PinSocket_1x24_P2.00mm_Vertical
Through hole straight socket strip, 1x24, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x24 2.00mm single row
0
24
24
Connector_PinSocket_2.00mm
PinSocket_1x24_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x24, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x24 2.00mm single row style1 pin1 left
0
24
24
Connector_PinSocket_2.00mm
PinSocket_1x24_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x24, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x24 2.00mm single row style2 pin1 right
0
24
24
Connector_PinSocket_2.00mm
PinSocket_1x25_P2.00mm_Horizontal
Through hole angled socket strip, 1x25, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x25 2.00mm single row
0
25
25
Connector_PinSocket_2.00mm
PinSocket_1x25_P2.00mm_Vertical
Through hole straight socket strip, 1x25, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x25 2.00mm single row
0
25
25
Connector_PinSocket_2.00mm
PinSocket_1x25_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x25, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x25 2.00mm single row style1 pin1 left
0
25
25
Connector_PinSocket_2.00mm
PinSocket_1x25_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x25, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x25 2.00mm single row style2 pin1 right
0
25
25
Connector_PinSocket_2.00mm
PinSocket_1x26_P2.00mm_Horizontal
Through hole angled socket strip, 1x26, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x26 2.00mm single row
0
26
26
Connector_PinSocket_2.00mm
PinSocket_1x26_P2.00mm_Vertical
Through hole straight socket strip, 1x26, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x26 2.00mm single row
0
26
26
Connector_PinSocket_2.00mm
PinSocket_1x26_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x26, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x26 2.00mm single row style1 pin1 left
0
26
26
Connector_PinSocket_2.00mm
PinSocket_1x26_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x26, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x26 2.00mm single row style2 pin1 right
0
26
26
Connector_PinSocket_2.00mm
PinSocket_1x27_P2.00mm_Horizontal
Through hole angled socket strip, 1x27, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x27 2.00mm single row
0
27
27
Connector_PinSocket_2.00mm
PinSocket_1x27_P2.00mm_Vertical
Through hole straight socket strip, 1x27, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x27 2.00mm single row
0
27
27
Connector_PinSocket_2.00mm
PinSocket_1x27_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x27, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x27 2.00mm single row style1 pin1 left
0
27
27
Connector_PinSocket_2.00mm
PinSocket_1x27_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x27, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x27 2.00mm single row style2 pin1 right
0
27
27
Connector_PinSocket_2.00mm
PinSocket_1x28_P2.00mm_Horizontal
Through hole angled socket strip, 1x28, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x28 2.00mm single row
0
28
28
Connector_PinSocket_2.00mm
PinSocket_1x28_P2.00mm_Vertical
Through hole straight socket strip, 1x28, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x28 2.00mm single row
0
28
28
Connector_PinSocket_2.00mm
PinSocket_1x28_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x28, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x28 2.00mm single row style1 pin1 left
0
28
28
Connector_PinSocket_2.00mm
PinSocket_1x28_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x28, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x28 2.00mm single row style2 pin1 right
0
28
28
Connector_PinSocket_2.00mm
PinSocket_1x29_P2.00mm_Horizontal
Through hole angled socket strip, 1x29, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x29 2.00mm single row
0
29
29
Connector_PinSocket_2.00mm
PinSocket_1x29_P2.00mm_Vertical
Through hole straight socket strip, 1x29, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x29 2.00mm single row
0
29
29
Connector_PinSocket_2.00mm
PinSocket_1x29_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x29, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x29 2.00mm single row style1 pin1 left
0
29
29
Connector_PinSocket_2.00mm
PinSocket_1x29_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x29, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x29 2.00mm single row style2 pin1 right
0
29
29
Connector_PinSocket_2.00mm
PinSocket_1x30_P2.00mm_Horizontal
Through hole angled socket strip, 1x30, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x30 2.00mm single row
0
30
30
Connector_PinSocket_2.00mm
PinSocket_1x30_P2.00mm_Vertical
Through hole straight socket strip, 1x30, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x30 2.00mm single row
0
30
30
Connector_PinSocket_2.00mm
PinSocket_1x30_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x30, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x30 2.00mm single row style1 pin1 left
0
30
30
Connector_PinSocket_2.00mm
PinSocket_1x30_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x30, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x30 2.00mm single row style2 pin1 right
0
30
30
Connector_PinSocket_2.00mm
PinSocket_1x31_P2.00mm_Horizontal
Through hole angled socket strip, 1x31, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x31 2.00mm single row
0
31
31
Connector_PinSocket_2.00mm
PinSocket_1x31_P2.00mm_Vertical
Through hole straight socket strip, 1x31, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x31 2.00mm single row
0
31
31
Connector_PinSocket_2.00mm
PinSocket_1x31_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x31, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x31 2.00mm single row style1 pin1 left
0
31
31
Connector_PinSocket_2.00mm
PinSocket_1x31_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x31, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x31 2.00mm single row style2 pin1 right
0
31
31
Connector_PinSocket_2.00mm
PinSocket_1x32_P2.00mm_Horizontal
Through hole angled socket strip, 1x32, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x32 2.00mm single row
0
32
32
Connector_PinSocket_2.00mm
PinSocket_1x32_P2.00mm_Vertical
Through hole straight socket strip, 1x32, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x32 2.00mm single row
0
32
32
Connector_PinSocket_2.00mm
PinSocket_1x32_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x32, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x32 2.00mm single row style1 pin1 left
0
32
32
Connector_PinSocket_2.00mm
PinSocket_1x32_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x32, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x32 2.00mm single row style2 pin1 right
0
32
32
Connector_PinSocket_2.00mm
PinSocket_1x33_P2.00mm_Horizontal
Through hole angled socket strip, 1x33, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x33 2.00mm single row
0
33
33
Connector_PinSocket_2.00mm
PinSocket_1x33_P2.00mm_Vertical
Through hole straight socket strip, 1x33, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x33 2.00mm single row
0
33
33
Connector_PinSocket_2.00mm
PinSocket_1x33_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x33, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x33 2.00mm single row style1 pin1 left
0
33
33
Connector_PinSocket_2.00mm
PinSocket_1x33_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x33, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x33 2.00mm single row style2 pin1 right
0
33
33
Connector_PinSocket_2.00mm
PinSocket_1x34_P2.00mm_Horizontal
Through hole angled socket strip, 1x34, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x34 2.00mm single row
0
34
34
Connector_PinSocket_2.00mm
PinSocket_1x34_P2.00mm_Vertical
Through hole straight socket strip, 1x34, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x34 2.00mm single row
0
34
34
Connector_PinSocket_2.00mm
PinSocket_1x34_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x34, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x34 2.00mm single row style1 pin1 left
0
34
34
Connector_PinSocket_2.00mm
PinSocket_1x34_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x34, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x34 2.00mm single row style2 pin1 right
0
34
34
Connector_PinSocket_2.00mm
PinSocket_1x35_P2.00mm_Horizontal
Through hole angled socket strip, 1x35, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x35 2.00mm single row
0
35
35
Connector_PinSocket_2.00mm
PinSocket_1x35_P2.00mm_Vertical
Through hole straight socket strip, 1x35, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x35 2.00mm single row
0
35
35
Connector_PinSocket_2.00mm
PinSocket_1x35_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x35, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x35 2.00mm single row style1 pin1 left
0
35
35
Connector_PinSocket_2.00mm
PinSocket_1x35_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x35, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x35 2.00mm single row style2 pin1 right
0
35
35
Connector_PinSocket_2.00mm
PinSocket_1x36_P2.00mm_Horizontal
Through hole angled socket strip, 1x36, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x36 2.00mm single row
0
36
36
Connector_PinSocket_2.00mm
PinSocket_1x36_P2.00mm_Vertical
Through hole straight socket strip, 1x36, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x36 2.00mm single row
0
36
36
Connector_PinSocket_2.00mm
PinSocket_1x36_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x36, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x36 2.00mm single row style1 pin1 left
0
36
36
Connector_PinSocket_2.00mm
PinSocket_1x36_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x36, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x36 2.00mm single row style2 pin1 right
0
36
36
Connector_PinSocket_2.00mm
PinSocket_1x37_P2.00mm_Horizontal
Through hole angled socket strip, 1x37, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x37 2.00mm single row
0
37
37
Connector_PinSocket_2.00mm
PinSocket_1x37_P2.00mm_Vertical
Through hole straight socket strip, 1x37, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x37 2.00mm single row
0
37
37
Connector_PinSocket_2.00mm
PinSocket_1x37_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x37, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x37 2.00mm single row style1 pin1 left
0
37
37
Connector_PinSocket_2.00mm
PinSocket_1x37_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x37, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x37 2.00mm single row style2 pin1 right
0
37
37
Connector_PinSocket_2.00mm
PinSocket_1x38_P2.00mm_Horizontal
Through hole angled socket strip, 1x38, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x38 2.00mm single row
0
38
38
Connector_PinSocket_2.00mm
PinSocket_1x38_P2.00mm_Vertical
Through hole straight socket strip, 1x38, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x38 2.00mm single row
0
38
38
Connector_PinSocket_2.00mm
PinSocket_1x38_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x38, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x38 2.00mm single row style1 pin1 left
0
38
38
Connector_PinSocket_2.00mm
PinSocket_1x38_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x38, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x38 2.00mm single row style2 pin1 right
0
38
38
Connector_PinSocket_2.00mm
PinSocket_1x39_P2.00mm_Horizontal
Through hole angled socket strip, 1x39, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x39 2.00mm single row
0
39
39
Connector_PinSocket_2.00mm
PinSocket_1x39_P2.00mm_Vertical
Through hole straight socket strip, 1x39, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x39 2.00mm single row
0
39
39
Connector_PinSocket_2.00mm
PinSocket_1x39_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x39, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x39 2.00mm single row style1 pin1 left
0
39
39
Connector_PinSocket_2.00mm
PinSocket_1x39_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x39, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x39 2.00mm single row style2 pin1 right
0
39
39
Connector_PinSocket_2.00mm
PinSocket_1x40_P2.00mm_Horizontal
Through hole angled socket strip, 1x40, 2.00mm pitch, 6.35mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x40 2.00mm single row
0
40
40
Connector_PinSocket_2.00mm
PinSocket_1x40_P2.00mm_Vertical
Through hole straight socket strip, 1x40, 2.00mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x40 2.00mm single row
0
40
40
Connector_PinSocket_2.00mm
PinSocket_1x40_P2.00mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x40, 2.00mm pitch, single row, style 1 (pin 1 left) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x40 2.00mm single row style1 pin1 left
0
40
40
Connector_PinSocket_2.00mm
PinSocket_1x40_P2.00mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x40, 2.00mm pitch, single row, style 2 (pin 1 right) (https://www.jayconsystems.com/fileuploader/download/download/?d=1&file=custom%2Fupload%2FFile-1375728122.pdf), script generated
Surface mounted socket strip SMD 1x40 2.00mm single row style2 pin1 right
0
40
40
Connector_PinSocket_2.00mm
PinSocket_2x01_P2.00mm_Horizontal
Through hole angled socket strip, 2x01, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x01 2.00mm double row
0
2
2
Connector_PinSocket_2.00mm
PinSocket_2x01_P2.00mm_Vertical
Through hole straight socket strip, 2x01, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x01 2.00mm double row
0
2
2
Connector_PinSocket_2.00mm
PinSocket_2x01_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x01, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x01 2.00mm double row
0
2
2
Connector_PinSocket_2.00mm
PinSocket_2x02_P2.00mm_Horizontal
Through hole angled socket strip, 2x02, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x02 2.00mm double row
0
4
4
Connector_PinSocket_2.00mm
PinSocket_2x02_P2.00mm_Vertical
Through hole straight socket strip, 2x02, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x02 2.00mm double row
0
4
4
Connector_PinSocket_2.00mm
PinSocket_2x02_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x02, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x02 2.00mm double row
0
4
4
Connector_PinSocket_2.00mm
PinSocket_2x03_P2.00mm_Horizontal
Through hole angled socket strip, 2x03, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x03 2.00mm double row
0
6
6
Connector_PinSocket_2.00mm
PinSocket_2x03_P2.00mm_Vertical
Through hole straight socket strip, 2x03, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x03 2.00mm double row
0
6
6
Connector_PinSocket_2.00mm
PinSocket_2x03_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x03, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x03 2.00mm double row
0
6
6
Connector_PinSocket_2.00mm
PinSocket_2x04_P2.00mm_Horizontal
Through hole angled socket strip, 2x04, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x04 2.00mm double row
0
8
8
Connector_PinSocket_2.00mm
PinSocket_2x04_P2.00mm_Vertical
Through hole straight socket strip, 2x04, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x04 2.00mm double row
0
8
8
Connector_PinSocket_2.00mm
PinSocket_2x04_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x04, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x04 2.00mm double row
0
8
8
Connector_PinSocket_2.00mm
PinSocket_2x05_P2.00mm_Horizontal
Through hole angled socket strip, 2x05, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x05 2.00mm double row
0
10
10
Connector_PinSocket_2.00mm
PinSocket_2x05_P2.00mm_Vertical
Through hole straight socket strip, 2x05, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x05 2.00mm double row
0
10
10
Connector_PinSocket_2.00mm
PinSocket_2x05_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x05, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x05 2.00mm double row
0
10
10
Connector_PinSocket_2.00mm
PinSocket_2x06_P2.00mm_Horizontal
Through hole angled socket strip, 2x06, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x06 2.00mm double row
0
12
12
Connector_PinSocket_2.00mm
PinSocket_2x06_P2.00mm_Vertical
Through hole straight socket strip, 2x06, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x06 2.00mm double row
0
12
12
Connector_PinSocket_2.00mm
PinSocket_2x06_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x06, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x06 2.00mm double row
0
12
12
Connector_PinSocket_2.00mm
PinSocket_2x07_P2.00mm_Horizontal
Through hole angled socket strip, 2x07, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x07 2.00mm double row
0
14
14
Connector_PinSocket_2.00mm
PinSocket_2x07_P2.00mm_Vertical
Through hole straight socket strip, 2x07, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x07 2.00mm double row
0
14
14
Connector_PinSocket_2.00mm
PinSocket_2x07_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x07, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x07 2.00mm double row
0
14
14
Connector_PinSocket_2.00mm
PinSocket_2x08_P2.00mm_Horizontal
Through hole angled socket strip, 2x08, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x08 2.00mm double row
0
16
16
Connector_PinSocket_2.00mm
PinSocket_2x08_P2.00mm_Vertical
Through hole straight socket strip, 2x08, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x08 2.00mm double row
0
16
16
Connector_PinSocket_2.00mm
PinSocket_2x08_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x08, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x08 2.00mm double row
0
16
16
Connector_PinSocket_2.00mm
PinSocket_2x09_P2.00mm_Horizontal
Through hole angled socket strip, 2x09, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x09 2.00mm double row
0
18
18
Connector_PinSocket_2.00mm
PinSocket_2x09_P2.00mm_Vertical
Through hole straight socket strip, 2x09, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x09 2.00mm double row
0
18
18
Connector_PinSocket_2.00mm
PinSocket_2x09_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x09, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x09 2.00mm double row
0
18
18
Connector_PinSocket_2.00mm
PinSocket_2x10_P2.00mm_Horizontal
Through hole angled socket strip, 2x10, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x10 2.00mm double row
0
20
20
Connector_PinSocket_2.00mm
PinSocket_2x10_P2.00mm_Vertical
Through hole straight socket strip, 2x10, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x10 2.00mm double row
0
20
20
Connector_PinSocket_2.00mm
PinSocket_2x10_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x10, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x10 2.00mm double row
0
20
20
Connector_PinSocket_2.00mm
PinSocket_2x11_P2.00mm_Horizontal
Through hole angled socket strip, 2x11, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x11 2.00mm double row
0
22
22
Connector_PinSocket_2.00mm
PinSocket_2x11_P2.00mm_Vertical
Through hole straight socket strip, 2x11, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x11 2.00mm double row
0
22
22
Connector_PinSocket_2.00mm
PinSocket_2x11_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x11, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x11 2.00mm double row
0
22
22
Connector_PinSocket_2.00mm
PinSocket_2x12_P2.00mm_Horizontal
Through hole angled socket strip, 2x12, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x12 2.00mm double row
0
24
24
Connector_PinSocket_2.00mm
PinSocket_2x12_P2.00mm_Vertical
Through hole straight socket strip, 2x12, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x12 2.00mm double row
0
24
24
Connector_PinSocket_2.00mm
PinSocket_2x12_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x12, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x12 2.00mm double row
0
24
24
Connector_PinSocket_2.00mm
PinSocket_2x13_P2.00mm_Horizontal
Through hole angled socket strip, 2x13, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x13 2.00mm double row
0
26
26
Connector_PinSocket_2.00mm
PinSocket_2x13_P2.00mm_Vertical
Through hole straight socket strip, 2x13, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x13 2.00mm double row
0
26
26
Connector_PinSocket_2.00mm
PinSocket_2x13_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x13, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x13 2.00mm double row
0
26
26
Connector_PinSocket_2.00mm
PinSocket_2x14_P2.00mm_Horizontal
Through hole angled socket strip, 2x14, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x14 2.00mm double row
0
28
28
Connector_PinSocket_2.00mm
PinSocket_2x14_P2.00mm_Vertical
Through hole straight socket strip, 2x14, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x14 2.00mm double row
0
28
28
Connector_PinSocket_2.00mm
PinSocket_2x14_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x14, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x14 2.00mm double row
0
28
28
Connector_PinSocket_2.00mm
PinSocket_2x15_P2.00mm_Horizontal
Through hole angled socket strip, 2x15, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x15 2.00mm double row
0
30
30
Connector_PinSocket_2.00mm
PinSocket_2x15_P2.00mm_Vertical
Through hole straight socket strip, 2x15, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x15 2.00mm double row
0
30
30
Connector_PinSocket_2.00mm
PinSocket_2x15_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x15, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x15 2.00mm double row
0
30
30
Connector_PinSocket_2.00mm
PinSocket_2x16_P2.00mm_Horizontal
Through hole angled socket strip, 2x16, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x16 2.00mm double row
0
32
32
Connector_PinSocket_2.00mm
PinSocket_2x16_P2.00mm_Vertical
Through hole straight socket strip, 2x16, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x16 2.00mm double row
0
32
32
Connector_PinSocket_2.00mm
PinSocket_2x16_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x16, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x16 2.00mm double row
0
32
32
Connector_PinSocket_2.00mm
PinSocket_2x17_P2.00mm_Horizontal
Through hole angled socket strip, 2x17, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x17 2.00mm double row
0
34
34
Connector_PinSocket_2.00mm
PinSocket_2x17_P2.00mm_Vertical
Through hole straight socket strip, 2x17, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x17 2.00mm double row
0
34
34
Connector_PinSocket_2.00mm
PinSocket_2x17_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x17, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x17 2.00mm double row
0
34
34
Connector_PinSocket_2.00mm
PinSocket_2x18_P2.00mm_Horizontal
Through hole angled socket strip, 2x18, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x18 2.00mm double row
0
36
36
Connector_PinSocket_2.00mm
PinSocket_2x18_P2.00mm_Vertical
Through hole straight socket strip, 2x18, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x18 2.00mm double row
0
36
36
Connector_PinSocket_2.00mm
PinSocket_2x18_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x18, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x18 2.00mm double row
0
36
36
Connector_PinSocket_2.00mm
PinSocket_2x19_P2.00mm_Horizontal
Through hole angled socket strip, 2x19, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x19 2.00mm double row
0
38
38
Connector_PinSocket_2.00mm
PinSocket_2x19_P2.00mm_Vertical
Through hole straight socket strip, 2x19, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x19 2.00mm double row
0
38
38
Connector_PinSocket_2.00mm
PinSocket_2x19_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x19, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x19 2.00mm double row
0
38
38
Connector_PinSocket_2.00mm
PinSocket_2x20_P2.00mm_Horizontal
Through hole angled socket strip, 2x20, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x20 2.00mm double row
0
40
40
Connector_PinSocket_2.00mm
PinSocket_2x20_P2.00mm_Vertical
Through hole straight socket strip, 2x20, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x20 2.00mm double row
0
40
40
Connector_PinSocket_2.00mm
PinSocket_2x20_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x20, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x20 2.00mm double row
0
40
40
Connector_PinSocket_2.00mm
PinSocket_2x21_P2.00mm_Horizontal
Through hole angled socket strip, 2x21, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x21 2.00mm double row
0
42
42
Connector_PinSocket_2.00mm
PinSocket_2x21_P2.00mm_Vertical
Through hole straight socket strip, 2x21, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x21 2.00mm double row
0
42
42
Connector_PinSocket_2.00mm
PinSocket_2x21_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x21, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x21 2.00mm double row
0
42
42
Connector_PinSocket_2.00mm
PinSocket_2x22_P2.00mm_Horizontal
Through hole angled socket strip, 2x22, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x22 2.00mm double row
0
44
44
Connector_PinSocket_2.00mm
PinSocket_2x22_P2.00mm_Vertical
Through hole straight socket strip, 2x22, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x22 2.00mm double row
0
44
44
Connector_PinSocket_2.00mm
PinSocket_2x22_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x22, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x22 2.00mm double row
0
44
44
Connector_PinSocket_2.00mm
PinSocket_2x23_P2.00mm_Horizontal
Through hole angled socket strip, 2x23, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x23 2.00mm double row
0
46
46
Connector_PinSocket_2.00mm
PinSocket_2x23_P2.00mm_Vertical
Through hole straight socket strip, 2x23, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x23 2.00mm double row
0
46
46
Connector_PinSocket_2.00mm
PinSocket_2x23_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x23, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x23 2.00mm double row
0
46
46
Connector_PinSocket_2.00mm
PinSocket_2x24_P2.00mm_Horizontal
Through hole angled socket strip, 2x24, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x24 2.00mm double row
0
48
48
Connector_PinSocket_2.00mm
PinSocket_2x24_P2.00mm_Vertical
Through hole straight socket strip, 2x24, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x24 2.00mm double row
0
48
48
Connector_PinSocket_2.00mm
PinSocket_2x24_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x24, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x24 2.00mm double row
0
48
48
Connector_PinSocket_2.00mm
PinSocket_2x25_P2.00mm_Horizontal
Through hole angled socket strip, 2x25, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x25 2.00mm double row
0
50
50
Connector_PinSocket_2.00mm
PinSocket_2x25_P2.00mm_Vertical
Through hole straight socket strip, 2x25, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x25 2.00mm double row
0
50
50
Connector_PinSocket_2.00mm
PinSocket_2x25_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x25, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x25 2.00mm double row
0
50
50
Connector_PinSocket_2.00mm
PinSocket_2x26_P2.00mm_Horizontal
Through hole angled socket strip, 2x26, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x26 2.00mm double row
0
52
52
Connector_PinSocket_2.00mm
PinSocket_2x26_P2.00mm_Vertical
Through hole straight socket strip, 2x26, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x26 2.00mm double row
0
52
52
Connector_PinSocket_2.00mm
PinSocket_2x26_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x26, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x26 2.00mm double row
0
52
52
Connector_PinSocket_2.00mm
PinSocket_2x27_P2.00mm_Horizontal
Through hole angled socket strip, 2x27, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x27 2.00mm double row
0
54
54
Connector_PinSocket_2.00mm
PinSocket_2x27_P2.00mm_Vertical
Through hole straight socket strip, 2x27, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x27 2.00mm double row
0
54
54
Connector_PinSocket_2.00mm
PinSocket_2x27_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x27, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x27 2.00mm double row
0
54
54
Connector_PinSocket_2.00mm
PinSocket_2x28_P2.00mm_Horizontal
Through hole angled socket strip, 2x28, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x28 2.00mm double row
0
56
56
Connector_PinSocket_2.00mm
PinSocket_2x28_P2.00mm_Vertical
Through hole straight socket strip, 2x28, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x28 2.00mm double row
0
56
56
Connector_PinSocket_2.00mm
PinSocket_2x28_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x28, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x28 2.00mm double row
0
56
56
Connector_PinSocket_2.00mm
PinSocket_2x29_P2.00mm_Horizontal
Through hole angled socket strip, 2x29, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x29 2.00mm double row
0
58
58
Connector_PinSocket_2.00mm
PinSocket_2x29_P2.00mm_Vertical
Through hole straight socket strip, 2x29, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x29 2.00mm double row
0
58
58
Connector_PinSocket_2.00mm
PinSocket_2x29_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x29, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x29 2.00mm double row
0
58
58
Connector_PinSocket_2.00mm
PinSocket_2x30_P2.00mm_Horizontal
Through hole angled socket strip, 2x30, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x30 2.00mm double row
0
60
60
Connector_PinSocket_2.00mm
PinSocket_2x30_P2.00mm_Vertical
Through hole straight socket strip, 2x30, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x30 2.00mm double row
0
60
60
Connector_PinSocket_2.00mm
PinSocket_2x30_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x30, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x30 2.00mm double row
0
60
60
Connector_PinSocket_2.00mm
PinSocket_2x31_P2.00mm_Horizontal
Through hole angled socket strip, 2x31, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x31 2.00mm double row
0
62
62
Connector_PinSocket_2.00mm
PinSocket_2x31_P2.00mm_Vertical
Through hole straight socket strip, 2x31, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x31 2.00mm double row
0
62
62
Connector_PinSocket_2.00mm
PinSocket_2x31_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x31, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x31 2.00mm double row
0
62
62
Connector_PinSocket_2.00mm
PinSocket_2x32_P2.00mm_Horizontal
Through hole angled socket strip, 2x32, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x32 2.00mm double row
0
64
64
Connector_PinSocket_2.00mm
PinSocket_2x32_P2.00mm_Vertical
Through hole straight socket strip, 2x32, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x32 2.00mm double row
0
64
64
Connector_PinSocket_2.00mm
PinSocket_2x32_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x32, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x32 2.00mm double row
0
64
64
Connector_PinSocket_2.00mm
PinSocket_2x33_P2.00mm_Horizontal
Through hole angled socket strip, 2x33, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x33 2.00mm double row
0
66
66
Connector_PinSocket_2.00mm
PinSocket_2x33_P2.00mm_Vertical
Through hole straight socket strip, 2x33, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x33 2.00mm double row
0
66
66
Connector_PinSocket_2.00mm
PinSocket_2x33_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x33, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x33 2.00mm double row
0
66
66
Connector_PinSocket_2.00mm
PinSocket_2x34_P2.00mm_Horizontal
Through hole angled socket strip, 2x34, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x34 2.00mm double row
0
68
68
Connector_PinSocket_2.00mm
PinSocket_2x34_P2.00mm_Vertical
Through hole straight socket strip, 2x34, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x34 2.00mm double row
0
68
68
Connector_PinSocket_2.00mm
PinSocket_2x34_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x34, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x34 2.00mm double row
0
68
68
Connector_PinSocket_2.00mm
PinSocket_2x35_P2.00mm_Horizontal
Through hole angled socket strip, 2x35, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x35 2.00mm double row
0
70
70
Connector_PinSocket_2.00mm
PinSocket_2x35_P2.00mm_Vertical
Through hole straight socket strip, 2x35, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x35 2.00mm double row
0
70
70
Connector_PinSocket_2.00mm
PinSocket_2x35_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x35, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x35 2.00mm double row
0
70
70
Connector_PinSocket_2.00mm
PinSocket_2x36_P2.00mm_Horizontal
Through hole angled socket strip, 2x36, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x36 2.00mm double row
0
72
72
Connector_PinSocket_2.00mm
PinSocket_2x36_P2.00mm_Vertical
Through hole straight socket strip, 2x36, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x36 2.00mm double row
0
72
72
Connector_PinSocket_2.00mm
PinSocket_2x36_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x36, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x36 2.00mm double row
0
72
72
Connector_PinSocket_2.00mm
PinSocket_2x37_P2.00mm_Horizontal
Through hole angled socket strip, 2x37, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x37 2.00mm double row
0
74
74
Connector_PinSocket_2.00mm
PinSocket_2x37_P2.00mm_Vertical
Through hole straight socket strip, 2x37, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x37 2.00mm double row
0
74
74
Connector_PinSocket_2.00mm
PinSocket_2x37_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x37, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x37 2.00mm double row
0
74
74
Connector_PinSocket_2.00mm
PinSocket_2x38_P2.00mm_Horizontal
Through hole angled socket strip, 2x38, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x38 2.00mm double row
0
76
76
Connector_PinSocket_2.00mm
PinSocket_2x38_P2.00mm_Vertical
Through hole straight socket strip, 2x38, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x38 2.00mm double row
0
76
76
Connector_PinSocket_2.00mm
PinSocket_2x38_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x38, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x38 2.00mm double row
0
76
76
Connector_PinSocket_2.00mm
PinSocket_2x39_P2.00mm_Horizontal
Through hole angled socket strip, 2x39, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x39 2.00mm double row
0
78
78
Connector_PinSocket_2.00mm
PinSocket_2x39_P2.00mm_Vertical
Through hole straight socket strip, 2x39, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x39 2.00mm double row
0
78
78
Connector_PinSocket_2.00mm
PinSocket_2x39_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x39, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x39 2.00mm double row
0
78
78
Connector_PinSocket_2.00mm
PinSocket_2x40_P2.00mm_Horizontal
Through hole angled socket strip, 2x40, 2.00mm pitch, 6.35mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x40 2.00mm double row
0
80
80
Connector_PinSocket_2.00mm
PinSocket_2x40_P2.00mm_Vertical
Through hole straight socket strip, 2x40, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x40 2.00mm double row
0
80
80
Connector_PinSocket_2.00mm
PinSocket_2x40_P2.00mm_Vertical_SMD
surface-mounted straight socket strip, 2x40, 2.00mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x40 2.00mm double row
0
80
80
Connector_PinSocket_2.54mm
PinSocket_1x01_P2.54mm_Horizontal
Through hole angled socket strip, 1x01, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x01 2.54mm single row
0
1
1
Connector_PinSocket_2.54mm
PinSocket_1x01_P2.54mm_Vertical
Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x01 2.54mm single row
0
1
1
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Horizontal
Through hole angled socket strip, 1x02, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x02 2.54mm single row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Vertical
Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x02 2.54mm single row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x02, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x02 2.54mm single row style1 pin1 left
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x02_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x02, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x02 2.54mm single row style2 pin1 right
0
2
2
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Horizontal
Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x03 2.54mm single row
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Vertical
Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x03 2.54mm single row
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x03 2.54mm single row style1 pin1 left
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x03_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x03, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x03 2.54mm single row style2 pin1 right
0
3
3
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Horizontal
Through hole angled socket strip, 1x04, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x04 2.54mm single row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Vertical
Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x04 2.54mm single row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x04, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x04 2.54mm single row style1 pin1 left
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x04_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x04 2.54mm single row style2 pin1 right
0
4
4
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Horizontal
Through hole angled socket strip, 1x05, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x05 2.54mm single row
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Vertical
Through hole straight socket strip, 1x05, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x05 2.54mm single row
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x05 2.54mm single row style1 pin1 left
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x05_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x05, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x05 2.54mm single row style2 pin1 right
0
5
5
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Horizontal
Through hole angled socket strip, 1x06, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x06 2.54mm single row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Vertical
Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x06 2.54mm single row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x06, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x06 2.54mm single row style1 pin1 left
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x06_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x06, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x06 2.54mm single row style2 pin1 right
0
6
6
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Horizontal
Through hole angled socket strip, 1x07, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x07 2.54mm single row
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Vertical
Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x07 2.54mm single row
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x07, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x07 2.54mm single row style1 pin1 left
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x07_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x07, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x07 2.54mm single row style2 pin1 right
0
7
7
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Horizontal
Through hole angled socket strip, 1x08, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x08 2.54mm single row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Vertical
Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x08 2.54mm single row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x08 2.54mm single row style1 pin1 left
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x08 2.54mm single row style2 pin1 right
0
8
8
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Horizontal
Through hole angled socket strip, 1x09, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x09 2.54mm single row
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Vertical
Through hole straight socket strip, 1x09, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x09 2.54mm single row
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x09, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x09 2.54mm single row style1 pin1 left
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x09_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x09, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x09 2.54mm single row style2 pin1 right
0
9
9
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Horizontal
Through hole angled socket strip, 1x10, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x10 2.54mm single row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Vertical
Through hole straight socket strip, 1x10, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x10 2.54mm single row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x10, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x10 2.54mm single row style1 pin1 left
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x10_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x10, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x10 2.54mm single row style2 pin1 right
0
10
10
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Horizontal
Through hole angled socket strip, 1x11, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x11 2.54mm single row
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Vertical
Through hole straight socket strip, 1x11, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x11 2.54mm single row
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x11, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x11 2.54mm single row style1 pin1 left
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x11_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x11, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x11 2.54mm single row style2 pin1 right
0
11
11
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Horizontal
Through hole angled socket strip, 1x12, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x12 2.54mm single row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Vertical
Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x12 2.54mm single row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x12, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x12 2.54mm single row style1 pin1 left
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x12_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x12, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x12 2.54mm single row style2 pin1 right
0
12
12
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Horizontal
Through hole angled socket strip, 1x13, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x13 2.54mm single row
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Vertical
Through hole straight socket strip, 1x13, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x13 2.54mm single row
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x13, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x13 2.54mm single row style1 pin1 left
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x13_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x13, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x13 2.54mm single row style2 pin1 right
0
13
13
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Horizontal
Through hole angled socket strip, 1x14, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x14 2.54mm single row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Vertical
Through hole straight socket strip, 1x14, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x14 2.54mm single row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x14 2.54mm single row style1 pin1 left
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x14_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x14, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x14 2.54mm single row style2 pin1 right
0
14
14
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Horizontal
Through hole angled socket strip, 1x15, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x15 2.54mm single row
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Vertical
Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x15 2.54mm single row
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x15, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x15 2.54mm single row style1 pin1 left
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x15_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x15, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x15 2.54mm single row style2 pin1 right
0
15
15
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Horizontal
Through hole angled socket strip, 1x16, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x16 2.54mm single row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Vertical
Through hole straight socket strip, 1x16, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x16 2.54mm single row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x16, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x16 2.54mm single row style1 pin1 left
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x16_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x16, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x16 2.54mm single row style2 pin1 right
0
16
16
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Horizontal
Through hole angled socket strip, 1x17, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x17 2.54mm single row
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Vertical
Through hole straight socket strip, 1x17, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x17 2.54mm single row
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x17, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x17 2.54mm single row style1 pin1 left
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x17_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x17, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x17 2.54mm single row style2 pin1 right
0
17
17
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Horizontal
Through hole angled socket strip, 1x18, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x18 2.54mm single row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Vertical
Through hole straight socket strip, 1x18, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x18 2.54mm single row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x18, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x18 2.54mm single row style1 pin1 left
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x18_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x18, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x18 2.54mm single row style2 pin1 right
0
18
18
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Horizontal
Through hole angled socket strip, 1x19, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x19 2.54mm single row
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Vertical
Through hole straight socket strip, 1x19, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x19 2.54mm single row
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x19, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x19 2.54mm single row style1 pin1 left
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x19_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x19, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x19 2.54mm single row style2 pin1 right
0
19
19
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Horizontal
Through hole angled socket strip, 1x20, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x20 2.54mm single row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Vertical
Through hole straight socket strip, 1x20, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x20 2.54mm single row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x20, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x20 2.54mm single row style1 pin1 left
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x20_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x20, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x20 2.54mm single row style2 pin1 right
0
20
20
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Horizontal
Through hole angled socket strip, 1x21, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x21 2.54mm single row
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Vertical
Through hole straight socket strip, 1x21, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x21 2.54mm single row
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x21, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x21 2.54mm single row style1 pin1 left
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x21_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x21, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x21 2.54mm single row style2 pin1 right
0
21
21
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Horizontal
Through hole angled socket strip, 1x22, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x22 2.54mm single row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Vertical
Through hole straight socket strip, 1x22, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x22 2.54mm single row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x22, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x22 2.54mm single row style1 pin1 left
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x22_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x22, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x22 2.54mm single row style2 pin1 right
0
22
22
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Horizontal
Through hole angled socket strip, 1x23, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x23 2.54mm single row
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Vertical
Through hole straight socket strip, 1x23, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x23 2.54mm single row
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x23, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x23 2.54mm single row style1 pin1 left
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x23_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x23, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x23 2.54mm single row style2 pin1 right
0
23
23
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Horizontal
Through hole angled socket strip, 1x24, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x24 2.54mm single row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Vertical
Through hole straight socket strip, 1x24, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x24 2.54mm single row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x24, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x24 2.54mm single row style1 pin1 left
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x24_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x24, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x24 2.54mm single row style2 pin1 right
0
24
24
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Horizontal
Through hole angled socket strip, 1x25, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x25 2.54mm single row
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Vertical
Through hole straight socket strip, 1x25, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x25 2.54mm single row
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x25, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x25 2.54mm single row style1 pin1 left
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x25_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x25, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x25 2.54mm single row style2 pin1 right
0
25
25
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Horizontal
Through hole angled socket strip, 1x26, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x26 2.54mm single row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Vertical
Through hole straight socket strip, 1x26, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x26 2.54mm single row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x26, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x26 2.54mm single row style1 pin1 left
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x26_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x26, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x26 2.54mm single row style2 pin1 right
0
26
26
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Horizontal
Through hole angled socket strip, 1x27, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x27 2.54mm single row
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Vertical
Through hole straight socket strip, 1x27, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x27 2.54mm single row
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x27, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x27 2.54mm single row style1 pin1 left
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x27_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x27, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x27 2.54mm single row style2 pin1 right
0
27
27
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Horizontal
Through hole angled socket strip, 1x28, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x28 2.54mm single row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Vertical
Through hole straight socket strip, 1x28, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x28 2.54mm single row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x28, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x28 2.54mm single row style1 pin1 left
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x28_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x28, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x28 2.54mm single row style2 pin1 right
0
28
28
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Horizontal
Through hole angled socket strip, 1x29, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x29 2.54mm single row
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Vertical
Through hole straight socket strip, 1x29, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x29 2.54mm single row
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x29, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x29 2.54mm single row style1 pin1 left
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x29_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x29, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x29 2.54mm single row style2 pin1 right
0
29
29
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Horizontal
Through hole angled socket strip, 1x30, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x30 2.54mm single row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Vertical
Through hole straight socket strip, 1x30, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x30 2.54mm single row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x30, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x30 2.54mm single row style1 pin1 left
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x30_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x30, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x30 2.54mm single row style2 pin1 right
0
30
30
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Horizontal
Through hole angled socket strip, 1x31, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x31 2.54mm single row
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Vertical
Through hole straight socket strip, 1x31, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x31 2.54mm single row
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x31, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x31 2.54mm single row style1 pin1 left
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x31_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x31, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x31 2.54mm single row style2 pin1 right
0
31
31
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Horizontal
Through hole angled socket strip, 1x32, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x32 2.54mm single row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Vertical
Through hole straight socket strip, 1x32, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x32 2.54mm single row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x32, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x32 2.54mm single row style1 pin1 left
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x32_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x32, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x32 2.54mm single row style2 pin1 right
0
32
32
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Horizontal
Through hole angled socket strip, 1x33, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x33 2.54mm single row
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Vertical
Through hole straight socket strip, 1x33, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x33 2.54mm single row
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x33, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x33 2.54mm single row style1 pin1 left
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x33_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x33, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x33 2.54mm single row style2 pin1 right
0
33
33
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Horizontal
Through hole angled socket strip, 1x34, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x34 2.54mm single row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Vertical
Through hole straight socket strip, 1x34, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x34 2.54mm single row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x34, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x34 2.54mm single row style1 pin1 left
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x34_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x34, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x34 2.54mm single row style2 pin1 right
0
34
34
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Horizontal
Through hole angled socket strip, 1x35, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x35 2.54mm single row
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Vertical
Through hole straight socket strip, 1x35, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x35 2.54mm single row
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x35, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x35 2.54mm single row style1 pin1 left
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x35_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x35, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x35 2.54mm single row style2 pin1 right
0
35
35
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Horizontal
Through hole angled socket strip, 1x36, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x36 2.54mm single row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Vertical
Through hole straight socket strip, 1x36, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x36 2.54mm single row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x36, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x36 2.54mm single row style1 pin1 left
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x36_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x36, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x36 2.54mm single row style2 pin1 right
0
36
36
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Horizontal
Through hole angled socket strip, 1x37, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x37 2.54mm single row
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Vertical
Through hole straight socket strip, 1x37, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x37 2.54mm single row
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x37, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x37 2.54mm single row style1 pin1 left
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x37_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x37, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x37 2.54mm single row style2 pin1 right
0
37
37
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Horizontal
Through hole angled socket strip, 1x38, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x38 2.54mm single row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Vertical
Through hole straight socket strip, 1x38, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x38 2.54mm single row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x38, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x38 2.54mm single row style1 pin1 left
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x38_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x38, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x38 2.54mm single row style2 pin1 right
0
38
38
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Horizontal
Through hole angled socket strip, 1x39, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x39 2.54mm single row
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Vertical
Through hole straight socket strip, 1x39, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x39 2.54mm single row
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x39, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x39 2.54mm single row style1 pin1 left
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x39_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x39, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x39 2.54mm single row style2 pin1 right
0
39
39
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Horizontal
Through hole angled socket strip, 1x40, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x40 2.54mm single row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Vertical
Through hole straight socket strip, 1x40, 2.54mm pitch, single row (from Kicad 4.0.7), script generated
Through hole socket strip THT 1x40 2.54mm single row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Vertical_SMD_Pin1Left
surface-mounted straight socket strip, 1x40, 2.54mm pitch, single row, style 1 (pin 1 left) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x40 2.54mm single row style1 pin1 left
0
40
40
Connector_PinSocket_2.54mm
PinSocket_1x40_P2.54mm_Vertical_SMD_Pin1Right
surface-mounted straight socket strip, 1x40, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated
Surface mounted socket strip SMD 1x40 2.54mm single row style2 pin1 right
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x01_P2.54mm_Horizontal
Through hole angled socket strip, 2x01, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x01 2.54mm double row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_2x01_P2.54mm_Vertical
Through hole straight socket strip, 2x01, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x01 2.54mm double row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_2x01_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x01, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x01 2.54mm double row
0
2
2
Connector_PinSocket_2.54mm
PinSocket_2x02_P2.54mm_Horizontal
Through hole angled socket strip, 2x02, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x02 2.54mm double row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_2x02_P2.54mm_Vertical
Through hole straight socket strip, 2x02, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x02 2.54mm double row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_2x02_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x02, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x02 2.54mm double row
0
4
4
Connector_PinSocket_2.54mm
PinSocket_2x03_P2.54mm_Horizontal
Through hole angled socket strip, 2x03, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x03 2.54mm double row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_2x03_P2.54mm_Vertical
Through hole straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x03 2.54mm double row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_2x03_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x03 2.54mm double row
0
6
6
Connector_PinSocket_2.54mm
PinSocket_2x04_P2.54mm_Horizontal
Through hole angled socket strip, 2x04, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x04 2.54mm double row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_2x04_P2.54mm_Vertical
Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x04 2.54mm double row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_2x04_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x04 2.54mm double row
0
8
8
Connector_PinSocket_2.54mm
PinSocket_2x05_P2.54mm_Horizontal
Through hole angled socket strip, 2x05, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x05 2.54mm double row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_2x05_P2.54mm_Vertical
Through hole straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x05 2.54mm double row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_2x05_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x05, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x05 2.54mm double row
0
10
10
Connector_PinSocket_2.54mm
PinSocket_2x06_P2.54mm_Horizontal
Through hole angled socket strip, 2x06, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x06 2.54mm double row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_2x06_P2.54mm_Vertical
Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x06 2.54mm double row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_2x06_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x06 2.54mm double row
0
12
12
Connector_PinSocket_2.54mm
PinSocket_2x07_P2.54mm_Horizontal
Through hole angled socket strip, 2x07, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x07 2.54mm double row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_2x07_P2.54mm_Vertical
Through hole straight socket strip, 2x07, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x07 2.54mm double row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_2x07_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x07, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x07 2.54mm double row
0
14
14
Connector_PinSocket_2.54mm
PinSocket_2x08_P2.54mm_Horizontal
Through hole angled socket strip, 2x08, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x08 2.54mm double row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_2x08_P2.54mm_Vertical
Through hole straight socket strip, 2x08, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x08 2.54mm double row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_2x08_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x08, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x08 2.54mm double row
0
16
16
Connector_PinSocket_2.54mm
PinSocket_2x09_P2.54mm_Horizontal
Through hole angled socket strip, 2x09, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x09 2.54mm double row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_2x09_P2.54mm_Vertical
Through hole straight socket strip, 2x09, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x09 2.54mm double row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_2x09_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x09, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x09 2.54mm double row
0
18
18
Connector_PinSocket_2.54mm
PinSocket_2x10_P2.54mm_Horizontal
Through hole angled socket strip, 2x10, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x10 2.54mm double row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_2x10_P2.54mm_Vertical
Through hole straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x10 2.54mm double row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_2x10_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x10, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x10 2.54mm double row
0
20
20
Connector_PinSocket_2.54mm
PinSocket_2x11_P2.54mm_Horizontal
Through hole angled socket strip, 2x11, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x11 2.54mm double row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_2x11_P2.54mm_Vertical
Through hole straight socket strip, 2x11, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x11 2.54mm double row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_2x11_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x11, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x11 2.54mm double row
0
22
22
Connector_PinSocket_2.54mm
PinSocket_2x12_P2.54mm_Horizontal
Through hole angled socket strip, 2x12, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x12 2.54mm double row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_2x12_P2.54mm_Vertical
Through hole straight socket strip, 2x12, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x12 2.54mm double row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_2x12_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x12, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x12 2.54mm double row
0
24
24
Connector_PinSocket_2.54mm
PinSocket_2x13_P2.54mm_Horizontal
Through hole angled socket strip, 2x13, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x13 2.54mm double row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_2x13_P2.54mm_Vertical
Through hole straight socket strip, 2x13, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x13 2.54mm double row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_2x13_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x13, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x13 2.54mm double row
0
26
26
Connector_PinSocket_2.54mm
PinSocket_2x14_P2.54mm_Horizontal
Through hole angled socket strip, 2x14, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x14 2.54mm double row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_2x14_P2.54mm_Vertical
Through hole straight socket strip, 2x14, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x14 2.54mm double row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_2x14_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x14, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x14 2.54mm double row
0
28
28
Connector_PinSocket_2.54mm
PinSocket_2x15_P2.54mm_Horizontal
Through hole angled socket strip, 2x15, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x15 2.54mm double row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_2x15_P2.54mm_Vertical
Through hole straight socket strip, 2x15, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x15 2.54mm double row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_2x15_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x15, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x15 2.54mm double row
0
30
30
Connector_PinSocket_2.54mm
PinSocket_2x16_P2.54mm_Horizontal
Through hole angled socket strip, 2x16, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x16 2.54mm double row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_2x16_P2.54mm_Vertical
Through hole straight socket strip, 2x16, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x16 2.54mm double row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_2x16_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x16, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x16 2.54mm double row
0
32
32
Connector_PinSocket_2.54mm
PinSocket_2x17_P2.54mm_Horizontal
Through hole angled socket strip, 2x17, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x17 2.54mm double row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_2x17_P2.54mm_Vertical
Through hole straight socket strip, 2x17, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x17 2.54mm double row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_2x17_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x17, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x17 2.54mm double row
0
34
34
Connector_PinSocket_2.54mm
PinSocket_2x18_P2.54mm_Horizontal
Through hole angled socket strip, 2x18, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x18 2.54mm double row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_2x18_P2.54mm_Vertical
Through hole straight socket strip, 2x18, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x18 2.54mm double row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_2x18_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x18, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x18 2.54mm double row
0
36
36
Connector_PinSocket_2.54mm
PinSocket_2x19_P2.54mm_Horizontal
Through hole angled socket strip, 2x19, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x19 2.54mm double row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_2x19_P2.54mm_Vertical
Through hole straight socket strip, 2x19, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x19 2.54mm double row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_2x19_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x19, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x19 2.54mm double row
0
38
38
Connector_PinSocket_2.54mm
PinSocket_2x20_P2.54mm_Horizontal
Through hole angled socket strip, 2x20, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x20 2.54mm double row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x20_P2.54mm_Vertical
Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x20 2.54mm double row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x20_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x20 2.54mm double row
0
40
40
Connector_PinSocket_2.54mm
PinSocket_2x21_P2.54mm_Horizontal
Through hole angled socket strip, 2x21, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x21 2.54mm double row
0
42
42
Connector_PinSocket_2.54mm
PinSocket_2x21_P2.54mm_Vertical
Through hole straight socket strip, 2x21, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x21 2.54mm double row
0
42
42
Connector_PinSocket_2.54mm
PinSocket_2x21_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x21, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x21 2.54mm double row
0
42
42
Connector_PinSocket_2.54mm
PinSocket_2x22_P2.54mm_Horizontal
Through hole angled socket strip, 2x22, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x22 2.54mm double row
0
44
44
Connector_PinSocket_2.54mm
PinSocket_2x22_P2.54mm_Vertical
Through hole straight socket strip, 2x22, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x22 2.54mm double row
0
44
44
Connector_PinSocket_2.54mm
PinSocket_2x22_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x22, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x22 2.54mm double row
0
44
44
Connector_PinSocket_2.54mm
PinSocket_2x23_P2.54mm_Horizontal
Through hole angled socket strip, 2x23, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x23 2.54mm double row
0
46
46
Connector_PinSocket_2.54mm
PinSocket_2x23_P2.54mm_Vertical
Through hole straight socket strip, 2x23, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x23 2.54mm double row
0
46
46
Connector_PinSocket_2.54mm
PinSocket_2x23_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x23, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x23 2.54mm double row
0
46
46
Connector_PinSocket_2.54mm
PinSocket_2x24_P2.54mm_Horizontal
Through hole angled socket strip, 2x24, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x24 2.54mm double row
0
48
48
Connector_PinSocket_2.54mm
PinSocket_2x24_P2.54mm_Vertical
Through hole straight socket strip, 2x24, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x24 2.54mm double row
0
48
48
Connector_PinSocket_2.54mm
PinSocket_2x24_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x24, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x24 2.54mm double row
0
48
48
Connector_PinSocket_2.54mm
PinSocket_2x25_P2.54mm_Horizontal
Through hole angled socket strip, 2x25, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x25 2.54mm double row
0
50
50
Connector_PinSocket_2.54mm
PinSocket_2x25_P2.54mm_Vertical
Through hole straight socket strip, 2x25, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x25 2.54mm double row
0
50
50
Connector_PinSocket_2.54mm
PinSocket_2x25_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x25, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x25 2.54mm double row
0
50
50
Connector_PinSocket_2.54mm
PinSocket_2x26_P2.54mm_Horizontal
Through hole angled socket strip, 2x26, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x26 2.54mm double row
0
52
52
Connector_PinSocket_2.54mm
PinSocket_2x26_P2.54mm_Vertical
Through hole straight socket strip, 2x26, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x26 2.54mm double row
0
52
52
Connector_PinSocket_2.54mm
PinSocket_2x26_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x26, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x26 2.54mm double row
0
52
52
Connector_PinSocket_2.54mm
PinSocket_2x27_P2.54mm_Horizontal
Through hole angled socket strip, 2x27, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x27 2.54mm double row
0
54
54
Connector_PinSocket_2.54mm
PinSocket_2x27_P2.54mm_Vertical
Through hole straight socket strip, 2x27, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x27 2.54mm double row
0
54
54
Connector_PinSocket_2.54mm
PinSocket_2x27_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x27, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x27 2.54mm double row
0
54
54
Connector_PinSocket_2.54mm
PinSocket_2x28_P2.54mm_Horizontal
Through hole angled socket strip, 2x28, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x28 2.54mm double row
0
56
56
Connector_PinSocket_2.54mm
PinSocket_2x28_P2.54mm_Vertical
Through hole straight socket strip, 2x28, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x28 2.54mm double row
0
56
56
Connector_PinSocket_2.54mm
PinSocket_2x28_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x28, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x28 2.54mm double row
0
56
56
Connector_PinSocket_2.54mm
PinSocket_2x29_P2.54mm_Horizontal
Through hole angled socket strip, 2x29, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x29 2.54mm double row
0
58
58
Connector_PinSocket_2.54mm
PinSocket_2x29_P2.54mm_Vertical
Through hole straight socket strip, 2x29, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x29 2.54mm double row
0
58
58
Connector_PinSocket_2.54mm
PinSocket_2x29_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x29, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x29 2.54mm double row
0
58
58
Connector_PinSocket_2.54mm
PinSocket_2x30_P2.54mm_Horizontal
Through hole angled socket strip, 2x30, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x30 2.54mm double row
0
60
60
Connector_PinSocket_2.54mm
PinSocket_2x30_P2.54mm_Vertical
Through hole straight socket strip, 2x30, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x30 2.54mm double row
0
60
60
Connector_PinSocket_2.54mm
PinSocket_2x30_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x30, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x30 2.54mm double row
0
60
60
Connector_PinSocket_2.54mm
PinSocket_2x31_P2.54mm_Horizontal
Through hole angled socket strip, 2x31, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x31 2.54mm double row
0
62
62
Connector_PinSocket_2.54mm
PinSocket_2x31_P2.54mm_Vertical
Through hole straight socket strip, 2x31, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x31 2.54mm double row
0
62
62
Connector_PinSocket_2.54mm
PinSocket_2x31_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x31, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x31 2.54mm double row
0
62
62
Connector_PinSocket_2.54mm
PinSocket_2x32_P2.54mm_Horizontal
Through hole angled socket strip, 2x32, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x32 2.54mm double row
0
64
64
Connector_PinSocket_2.54mm
PinSocket_2x32_P2.54mm_Vertical
Through hole straight socket strip, 2x32, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x32 2.54mm double row
0
64
64
Connector_PinSocket_2.54mm
PinSocket_2x32_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x32, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x32 2.54mm double row
0
64
64
Connector_PinSocket_2.54mm
PinSocket_2x33_P2.54mm_Horizontal
Through hole angled socket strip, 2x33, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x33 2.54mm double row
0
66
66
Connector_PinSocket_2.54mm
PinSocket_2x33_P2.54mm_Vertical
Through hole straight socket strip, 2x33, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x33 2.54mm double row
0
66
66
Connector_PinSocket_2.54mm
PinSocket_2x33_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x33, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x33 2.54mm double row
0
66
66
Connector_PinSocket_2.54mm
PinSocket_2x34_P2.54mm_Horizontal
Through hole angled socket strip, 2x34, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x34 2.54mm double row
0
68
68
Connector_PinSocket_2.54mm
PinSocket_2x34_P2.54mm_Vertical
Through hole straight socket strip, 2x34, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x34 2.54mm double row
0
68
68
Connector_PinSocket_2.54mm
PinSocket_2x34_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x34, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x34 2.54mm double row
0
68
68
Connector_PinSocket_2.54mm
PinSocket_2x35_P2.54mm_Horizontal
Through hole angled socket strip, 2x35, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x35 2.54mm double row
0
70
70
Connector_PinSocket_2.54mm
PinSocket_2x35_P2.54mm_Vertical
Through hole straight socket strip, 2x35, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x35 2.54mm double row
0
70
70
Connector_PinSocket_2.54mm
PinSocket_2x35_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x35, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x35 2.54mm double row
0
70
70
Connector_PinSocket_2.54mm
PinSocket_2x36_P2.54mm_Horizontal
Through hole angled socket strip, 2x36, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x36 2.54mm double row
0
72
72
Connector_PinSocket_2.54mm
PinSocket_2x36_P2.54mm_Vertical
Through hole straight socket strip, 2x36, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x36 2.54mm double row
0
72
72
Connector_PinSocket_2.54mm
PinSocket_2x36_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x36, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x36 2.54mm double row
0
72
72
Connector_PinSocket_2.54mm
PinSocket_2x37_P2.54mm_Horizontal
Through hole angled socket strip, 2x37, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x37 2.54mm double row
0
74
74
Connector_PinSocket_2.54mm
PinSocket_2x37_P2.54mm_Vertical
Through hole straight socket strip, 2x37, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x37 2.54mm double row
0
74
74
Connector_PinSocket_2.54mm
PinSocket_2x37_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x37, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x37 2.54mm double row
0
74
74
Connector_PinSocket_2.54mm
PinSocket_2x38_P2.54mm_Horizontal
Through hole angled socket strip, 2x38, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x38 2.54mm double row
0
76
76
Connector_PinSocket_2.54mm
PinSocket_2x38_P2.54mm_Vertical
Through hole straight socket strip, 2x38, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x38 2.54mm double row
0
76
76
Connector_PinSocket_2.54mm
PinSocket_2x38_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x38, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x38 2.54mm double row
0
76
76
Connector_PinSocket_2.54mm
PinSocket_2x39_P2.54mm_Horizontal
Through hole angled socket strip, 2x39, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x39 2.54mm double row
0
78
78
Connector_PinSocket_2.54mm
PinSocket_2x39_P2.54mm_Vertical
Through hole straight socket strip, 2x39, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x39 2.54mm double row
0
78
78
Connector_PinSocket_2.54mm
PinSocket_2x39_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x39, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x39 2.54mm double row
0
78
78
Connector_PinSocket_2.54mm
PinSocket_2x40_P2.54mm_Horizontal
Through hole angled socket strip, 2x40, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 2x40 2.54mm double row
0
80
80
Connector_PinSocket_2.54mm
PinSocket_2x40_P2.54mm_Vertical
Through hole straight socket strip, 2x40, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Through hole socket strip THT 2x40 2.54mm double row
0
80
80
Connector_PinSocket_2.54mm
PinSocket_2x40_P2.54mm_Vertical_SMD
surface-mounted straight socket strip, 2x40, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated
Surface mounted socket strip SMD 2x40 2.54mm double row
0
80
80
Diode_SMD
D_0201_0603Metric
Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator
diode
0
4
2
Diode_SMD
D_0201_0603Metric_Pad0.64x0.40mm_HandSolder
Diode SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator
diode handsolder
0
4
2
Diode_SMD
D_0402_1005Metric
Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_0402_1005Metric_Pad0.77x0.64mm_HandSolder
Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_0603_1608Metric
Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_0603_1608Metric_Pad1.05x0.95mm_HandSolder
Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_0805_2012Metric
Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_0805_2012Metric_Pad1.15x1.40mm_HandSolder
Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_01005_0402Metric
Diode SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator
diode
0
4
2
Diode_SMD
D_01005_0402Metric_Pad0.57x0.30mm_HandSolder
Diode SMD 01005 (0402 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.vishay.com/docs/20056/crcw01005e3.pdf), generated with kicad-footprint-generator
diode handsolder
0
4
2
Diode_SMD
D_1206_3216Metric
Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1206_3216Metric_Pad1.42x1.75mm_HandSolder
Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_1210_3225Metric
Diode SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1210_3225Metric_Pad1.42x2.65mm_HandSolder
Diode SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_1812_4532Metric
Diode SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_1812_4532Metric_Pad1.30x3.40mm_HandSolder
Diode SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2010_5025Metric
Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2010_5025Metric_Pad1.52x2.65mm_HandSolder
Diode SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2114_3652Metric
Diode SMD 2114 (3652 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2114_3652Metric_Pad1.85x3.75mm_HandSolder
Diode SMD 2114 (3652 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_2512_6332Metric
Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_2512_6332Metric_Pad1.52x3.35mm_HandSolder
Diode SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_3220_8050Metric
Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode
0
2
2
Diode_SMD
D_3220_8050Metric_Pad2.65x5.15mm_HandSolder
Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator
diode handsolder
0
2
2
Diode_SMD
D_MELF
Diode, MELF,,
Diode MELF 
0
2
2
Diode_SMD
D_MELF-RM10_Universal_Handsoldering
Diode, Universal, MELF, RM10, Handsoldering, SMD, Thruhole,
Diode Universal MELF RM10 Handsoldering SMD Thruhole 
0
2
2
Diode_SMD
D_MELF_Handsoldering
Diode MELF Handsoldering
Diode MELF Handsoldering
0
2
2
Diode_SMD
D_MicroMELF
Diode, MicroMELF, Reflow Soldering, http://www.vishay.com/docs/85597/bzm55.pdf
MicroMELF Diode
0
2
2
Diode_SMD
D_MicroMELF_Handsoldering
Diode, MicroMELF, Hand Soldering, http://www.vishay.com/docs/85597/bzm55.pdf
MicroMELF Diode
0
2
2
Diode_SMD
D_MiniMELF
Diode Mini-MELF (SOD-80)
Diode Mini-MELF (SOD-80)
0
2
2
Diode_SMD
D_MiniMELF_Handsoldering
Diode Mini-MELF (SOD-80) Handsoldering
Diode Mini-MELF (SOD-80) Handsoldering
0
2
2
Diode_SMD
D_PowerDI-5
PowerDI,Diode,Vishay,https://www.diodes.com/assets/Package-Files/PowerDI5.pdf
PowerDI diode vishay
0
3
2
Diode_SMD
D_PowerDI-123
http://www.diodes.com/_files/datasheets/ds30497.pdf
PowerDI diode vishay
0
2
2
Diode_SMD
D_Powermite2_AK
Microsemi Powermite 2 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5341)
PowerMite2
0
2
2
Diode_SMD
D_Powermite2_KA
Microsemi Powermite 2 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5341)
PowerMite2
0
2
2
Diode_SMD
D_Powermite3
Microsemi Powermite 3 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5340)
PowerMite3
0
3
3
Diode_SMD
D_Powermite_AK
Microsemi Powermite SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5339, https://www.onsemi.com/pub/Collateral/457-04.PDF)
Powermite
0
2
2
Diode_SMD
D_Powermite_KA
Microsemi Powermite SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5339, https://www.onsemi.com/pub/Collateral/457-04.PDF)
Powermite
0
2
2
Diode_SMD
D_QFN_3.3x3.3mm_P0.65mm
QFN, diode, 3.3x3.3x1mm (https://www.wolfspeed.com/media/downloads/846/C3D1P7060Q.pdf)
diode qfn 3.3
0
3
2
Diode_SMD
D_SC-80
JEITA SC-80
SC-80
0
2
2
Diode_SMD
D_SC-80_HandSoldering
JEITA SC-80
SC-80
0
2
2
Diode_SMD
D_SMA
Diode SMA (DO-214AC)
Diode SMA (DO-214AC)
0
2
2
Diode_SMD
D_SMA-SMB_Universal_Handsoldering
Diode, Universal, SMA (DO-214AC) or SMB (DO-214AA), Handsoldering,
Diode Universal SMA (DO-214AC) SMB (DO-214AA) Handsoldering 
0
2
2
Diode_SMD
D_SMA_Handsoldering
Diode SMA (DO-214AC) Handsoldering
Diode SMA (DO-214AC) Handsoldering
0
2
2
Diode_SMD
D_SMB
Diode SMB (DO-214AA)
Diode SMB (DO-214AA)
0
2
2
Diode_SMD
D_SMB-SMC_Universal_Handsoldering
Diode, Universal, SMB(DO-214AA) or SMC (DO-214AB), Handsoldering,
Diode Universal SMB(DO-214AA) SMC (DO-214AB) Handsoldering 
0
2
2
Diode_SMD
D_SMB_Handsoldering
Diode SMB (DO-214AA) Handsoldering
Diode SMB (DO-214AA) Handsoldering
0
2
2
Diode_SMD
D_SMB_Modified
Diode SMB (DO-214AA) Modified (http://www.littelfuse.com/~/media/electronics/datasheets/sidactors/littelfuse_sidactor_battrax_positive_negative_modified_do_214_datasheet.pdf.pdf)
Diode SMB (DO-214AA)
0
3
3
Diode_SMD
D_SMC
Diode SMC (DO-214AB)
Diode SMC (DO-214AB)
0
2
2
Diode_SMD
D_SMC-RM10_Universal_Handsoldering
Diode, Universal, SMC (DO-214AB), RM10, Handsoldering, SMD, Thruhole
Diode Universal SMC (DO-214AB) RM10 Handsoldering SMD Thruhole
0
2
2
Diode_SMD
D_SMC_Handsoldering
Diode SMC (DO-214AB) Handsoldering
Diode SMC (DO-214AB) Handsoldering
0
2
2
Diode_SMD
D_SMF
Diode SMF (DO-219AB), http://www.vishay.com/docs/95572/smf_do-219ab.pdf
Diode SMF (DO-214AB)
0
2
2
Diode_SMD
D_SOD-110
SOD-110
SOD-110
0
2
2
Diode_SMD
D_SOD-123
SOD-123
SOD-123
0
2
2
Diode_SMD
D_SOD-123F
D_SOD-123F
D_SOD-123F
0
2
2
Diode_SMD
D_SOD-128
D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf
D_SOD-128
0
2
2
Diode_SMD
D_SOD-323
SOD-323
SOD-323
0
2
2
Diode_SMD
D_SOD-323F
SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf
SOD-323F
0
2
2
Diode_SMD
D_SOD-323_HandSoldering
SOD-323
SOD-323
0
2
2
Diode_SMD
D_SOD-523
http://www.diodes.com/datasheets/ap02001.pdf p.144
Diode SOD523
0
2
2
Diode_SMD
D_SOD-923
https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF#page=4
Diode SOD923
0
2
2
Diode_SMD
D_TUMD2
ROHM - TUMD2
TUMD2
0
2
2
Diode_SMD
Diode_Bridge_Bourns_CD-DF4xxS
8.1x10.5mm, 4A, single phase bridge rectifier, https://www.bourns.com/docs/Product-Datasheets/CD-DF4xxSL.pdf
Surface Mount Bridge Rectifier Diode
0
4
4
Diode_SMD
Diode_Bridge_Diotec_ABS
SMD diode bridge ABS (Diotec), see https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf
ABS MBLS
0
4
4
Diode_SMD
Diode_Bridge_Diotec_MicroDil_3.0x3.0x1.8mm
SMD package Diotec Diotec MicroDil, body 3.0x3.0x1.8mm (e.g. diode bridge), see https://diotec.com/tl_files/diotec/files/pdf/datasheets/mys40.pdf
Diotec MicroDil diode bridge
0
4
4
Diode_SMD
Diode_Bridge_Diotec_SO-DIL-Slim
SMD diode bridge Diotec SO-DIL Slim, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40fs.pdf
DFS SO-DIL Slim
0
4
4
Diode_SMD
Diode_Bridge_OnSemi_SDIP-4L
SMD diode bridge OnSemi SDIP-4L, see https://www.onsemi.com/pdf/datasheet/df10s1-d.pdf
OnSemi Diode Bridge SDIP-4L
0
4
4
Diode_SMD
Diode_Bridge_Vishay_DFS
SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf
DFS
0
4
4
Diode_SMD
Diode_Bridge_Vishay_DFSFlat
SMD diode bridge Low Profile DFS "Flat", see http://www.vishay.com/docs/88874/dfl15005.pdf
DFS
0
4
4
Diode_SMD
Diode_Bridge_Vishay_MBLS
SMD diode bridge MBLS, see http://www.vishay.com/docs/89959/mbl104s.pdf http://www.vishay.com/docs/88854/padlayouts.pdf
DFS
0
4
4
Diode_SMD
Littelfuse_PolyZen-LS
http://m.littelfuse.com/~/media/electronics/datasheets/polyzen_devices/littelfuse_polyzen_standard_polyzen_catalog_datasheet.pdf.pdf
Diode Polymer Protected Zener Diode Littelfuse LS
0
3
3
Diode_SMD
Nexperia_CFP3_SOD-123W
Nexperia CFP3 (SOD-123W), https://assets.nexperia.com/documents/outline-drawing/SOD123W.pdf
CFP3 SOD-123W
0
2
2
HD_Capacitors
C0402


0
2
2
HD_Capacitors
C0603


0
2
2
HD_Capacitors
C0805
Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
capacitor
0
2
2
HD_Capacitors
C1206
Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
HD_Capacitors
C1210
Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
HD_Capacitors
C1812
Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
HD_Capacitors
C2010
Capacitor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
HD_Capacitors
C2512
Capacitor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
HD_Connectors
Barrel_Jack_SMT


0
4
2
HD_Connectors
GMX-SMT2-N-44


0
4
4
HD_Connectors
Header_1x02_P2.54mm


0
2
2
HD_Connectors
Header_1x03_P2.54mm
Through hole straight pin header, 1x03, 2.54mm pitch, single row
Through hole pin header THT 1x03 2.54mm single row
0
3
3
HD_Connectors
Hirose_DF1BZ-4DP-2.5DS


0
4
4
HD_Connectors
JST_ZH_5PIN_B5B-ZR-SM4-TF


0
7
6
HD_Connectors
JST_ZH_5PIN_S5B-ZR-SM4A-TF


0
7
6
HD_Connectors
PROGTEST_PROBE_EDGE_CONNECTOR


0
36
36
HD_Connectors
PROGTEST_TESTER_EDGE_SOCKET


0
36
36
HD_Connectors
PinHeader_2x07_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x07 1.27mm double row
0
14
14
HD_Connectors
PinSocket_1x05_P2.54mm_Horizontal
Through hole angled socket strip, 1x05, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x05 2.54mm single row
0
5
5
HD_Connectors
RPi_Connector


0
40
40
HD_Connectors
SWD_Connector_THT


0
5
5
HD_Connectors
SWD_Connector_for_PogoHeader


0
5
5
HD_Connectors
Solder_Pads_Thin_1x2


0
2
2
HD_Connectors
Sullins_SWR204-NRTN-D02-RA-GA


0
4
4
HD_Connectors
TerminalBlock_1x4_PhoenixContact_P3.5mm


0
4
4
HD_Connectors
Testing_Probe_Socket


0
1
1
HD_Connectors
U.FL_TE_1909763-1


0
3
2
HD_Connectors
USB_C_Receptacle_GCT_USB4085
USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf
USB Type-C Receptacle Through-hole Right angle
0
20
17
HD_Connectors
WAGO_2060-452


0
4
2
HD_DFN_QFN
4-VDFN_2x2mm


0
4
4
HD_DFN_QFN
QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm
QFN, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf#page=34), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
25
21
HD_DFN_QFN
QFN-28_4x4mm_P0.5mm
QFN, 28 Pin (http://www.st.com/resource/en/datasheet/stm32f031k6.pdf#page=90), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
28
28
HD_DFN_QFN
QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm_ThermalVias
QFN, 36 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/36L_QFN_6x6_with_3_7x3_7_EP_Punch_Dimpled_4E_C04-0241A.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
63
37
HD_DFN_QFN
QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm


0
65
49
HD_DFN_QFN
ST_UFQFPN-20_3x3mm_P0.5mm
UFQFPN 20-lead, 3 x 3 mm, 0.5 mm pitch, ultra thin fine pitch quad flat package (http://www.st.com/resource/en/datasheet/stm8s003f3.pdf)
UFQFPN 0.5
0
20
20
HD_DFN_QFN
TDFN-8-1EP_2x2mm_P0.5mm


0
8
8
HD_DFN_QFN
TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm
TDFN, 8 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0168.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py
TDFN NoLead
0
13
9
HD_DFN_QFN
TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm
TDFN, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6V66-Family-Data-Sheet-DS20006266A.pdf#page=35), generated with kicad-footprint-generator ipc_noLead_generator.py
TDFN NoLead
0
13
9
HD_DFN_QFN
Texas_S-PWQFN-N24_EP2.7x2.7mm
QFN, 24 Pin (http://www.ti.com/lit/ds/symlink/bq25601.pdf#page=54), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
29
25
HD_Diodes
D_SOD-323
SOD-323
SOD-323
0
2
2
HD_Diodes
D_SOD-323F
SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf
SOD-323F
0
2
2
HD_Diodes
LED_ASMB-KTF0-0A306


0
4
4
HD_Diodes
LED_QLS6B-FKW-CNSNSF043


0
6
6
HD_Diodes
RF-W2SA50TS-A39R


0
6
6
HD_Inductors
L0402
Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
HD_Inductors
L0603
Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
HD_Inductors
L0805
Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
inductor
0
2
2
HD_Inductors
L_EPL2014


0
2
2
HD_Inductors
L_NR40xx


0
2
2
HD_LGA
LGA-12_2x2mm_P0.5mm
LGA12
lga land grid array
0
12
12
HD_LGA
LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y
LGA, 16 Pin (http://www.st.com/resource/en/datasheet/lis331hh.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py
LGA NoLead
0
16
16
HD_Logos
OSHW-Logo2_7.3x6mm_SilkScreen
Open Source Hardware Symbol
Logo Symbol OSHW
0
0
0
HD_Logos
OSHW-Logo2_7.3x6mm_SilkScreen_no_text


0
0
0
HD_Logos
OSHW-Logo2_9.8x8mm_SilkScreen
Open Source Hardware Symbol
Logo Symbol OSHW
0
0
0
HD_Logos
OSHW-Logo_5.7x6mm_SilkScreen
Open Source Hardware Logo
Logo OSHW
0
0
0
HD_Logos
OSHW-Logo_7.5x8mm_SilkScreen
Open Source Hardware Logo
Logo OSHW
0
0
0
HD_Logos
OSHW-Logo_11.4x12mm_SilkScreen
Open Source Hardware Logo
Logo OSHW
0
0
0
HD_Other
0900FM15D0039


0
10
10
HD_Other
ANT_W3012_3


0
3
2
HD_Other
Breakaway_tab_holes


0
0
0
HD_Other
CMT-7525S-SMT-TR


0
4
4
HD_Other
EMI_Gasket_16.51x16.51mm


0
16
1
HD_Other
EMI_Gasket_20x20mm


0
20
1
HD_Other
F0603


0
2
2
HD_Other
F1206


0
2
2
HD_Other
Fiducial_0.5mm_Mask1.5mm
Circular Fiducial, 0.5mm bare copper, 1.5mm soldermask opening
fiducial
0
1
0
HD_Other
Fiducial_0.5mm_Mask1mm
Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)
fiducial
0
1
0
HD_Other
Fiducial_1.5mm_Mask3mm
Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening
fiducial
0
1
0
HD_Other
Fiducial_1.5mm_Mask4.5mm
Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening
fiducial
0
1
0
HD_Other
Fiducial_1mm_Mask2mm
Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)
fiducial
0
1
0
HD_Other
Fiducial_1mm_Mask3mm
Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)
fiducial
0
1
0
HD_Other
LFB182G45CGFD436


0
3
3
HD_Other
MLPF-WB55-01E3


0
6
6
HD_Other
MODULE_STLINK-V3MODS


0
32
32
HD_Other
Meander_PCB_Antenna_2.4GHz


0
1
1
HD_Other
ProgTest_Tester_Module


0
14
14
HD_Other
RF_FORK


0
3
3
HD_Other
SB0603


0
2
2
HD_Other
SB0603_dual


0
4
3
HD_Other
SERIAL_NUMBER_SPACE


0
0
0
HD_Other
SIMCom_SIM800L


0
11
11
HD_Other
SW_KMS221GLFS


0
5
2
HD_Other
SW_KMS233GLFG


0
5
2
HD_Other
TEST_CHECKMARKS


0
0
0
HD_Other
TSNP-6-2


0
6
6
HD_Other
Tactile_Switch_6x6_SMT


0
4
2
HD_Other
Testpoint_SMD_1mm


0
1
1
HD_Other
Testpoint_SMD_2mm


0
1
1
HD_Other
soil_moisture_sensor_electrode


0
3
2
HD_QFP
LQFP-32_7x7mm_P0.8mm
LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
32
32
HD_QFP
LQFP-48_7x7mm_P0.5mm
LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
48
48
HD_QFP
LQFP-64_10x10mm_P0.5mm
64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)
QFP 0.5
0
64
64
HD_QFP
LQFP-100_14x14mm_P0.5mm
LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)
QFP 0.5
0
100
100
HD_QFP
LQFP-144_20x20mm_P0.5mm
144-Lead Plastic Low Profile Quad Flatpack (PL) - 20x20x1.40 mm Body [LQFP], 2.00 mm Footprint (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.5
0
144
144
HD_Resistors
R0402
Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
HD_Resistors
R0603


0
2
2
HD_Resistors
R0805


0
2
2
HD_Resistors
R1206
Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
HD_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
15
11
HD_SO
SOIC-8_3.9x4.9mm_P1.27mm
SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
HD_SO
SOT-223-3(TAB-pin-2)
module CMS SOT223 4 pins
CMS SOT
0
4
3
HD_SON
Texas_VSON8


0
9
9
HD_SOT
SOT-23
3-pin SOT-23 package

0
3
3
HD_SOT
SOT-23-5
5-pin SOT-23 package
SOT-23-6
0
5
5
HD_SOT
SOT-26-6
6-pin SOT-23 package

0
6
6
HD_SOT
SOT-223-3(TAB-pin-2)
module CMS SOT223 4 pins
CMS SOT
0
4
3
HD_SOT
SOT-363_SC-70-6
SOT-363, SC-70-6
SOT-363 SC-70-6
0
6
6
HD_SOT
SOT−563-6


0
6
6
HD_Sensors
SCD4x


0
21
21
HD_Sensors
SGP4x


0
7
7
HD_Sensors
SHT3x


0
9
9
HD_Sensors
SHT4x


0
4
4
HD_TO_SMD
TO-252-2(DPAK)


0
3
3
HD_TO_SMD
TO-263-2
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
7
3
HD_TO_SMD
TO-263-2(D2PAK)


0
3
3
HD_XTALs
ABM8G


0
4
4
HD_XTALs
ECX-32


0
4
4
HD_XTALs
NX2012SA


0
2
2
HD_XTALs
NX2016SA


0
4
4
MRS_Communication
ESP32-WROOM


0
39
39
MRS_Communication
HOPERF_RFM69HW
Radio, RF, Module, http://www.hoperf.com/upload/rf/RFM69HW-V1.3.pdf
Radio RF Module
0
16
16
MRS_Communication
RN2483A


0
47
47
MRS_Connectors
5-103361-1


0
3
3
MRS_Connectors
A2501WR-2P1


0
2
2
MRS_Connectors
A2501WR-3P1


0
3
3
MRS_Connectors
A2506WR-2P


0
2
2
MRS_Connectors
A2506WR-3P


0
3
3
MRS_Connectors
ADC-028-2-TR


0
4
2
MRS_Connectors
ANT_WIRE_THT


0
1
1
MRS_Connectors
BarrelJack_Horizontal
DC Barrel Jack
Power Jack
0
3
3
MRS_Connectors
BatteryHolder_Keystone_2468_2xAAA
2xAAA cell battery holder, Keystone P/N 2468, http://www.keyelco.com/product-pdf.cfm?p=1033
AAA battery cell holder
0
2
2
MRS_Connectors
DF13-4contacts


0
6
5
MRS_Connectors
DF13-9contacts


0
11
10
MRS_Connectors
ESC_CONNECTOR


0
18
5
MRS_Connectors
ESC_CONNECTOR2


0
18
5
MRS_Connectors
ESC_CONNECTOR_THIN


0
18
5
MRS_Connectors
ESC_CONNECTOR_THIN2


0
15
5
MRS_Connectors
HRS_DF40C-50DS-0.4V(51)


0
50
50
MRS_Connectors
Header_1x01_P2.54mm
Through hole straight pin header, 1x01, 2.54mm pitch, single row
Through hole pin header THT 1x01 2.54mm single row
0
1
1
MRS_Connectors
Header_1x01_P2.54mm_Horizontal
Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x01 2.54mm single row
0
1
1
MRS_Connectors
Header_1x01_P2.54mm_SMT
Through hole straight pin header, 1x01, 2.54mm pitch, single row
Through hole pin header THT 1x01 2.54mm single row
0
1
1
MRS_Connectors
Header_1x01_SMT_Square


0
1
1
MRS_Connectors
Header_1x02_P2.54mm
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
2
2
MRS_Connectors
Header_1x02_P2.54mm_Horizontal
Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x02 2.54mm single row
0
2
2
MRS_Connectors
Header_1x02_P2.54mm_SMT


0
2
2
MRS_Connectors
Header_1x02_P2mm_SMT
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
2
2
MRS_Connectors
Header_1x03_P2.54mm
Through hole straight pin header, 1x03, 2.54mm pitch, single row
Through hole pin header THT 1x03 2.54mm single row
0
3
3
MRS_Connectors
Header_1x03_P2.54mm_Horizontal
Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x03 2.54mm single row
0
3
3
MRS_Connectors
Header_1x03_P2mm_SMT


0
3
3
MRS_Connectors
Header_1x04_P2.54mm
Through hole straight pin header, 1x04, 2.54mm pitch, single row
Through hole pin header THT 1x04 2.54mm single row
0
4
4
MRS_Connectors
Header_1x04_P2.54mm_Horizontal
Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x04 2.54mm single row
0
4
4
MRS_Connectors
Header_1x05_P2.54mm
Through hole straight pin header, 1x05, 2.54mm pitch, single row
Through hole pin header THT 1x05 2.54mm single row
0
5
5
MRS_Connectors
Header_1x05_P2.54mm_Horizontal
Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x05 2.54mm single row
0
5
5
MRS_Connectors
Header_1x06_P2.54mm
Through hole straight pin header, 1x06, 2.54mm pitch, single row
Through hole pin header THT 1x06 2.54mm single row
0
6
6
MRS_Connectors
Header_1x06_P2.54mm_Horizontal
Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x06 2.54mm single row
0
6
6
MRS_Connectors
Header_1x07_P2.54mm
Through hole straight pin header, 1x07, 2.54mm pitch, single row
Through hole pin header THT 1x07 2.54mm single row
0
7
7
MRS_Connectors
Header_1x07_P2.54mm_Horizontal
Through hole angled pin header, 1x07, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x07 2.54mm single row
0
7
7
MRS_Connectors
Header_1x08_P2.54mm
Through hole straight pin header, 1x08, 2.54mm pitch, single row
Through hole pin header THT 1x08 2.54mm single row
0
8
8
MRS_Connectors
Header_1x08_P2.54mm_Horizontal
Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x08 2.54mm single row
0
8
8
MRS_Connectors
Header_1x08_P2mm_SMT


0
8
8
MRS_Connectors
Header_1x09_P2.54mm
Through hole straight pin header, 1x09, 2.54mm pitch, single row
Through hole pin header THT 1x09 2.54mm single row
0
9
9
MRS_Connectors
Header_1x09_P2.54mm_Horizontal
Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x09 2.54mm single row
0
9
9
MRS_Connectors
Header_1x10_P2.54mm
Through hole straight pin header, 1x10, 2.54mm pitch, single row
Through hole pin header THT 1x10 2.54mm single row
0
10
10
MRS_Connectors
Header_1x10_P2.54mm_Horizontal
Through hole angled pin header, 1x10, 2.54mm pitch, 6mm pin length, single row
Through hole angled pin header THT 1x10 2.54mm single row
0
10
10
MRS_Connectors
Header_1x10_P2mm_SMT
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
10
10
MRS_Connectors
Header_3x04_P2.54mm_Horizontal


0
12
12
MRS_Connectors
Hirose_DF52-4S-0.8H_1x04-1MP_P0.80mm_Horizontal
Hirose  series connector, DF52-4S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator
connector Hirose  top entry
0
6
5
MRS_Connectors
JST_GH-2


0
4
3
MRS_Connectors
JST_GH-2_side


0
4
3
MRS_Connectors
JST_GH-3


0
5
4
MRS_Connectors
JST_GH-3_side


0
5
4
MRS_Connectors
JST_GH-4


0
6
5
MRS_Connectors
JST_GH-4_side


0
6
5
MRS_Connectors
JST_GH-6


0
8
7
MRS_Connectors
JST_GH-6_side


0
8
7
MRS_Connectors
JST_GH-8


0
10
9
MRS_Connectors
JST_GH-8_side


0
10
9
MRS_Connectors
JST_GH-10


0
12
11
MRS_Connectors
JST_GH-10_side


0
12
11
MRS_Connectors
JST_PH-2_TOP_ENTRY


0
4
3
MRS_Connectors
JST_PH_2


0
4
3
MRS_Connectors
JST_PH_2_TB


0
4
3
MRS_Connectors
JST_XH_5pin


0
5
5
MRS_Connectors
Jumper
Through hole straight pin header, 1x02, 2.54mm pitch, single row
Through hole pin header THT 1x02 2.54mm single row
0
2
2
MRS_Connectors
MOLEX_2-1445057-2


0
4
3
MRS_Connectors
MOLEX_54548-2271


0
24
24
MRS_Connectors
Molex_22-03-5035


0
3
3
MRS_Connectors
Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical
Molex PicoBlade Connector System, 53047-0410, 4 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator
connector Molex PicoBlade side entry
0
4
4
MRS_Connectors
Molex_PicoBlade_53048-0410_1x04_P1.25mm_Horizontal
Molex PicoBlade Connector System, 53048-0410, 4 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator
connector Molex PicoBlade top entry
0
4
4
MRS_Connectors
NAKI_Light_Connector


0
3
3
MRS_Connectors
NXW-02


0
2
2
MRS_Connectors
NXW-03


0
3
3
MRS_Connectors
PinHeader_1x10_P2.00mm_Vertical
Through hole straight pin header, 1x10, 2.00mm pitch, single row
Through hole pin header THT 1x10 2.00mm single row
0
10
10
MRS_Connectors
PinHeader_2x04_P2.54mm_Vertical_SMD
surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows
Surface mounted pin header SMD 2x04 2.54mm double row
0
8
8
MRS_Connectors
S2B-ZR


0
2
2
MRS_Connectors
S3B-ZR


0
3
3
MRS_Connectors
SB0603


0
2
2
MRS_Connectors
SB0603_dual


0
4
3
MRS_Connectors
SB0603_pasted


0
2
2
MRS_Connectors
Socket_3x06_P2.54


0
18
18
MRS_Connectors
TE_BNC


0
5
2
MRS_Connectors
USB2_0_A_DOUBLE_WURTH_61400826021


0
12
9
MRS_Connectors
USB2_0_A_WURTH_62900416021


0
6
5
MRS_Connectors
USB2_0_A_WURTH_614004190021


0
6
5
MRS_Connectors
USB3.0B


0
11
10
MRS_Connectors
USB3_0_A_WURTH_692122030100


0
11
10
MRS_Connectors
USB_2_0_A_AMPHENOL_87583-2010BLF


0
6
5
MRS_Connectors
USB_C_Receptacle_Amphenol_12401548E4-2A
USB TYPE C, RA RCPT PCB, Hybrid, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401548E4%7e2A
USB C Type-C Receptacle Hybrid
0
28
25
MRS_Connectors
USB_C_Receptacle_Amphenol_12401610E4-2A
USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A
USB C Type-C Receptacle SMD
0
28
25
MRS_Connectors
USB_Mini-B_Lumberg_2486_01_Horizontal
USB Mini-B 5-pin SMD connector, http://downloads.lumberg.com/datenblaetter/en/2486_01.pdf
USB USB_B USB_Mini connector
0
9
6
MRS_Connectors
WE_1.0MM_ZIF_FPC_HORIZONTAL_TOP


0
30
29
MRS_Connectors
WE_1.0MM_ZIF_FPC_HORIZONTAL_TOP_28pin


0
30
29
MRS_Connectors
WE_1.0MM_ZIF_FPC_HORIZONTAL_TOP_30pin


0
32
31
MRS_Connectors
XT30PW-F


0
4
2
MRS_Connectors
XT30PW-M


0
4
2
MRS_Connectors
XT60


0
4
3
MRS_Connectors
XT60PW-M


0
4
4
MRS_Connectors
XT60_Vertical


0
2
2
MRS_Connectors
XT90PW-M


0
4
4
MRS_Connectors
XT90_Vertical


0
2
2
MRS_Connectors
power_connector_SMT


0
2
2
MRS_Connectors
power_connector_small


0
2
2
MRS_Connectors
power_connector_small_SMT


0
2
2
MRS_Connectors
power_connector_small_wide_vias_SMT


0
24
2
MRS_Connectors
power_input


0
18
2
MRS_Connectors
power_input_SMD


0
14
2
MRS_Diodes
D_SMA
Diode SMA (DO-214AC)
Diode SMA (DO-214AC)
0
2
2
MRS_Diodes
D_SMB


0
2
2
MRS_Diodes
D_SMC
Diode SMC (DO-214AB)
Diode SMC (DO-214AB)
0
2
2
MRS_Diodes
D_UDFN-6L


0
6
6
MRS_Diodes
ESD7016


0
10
8
MRS_Diodes
ESD7102


0
3
3
MRS_Diodes
LED_3,5x2,8mm_MULTICOMP


0
2
2
MRS_Diodes
LED_0603


0
2
2
MRS_Diodes
LED_0805


0
2
2
MRS_Diodes
LED_SML-LX1610RGBWA


0
4
4
MRS_Diodes
MicroQFN-8-L


0
12
8
MRS_Diodes
PM2B-1LLE


0
3
3
MRS_Diodes
RF-W2SA50TS-A39R


0
6
6
MRS_Diodes
SOD-123


0
2
2
MRS_Diodes
SOD-323


0
2
2
MRS_Diodes
SOD-723


0
2
2
MRS_Diodes
SOD-882


0
2
2
MRS_LGA
HLGA-10L


0
10
10
MRS_LGA
LGA_24_3.5x3


0
24
24
MRS_LGA
Texas_SIL0010A_MicroSiP-10-1EP_3.8x3mm_P0.6mm_EP0.7x2.9mm
Texas SIL0010A MicroSiP, 10 Pin (http://www.ti.com/lit/ml/mpds579b/mpds579b.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py
Texas MicroSiP NoLead
0
14
11
MRS_Logo
MRS_10mm


0
0
0
MRS_Logo
MRS_20mm


0
0
0
MRS_Logo
MRS_30mm


0
0
0
MRS_Logo
MRS_36mm


0
0
0
MRS_Logo
MRS_80mm


0
0
0
MRS_Logo
UVDAR_7mm


0
0
0
MRS_Logo
UVDAR_10mm


0
0
0
MRS_Logo
UVDAR_20mm


0
0
0
MRS_Mechanical
Breakaway_tab_holes


0
0
0
MRS_Mechanical
F330_arms_mounting_holes


0
0
0
MRS_Mechanical
F330_arms_mounting_holes_bottom


0
0
0
MRS_Mechanical
F450_Bottom_board_outline


0
0
0
MRS_Mechanical
F450_arm_mounting_holes1


0
36
1
MRS_Mechanical
F450_arm_mounting_holes2


0
36
1
MRS_Mechanical
Garmin_Mounting_holes


0
4
1
MRS_Mechanical
Jetson_Mounting_Holes


0
4
1
MRS_Mechanical
Mounting_hole_plated_1.7mm


0
1
1
MRS_Mechanical
Mounting_hole_plated_2.2mm


0
1
1
MRS_Mechanical
Mounting_hole_plated_3,2mm


0
9
1
MRS_Mechanical
Mounting_hole_plated_3,2mm_thin


0
1
1
MRS_Mechanical
Mounting_hole_plated_3mm


0
9
1
MRS_Mechanical
Mounting_hole_unplated_2.2mm


0
0
0
MRS_Mechanical
Mounting_hole_unplated_2.5mm


0
0
0
MRS_Mechanical
Mounting_hole_unplated_3,2mm


0
0
0
MRS_Mechanical
Mounting_hole_unplated_3mm


0
0
0
MRS_Mechanical
NUC_Mounting_Holes


0
4
1
MRS_Mechanical
PM07_mounting_holes


0
0
0
MRS_Mechanical
Pixhawk_2.1_Mounting_Holes


0
4
1
MRS_Mechanical
Pixhawk_4_Mounting_Holes


0
4
1
MRS_Mechanical
f450_arm_mouting_holes_bottom


0
18
2
MRS_Mechanical
f450_arm_mouting_holes_bottom_unplated


0
0
0
MRS_Passives
B1047AS-8R2N


0
2
2
MRS_Passives
C0402
Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
C0603


0
2
2
MRS_Passives
C0805
Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
C1206
Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
C1210
Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
C1812
Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
C2010
Capacitor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
C2512
Capacitor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
MRS_Passives
CTAN1206


0
2
2
MRS_Passives
CTAN2312


0
2
2
MRS_Passives
CTAN2412


0
2
2
MRS_Passives
CTAN2917


0
2
2
MRS_Passives
L0402
Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L0603
Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L0805
Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L1206
Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L1210
Inductor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L1812
Inductor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L2010
Inductor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L2512
Inductor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L2816
Inductor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator
inductor
0
2
2
MRS_Passives
L_ASPI-0418


0
2
2
MRS_Passives
L_ASPI-2410


0
2
2
MRS_Passives
L_Coilcraft_MLC12xx


0
2
2
MRS_Passives
L_Coilcraft_XxL4020
L_Coilcraft_XxL4020 https://www.coilcraft.com/pdfs/xfl4020.pdf
L Coilcraft XxL4020
0
2
2
MRS_Passives
L_DJNR3015


0
2
2
MRS_Passives
L_HC9-220-R


0
2
2
MRS_Passives
L_HPI1040


0
2
2
MRS_Passives
L_MSS1210-683MEB


0
2
2
MRS_Passives
L_PA4342.473ANLT


0
2
2
MRS_Passives
L_SRP6540


0
2
2
MRS_Passives
L_SRR1208


0
2
2
MRS_Passives
L_SRU1038


0
2
2
MRS_Passives
L_TYS252010L100M


0
2
2
MRS_Passives
L_XAL1010


0
2
2
MRS_Passives
R0402
Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
MRS_Passives
R0603


0
2
2
MRS_Passives
R0805


0
2
2
MRS_Passives
R1206
Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
MRS_Passives
R1812
Resistor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
resistor
0
2
2
MRS_Passives
R2010
Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
MRS_Passives
R2512


0
2
2
MRS_Passives
R3637_Reversed


0
2
2
MRS_Passives
R_Array_Concave_4x0402
Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)
resistor array
0
8
8
MRS_Power_Management
HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm
HVQFN, 24 Pin (https://www.nxp.com/docs/en/package-information/SOT616-3.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py
HVQFN NoLead
0
29
23
MRS_QFN
B3QFN


0
27
15
MRS_QFN
B3QFN-RLX0041A


0
126
41
MRS_QFN
DFN-6_2x2mm_EP


0
7
7
MRS_QFN
LQFP-64_10x10mm_P0.5mm
64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)
QFP 0.5
0
64
64
MRS_QFN
QFN-24


0
38
25
MRS_QFN
QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm_ThermalVias
QFN, 36 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/36L_QFN_6x6_with_3_7x3_7_EP_Punch_Dimpled_4E_C04-0241A.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
63
37
MRS_QFN
QFN-FCMOD-9


0
20
9
MRS_QFN
QFN_16-4x4mm


0
22
17
MRS_QFN
QFN_28-4x4mm
QFN, 28 Pin (http://www.st.com/resource/en/datasheet/stm32f031k6.pdf (Page 280)), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
28
28
MRS_QFN
QFN_32-5x5mm


0
33
33
MRS_QFN
VQFN100_12x12mm


0
137
101
MRS_QFN
WQFN-16_3x3mm


0
26
17
MRS_QFP
LQFP-32_7x7mm_P0.8mm
LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
32
32
MRS_QFP
LQFP-48_7x7mm_P0.5mm
LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
48
48
MRS_QFP
LQFP-64_10x10mm_P0.5mm
64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)
QFP 0.5
0
64
64
MRS_QFP
LQFP-100_14x14mm_P0.5mm
LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)
QFP 0.5
0
100
100
MRS_QFP
LQFP-144_20x20mm_P0.5mm
144-Lead Plastic Low Profile Quad Flatpack (PL) - 20x20x1.40 mm Body [LQFP], 2.00 mm Footprint (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.5
0
144
144
MRS_RF
XBEE-LONGPAD
DIGI XBEE AND XBEE-PRO RF MODULES (LONG PADS)
DIGI XBEE AND XBEE-PRO RF MODULES (LONG PADS)
0
20
20
MRS_SO
Diodes_SO-8EP
8-Lead Plastic SO, Exposed Die Pad (see https://www.diodes.com/assets/Package-Files/SO-8EP.pdf)
SO exposed pad
0
9
9
MRS_SO
PowerPAK_SO-8_Single
PowerPAK SO-8 Single (https://www.vishay.com/docs/71655/powerpak.pdf, https://www.vishay.com/docs/72599/72599.pdf)
PowerPAK SO-8 Single
0
9
5
MRS_SO
SOIC-8
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)
SOIC 1.27
0
8
8
MRS_SO
SOIC-14
14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)
SOIC 1.27
0
14
14
MRS_SO
TSSOP-16


0
16
16
MRS_SO
TSSOP-20_4.4x6.5mm_P0.65mm
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
20
20
MRS_SO
Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias
Texas Instruments HSOP 9, 1.27mm pitch, 3.9x4.9mm body, exposed pad, thermal vias, DDA0008J (http://www.ti.com/lit/ds/symlink/tps5430.pdf)
HSOP 1.27
0
20
9
MRS_SO
VSSOP-8_3.0x3.0mm_P0.65mm
VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf
VSSOP-8 3.0 x 3.0
0
8
8
MRS_SON
VSON-8_3.3x3.3mm_P0.65mm_NexFET
8-Lead Plastic Dual Flat, No Lead Package (MF) - 3.3x3.3x1 mm Body [VSON] http://www.ti.com/lit/ds/symlink/csd87334q3d.pdf
VSON 0.65
0
12
5
MRS_SON
WSON12_3x3mm


0
17
13
MRS_SOT
SOT-23


0
3
3
MRS_SOT
SOT-23-5
6-pin SOT-23 package
SOT-23-6
0
5
5
MRS_SOT
SOT-23-6
6-pin SOT-23 package
SOT-23-6
0
6
6
MRS_SOT
SOT-26-6


0
6
6
MRS_SOT
SOT-89


0
4
3
MRS_SOT
SOT-223-3(TAB-pin-2)
module CMS SOT223 4 pins
CMS SOT
0
4
3
MRS_SOT
SOT-323_SC-70
SOT-323, SC-70
SOT-323 SC-70
0
3
3
MRS_SOT
SOT-363-6
SOT-363, SC-70-6
SOT-363 SC-70-6
0
6
6
MRS_SOT
SOT−563-6


0
6
6
MRS_Sensors
ACS72981xLR


0
7
7
MRS_Sensors
APDS-9300-020


0
6
6
MRS_Sensors
MRS_MODULE_BIG


0
13
11
MRS_Sensors
MRS_MODULE_MEDIUM


0
12
11
MRS_Sensors
MRS_MODULE_SMALL


0
12
11
MRS_Sensors
SCD30


0
7
7
MRS_Sensors
SHT31


0
9
9
MRS_Switches
Buzzer_CMI-9655S-SMT-TR


0
2
2
MRS_Switches
Buzzer_PK12N40PETQ


0
2
2
MRS_Switches
Tactile_Switch_6x6_SMT


0
4
2
MRS_Switches
Tactile_Switch_12x12_THT


0
4
2
MRS_Switches
Tactile_Switch_SMT_4,2x2,8mm


0
4
2
MRS_Switches
Tactile_Switch_TL3300


0
4
2
MRS_TO
TO-252-2(DPAK)


0
3
3
MRS_TO
TO-263-2(D2PAK)


0
3
3
MRS_TO
TO-263-5_TabPin3
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
10
5
MRS_TO
TO-277-3


0
3
2
MRS_TO
TO-PMOD-11


0
12
12
MRS_Transistors
AO DFN5x6_8L_EP1_P


0
9
3
MRS_Transistors
AO_DFN5x6-8L-EP1-P
http://www.aosmd.com/res/packaging_information/DFN5x6_8L_EP1_P.pdf

0
9
3
MRS_XTALs
ABM8G


0
4
4
MRS_XTALs
CSM-8M


0
4
4
Package_SO
Diodes_PSOP-8
8-Lead Plastic PSOP, Exposed Die Pad (see https://www.diodes.com/assets/Datasheets/AP2204.pdf)
SSOP 0.50 exposed pad
0
12
9
Package_SO
Diodes_SO-8EP
8-Lead Plastic SO, Exposed Die Pad (see https://www.diodes.com/assets/Package-Files/SO-8EP.pdf)
SO exposed pad
0
9
9
Package_SO
ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body with Exposed Pad [eTSSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
27
21
Package_SO
HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.3x2.3mm
HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l7980.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
13
9
Package_SO
HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.3x2.3mm_ThermalVias
HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l7980.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
18
9
Package_SO
HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm
HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l5973d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
13
9
Package_SO
HSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.1mm_ThermalVias
HSOP, 8 Pin (https://www.st.com/resource/en/datasheet/l5973d.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
20
9
Package_SO
HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown
HSOP 11.0x15.9mm Pitch 1.27mm Slug Down (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 1.27mm
0
23
21
Package_SO
HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugDown_ThermalVias
HSOP 11.0x15.9mm Pitch 1.27mm Slug Down Thermal Vias (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 1.27mm
0
45
21
Package_SO
HSOP-20-1EP_11.0x15.9mm_P1.27mm_SlugUp
HSOP 11.0x15.9mm Pitch 1.27mm Slug Up (PowerSO-20) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/tda7266d.pdf, www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 1.27mm
0
20
20
Package_SO
HSOP-32-1EP_7.5x11mm_P0.65mm_EP4.7x4.7mm
HSOP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT1746-3.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
37
33
Package_SO
HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown
HSOP 11.0x15.9mm Pitch 0.65mm Slug Down (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 0.65mm
0
39
37
Package_SO
HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugDown_ThermalVias
HSOP 11.0x15.9mm Pitch 0.65mm Slug Down Thermal Vias (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 0.65mm
0
61
37
Package_SO
HSOP-36-1EP_11.0x15.9mm_P0.65mm_SlugUp
HSOP 11.0x15.9mm Pitch 0.65mm Slug Up (PowerSO-36) [JEDEC MO-166] (http://www.st.com/resource/en/datasheet/vn808cm-32-e.pdf, http://www.st.com/resource/en/application_note/cd00003801.pdf)
HSOP 11.0 x 15.9mm Pitch 0.65mm
0
36
36
Package_SO
HSOP-54-1EP_7.5x17.9mm_P0.65mm_EP4.6x4.6mm
HSOP, 54 Pin (https://www.nxp.com/docs/en/package-information/98ASA10506D.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOP SO
0
59
55
Package_SO
HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm
HTSOP, 8 Pin (https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSOP SO
0
13
9
Package_SO
HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm_ThermalVias
HTSOP, 8 Pin (https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSOP SO
0
20
9
Package_SO
HTSSOP-14-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3.1mm
HTSSOP, 14 Pin (http://www.ti.com/lit/ds/symlink/lm5161.pdf#page=34), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
20
15
Package_SO
HTSSOP-14-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3.1mm_ThermalVias
HTSSOP, 14 Pin (http://www.ti.com/lit/ds/symlink/lm5161.pdf#page=34), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
36
15
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm
16-Lead Plastic HTSSOP (4.4x5x1.2mm); Thermal pad; (http://www.ti.com/lit/ds/symlink/drv8833.pdf)
SSOP 0.65
0
29
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm
HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
20
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm_ThermalVias
HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
27
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask3x3mm_ThermalVias
16-Lead Plastic HTSSOP (4.4x5x1.2mm); Thermal pad with vias; (http://www.ti.com/lit/ds/symlink/drv8800.pdf)
SSOP 0.65
0
46
17
Package_SO
HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm
HTSSOP, 16 Pin (https://www.st.com/resource/en/datasheet/stp08cp05.pdf#page=20), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
21
17
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.74x3.86mm
HTSSOP, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4011fb.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
23
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP2.85x4mm
HTSSOP, 20 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF U20E-1), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
23
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias
HTSSOP 0.65
0
29
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.4x3.7mm
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/bq24006.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
24
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=37&zoom=160,-90,3), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
26
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm_ThermalVias
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=37&zoom=160,-90,3), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
42
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.75x3.43mm_ThermalVias_HandSolder
HTSSOP, 20 Pin (http://www.ti.com/lit/ds/symlink/tlc5971.pdf#page=37&zoom=160,-90,3), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
42
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.96x2.96mm
HTSSOP, 20 Pin (https://www.ti.com/lit/ds/symlink/tps2663.pdf#page=49), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
23
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_Mask2.96x2.96mm_ThermalVias
HTSSOP, 20 Pin (https://www.ti.com/lit/ds/symlink/tps2663.pdf#page=49), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
42
21
Package_SO
HTSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3.4x6.5mm_ThermalVias
20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [HTSSOP], with thermal pad with vias
HTSSOP 0.65
0
45
21
Package_SO
HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm
HTSSOP, 24 Pin (https://www.st.com/resource/en/datasheet/stp16cp05.pdf#page=25), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
31
25
Package_SO
HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm
HTSSOP, 24 Pin (http://www.ti.com/lit/ds/symlink/tps703.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
28
25
Package_SO
HTSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.4x7.8mm_Mask2.4x4.68mm_ThermalVias
HTSSOP, 24 Pin (http://www.ti.com/lit/ds/symlink/tps703.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
47
25
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm
HTSSOP, 28 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
30
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x5.4mm_ThermalVias
HTSSOP, 28 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
41
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
39
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
40
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_Mask2.4x6.17mm_ThermalVias
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
55
29
Package_SO
HTSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP3.4x9.5mm_ThermalVias
HTSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; thermal pad
TSSOP HTSSOP 0.65 thermal pad
0
58
29
Package_SO
HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm
HTSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)
SSOP 0.65 PowerPAD
0
43
33
Package_SO
HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm_ThermalVias
HTSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)
SSOP 0.65 PowerPAD
0
83
33
Package_SO
HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm
HTSSOP, 38 Pin (http://www.ti.com/lit/ds/symlink/tlc5951.pdf#page=47&zoom=140,-67,15), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
46
39
Package_SO
HTSSOP-38-1EP_6.1x12.5mm_P0.65mm_EP5.2x12.5mm_Mask3.39x6.35mm_ThermalVias
HTSSOP, 38 Pin (http://www.ti.com/lit/ds/symlink/tlc5951.pdf#page=47&zoom=140,-67,15), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
87
39
Package_SO
HTSSOP-44_6.1x14mm_P0.635mm_TopEP4.14x7.01mm
HTSSOP, 44 Pin (http://www.ti.com/lit/ds/symlink/tpa3251.pdf#page=38), generated with kicad-footprint-generator ipc_gullwing_generator.py
HTSSOP SO
0
44
44
Package_SO
HTSSOP-56-1EP_6.1x14mm_P0.5mm_EP3.61x6.35mm
HTSSOP56: plastic thin shrink small outline package http://www.ti.com/lit/ds/symlink/drv8301.pdf
HTSSOP 0.5
0
72
57
Package_SO
HVSSOP-10-1EP_3x3mm_P0.5mm_EP1.57x1.88mm
HVSSOP, 10 Pin (https://www.ti.com/lit/ds/symlink/bq24090.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HVSSOP SO
0
15
11
Package_SO
HVSSOP-10-1EP_3x3mm_P0.5mm_EP1.57x1.88mm_ThermalVias
HVSSOP, 10 Pin (https://www.ti.com/lit/ds/symlink/bq24090.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HVSSOP SO
0
20
11
Package_SO
Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm
Infineon  PG-DSO, 8 Pin (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-8-27), generated with kicad-footprint-generator ipc_gullwing_generator.py
Infineon PG-DSO SO
0
13
9
Package_SO
Infineon_PG-DSO-8-27_3.9x4.9mm_EP2.65x3mm_ThermalVias
Infineon  PG-DSO, 8 Pin (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-8-27), generated with kicad-footprint-generator ipc_gullwing_generator.py
Infineon PG-DSO SO
0
23
9
Package_SO
Infineon_PG-DSO-8-43
Infineon_PG-DSO-8-43
DSO DSO-8 SOIC SOIC-8
0
12
9
Package_SO
Infineon_PG-DSO-12-9
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-9/)
PG-DSO
0
23
13
Package_SO
Infineon_PG-DSO-12-9_ThermalVias
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-9/)
PG-DSO
0
42
13
Package_SO
Infineon_PG-DSO-12-11
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-11/)
PG-DSO
0
23
13
Package_SO
Infineon_PG-DSO-12-11_ThermalVias
Infineon PG-DSO 12 pin, exposed pad: 4.5x8.1mm, with thermal vias (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-12-11/)
PG-DSO
0
42
13
Package_SO
Infineon_PG-DSO-20-30
Infineon SO package 20pin, exposed pad 4.5x7mm (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-71/)
DSO-20
0
31
21
Package_SO
Infineon_PG-DSO-20-30_ThermalVias
Infineon SO package 20pin, exposed pad 4.5x7mm (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-71/)
DSO-20
0
45
21
Package_SO
Infineon_PG-DSO-20-32
Infineon SO package 20pin without exposed pad (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-32/)
DSO-20
0
20
20
Package_SO
Infineon_PG-DSO-20-85
Infineon SO package 20pin with exposed pad (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-85/)
DSO-20
0
31
21
Package_SO
Infineon_PG-DSO-20-85_ThermalVias
Infineon SO package 20pin with exposed pad (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-85/)
DSO-20
0
113
21
Package_SO
Infineon_PG-DSO-20-87
Infineon SO package 20pin without exposed pad (https://www.infineon.com/cms/en/product/packages/PG-DSO/PG-DSO-20-87/)
DSO-20
0
20
20
Package_SO
Infineon_PG-TSDSO-14-22
Infineon_PG-TSDSO-14-22
Infineon TSDSO 14-22 
0
17
15
Package_SO
Linear_MSOP-12-16-1EP_3x4mm_P0.5mm
12-Lead Plastic Micro Small Outline Package (MS) [MSOP], variant of MSOP-16 (see http://cds.linear.com/docs/en/datasheet/3630fd.pdf)
SSOP 0.5
0
15
13
Package_SO
Linear_MSOP-12-16_3x4mm_P0.5mm
12-Lead Plastic Micro Small Outline Package (MS) [MSOP], variant of MSOP-16 (see https://www.analog.com/media/en/technical-documentation/data-sheets/3748fb.pdf)
SSOP 0.5
0
12
12
Package_SO
MFSOP6-4_4.4x3.6mm_P1.27mm
https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.4pin%20MFSOP6.html
MFSOP 4 pin SMD
0
4
4
Package_SO
MFSOP6-5_4.4x3.6mm_P1.27mm
https://toshiba.semicon-storage.com/ap-en/design-support/package/detail.5pin%20MFSOP6.html
MFSOP 4 pin SMD
0
5
5
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm
MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
13
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm_ThermalVias
MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
18
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm
MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
13
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.73x1.85mm_ThermalVias
MSOP, 8 Pin (http://www.ti.com/lit/ds/symlink/lm25085.pdf#page=32), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
18
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.95x2.15mm
MSOP, 8 Pin (http://www.st.com/resource/en/datasheet/pm8834.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
13
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP1.95x2.15mm_ThermalVias
MSOP, 8 Pin (http://www.st.com/resource/en/datasheet/pm8834.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
18
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm
MSOP, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf#page=15), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
14
9
Package_SO
MSOP-8-1EP_3x3mm_P0.65mm_EP2.5x3mm_Mask1.73x2.36mm_ThermalVias
MSOP, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/mic5355_6.pdf#page=15), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
19
9
Package_SO
MSOP-8_3x3mm_P0.65mm
MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
8
8
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
15
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm_ThermalVias
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
20
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.73x1.98mm
MSOP, 10 Pin (www.allegromicro.com/~/media/Files/Datasheets/A4952-3-Datasheet.ashx?la=en#page=10), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
15
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.73x1.98mm_ThermalVias
MSOP, 10 Pin (www.allegromicro.com/~/media/Files/Datasheets/A4952-3-Datasheet.ashx?la=en#page=10), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
20
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP2.2x3.1mm_Mask1.83x1.89mm
MSOP, 10 Pin (https://www.ti.com/lit/ds/symlink/xtr111.pdf#page=27), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
16
11
Package_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP2.2x3.1mm_Mask1.83x1.89mm_ThermalVias
MSOP, 10 Pin (https://www.ti.com/lit/ds/symlink/xtr111.pdf#page=27), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
23
11
Package_SO
MSOP-10_3x3mm_P0.5mm
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
10
10
Package_SO
MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm
MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
17
13
Package_SO
MSOP-12-1EP_3x4mm_P0.65mm_EP1.65x2.85mm_ThermalVias
MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3652fe.pdf#page=24), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
24
13
Package_SO
MSOP-12-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
19
13
Package_SO
MSOP-12-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm_ThermalVias
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
25
13
Package_SO
MSOP-12-16_3x4mm_P0.5mm
10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.5
0
12
12
Package_SO
MSOP-12_3x4mm_P0.65mm
MSOP, 12 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf#page=36), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
12
12
Package_SO
MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm
MSOP, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081667_F_MSE16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
21
17
Package_SO
MSOP-16-1EP_3x4.039mm_P0.5mm_EP1.651x2.845mm_ThermalVias
MSOP, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081667_F_MSE16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
28
17
Package_SO
MSOP-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm
MSOP, 16 Pin (http://cds.linear.com/docs/en/datasheet/37551fd.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
21
17
Package_SO
MSOP-16-1EP_3x4mm_P0.5mm_EP1.65x2.85mm_ThermalVias
MSOP, 16 Pin (http://cds.linear.com/docs/en/datasheet/37551fd.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
28
17
Package_SO
MSOP-16_3x4.039mm_P0.5mm
MSOP, 16 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-msop/05081669_A_MS16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
16
16
Package_SO
MSOP-16_3x4mm_P0.5mm
MSOP, 16 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/436412f.pdf#page=22), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
16
16
Package_SO
ONSemi_SO-8FL_488AA
ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A https://www.onsemi.com/pub/Collateral/488AA.PDF
ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A 
0
5
5
Package_SO
OnSemi_Micro8
ON Semiconductor Micro8 (Case846A-02): https://www.onsemi.com/pub/Collateral/846A-02.PDF
micro8
0
8
8
Package_SO
PSOP-44_16.9x27.17mm_P1.27mm
PSOP44: plastic thin shrink small outline package; 44 leads; body width 16.90 mm
PSOP 1.27
0
44
44
Package_SO
PowerIntegrations_SO-8
Power-Integrations variant of 8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], see https://ac-dc.power.com/sites/default/files/product-docs/senzero_family_datasheet.pdf
SOIC 1.27
0
8
8
Package_SO
PowerIntegrations_SO-8B
Power-Integrations variant of 8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], see https://www.mouser.com/ds/2/328/linkswitch-pl_family_datasheet-12517.pdf
SOIC 1.27
0
7
7
Package_SO
PowerIntegrations_SO-8C
Power-Integrations variant of 8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], see https://www.mouser.com/ds/2/328/linkswitch-pl_family_datasheet-12517.pdf
SOIC 1.27
0
7
7
Package_SO
PowerIntegrations_eSOP-12B
eSOP-12B SMT Flat Package with Heatsink Tab, see https://ac-dc.power.com/sites/default/files/product-docs/topswitch-jx_family_datasheet.pdf
Power Integrations K Package
0
12
12
Package_SO
PowerPAK_SO-8_Dual
PowerPAK SO-8 Dual (https://www.vishay.com/docs/71655/powerpak.pdf, https://www.vishay.com/docs/72600/72600.pdf)
PowerPAK SO-8 Dual
0
10
6
Package_SO
PowerPAK_SO-8_Single
PowerPAK SO-8 Single (https://www.vishay.com/docs/71655/powerpak.pdf, https://www.vishay.com/docs/72599/72599.pdf)
PowerPAK SO-8 Single
0
9
5
Package_SO
QSOP-16_3.9x4.9mm_P0.635mm
16-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150" Body [QSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.635
0
16
16
Package_SO
QSOP-20_3.9x8.7mm_P0.635mm
20-Lead Plastic Shrink Small Outline Narrow Body (http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf)
QSOP 0.635
0
20
20
Package_SO
QSOP-24_3.9x8.7mm_P0.635mm
24-Lead Plastic Shrink Small Outline Narrow Body (QR)-.150" Body [QSOP] (see Microchip Packaging Specification 00000049CH.pdf)
QSOP 0.635
0
24
24
Package_SO
SC-74-6_1.5x2.9mm_P0.95mm
SC-74, 6 Pin (https://www.nxp.com/docs/en/package-information/SOT457.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SC-74 SO
0
6
6
Package_SO
SO-4_4.4x2.3mm_P1.27mm
4-Lead Plastic Small Outline (SO), see http://datasheet.octopart.com/OPIA403BTRE-Optek-datasheet-5328560.pdf
SO SOIC 1.27
0
4
4
Package_SO
SO-4_4.4x3.6mm_P2.54mm
4-Lead Plastic Small Outline (SO), see https://www.elpro.org/de/index.php?controller=attachment&id_attachment=339
SO SOIC 2.54
0
4
4
Package_SO
SO-4_4.4x3.9mm_P2.54mm
SO, 4 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=10047&prodName=TLP3123), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
4
4
Package_SO
SO-4_4.4x4.3mm_P2.54mm
4-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/docs/AV02-0173EN
SO SOIC 2.54
0
4
4
Package_SO
SO-4_7.6x3.6mm_P2.54mm
4-Lead Plastic Small Outline (SO) (http://www.everlight.com/file/ProductFile/201407061745083848.pdf)
SO SOIC 2.54
0
4
4
Package_SO
SO-5_4.4x3.6mm_P1.27mm
5-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SO SOIC 1.27
0
5
5
Package_SO
SO-6L_10x3.84mm_P1.27mm
6-pin plasic small outline 7,5mm long https://toshiba.semicon-storage.com/info/docget.jsp?did=53548&prodName=TLP2770
SO-6L
0
6
6
Package_SO
SO-6_4.4x3.6mm_P1.27mm
6-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SO SOIC 1.27
0
6
6
Package_SO
SO-8_3.9x4.9mm_P1.27mm
SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
8
8
Package_SO
SO-8_5.3x6.2mm_P1.27mm
SO, 8 Pin (https://www.ti.com/lit/ml/msop001a/msop001a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
8
8
Package_SO
SO-14_3.9x8.65mm_P1.27mm
SO, 14 Pin (https://www.st.com/resource/en/datasheet/l6491.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
14
14
Package_SO
SO-14_5.3x10.2mm_P1.27mm
SO, 14 Pin (https://www.ti.com/lit/ml/msop002a/msop002a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
14
14
Package_SO
SO-16_3.9x9.9mm_P1.27mm
SO, 16 Pin (https://www.nxp.com/docs/en/package-information/SOT109-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
16
16
Package_SO
SO-16_5.3x10.2mm_P1.27mm
SO, 16 Pin (https://www.ti.com/lit/ml/msop002a/msop002a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
16
16
Package_SO
SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm
SO, 20 Pin (http://www.ti.com/lit/ds/symlink/opa569.pdf, http://www.ti.com/lit/an/slma004b/slma004b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
23
21
Package_SO
SO-20-1EP_7.52x12.825mm_P1.27mm_EP6.045x12.09mm_Mask3.56x4.47mm_ThermalVias
SO, 20 Pin (http://www.ti.com/lit/ds/symlink/opa569.pdf, http://www.ti.com/lit/an/slma004b/slma004b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
51
21
Package_SO
SO-20_5.3x12.6mm_P1.27mm
SO, 20 Pin (https://www.ti.com/lit/ml/msop002a/msop002a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
20
20
Package_SO
SO-20_12.8x7.5mm_P1.27mm
SO-20, 12.8x7.5mm, https://www.nxp.com/docs/en/data-sheet/SA605.pdf
S0-20 
0
20
20
Package_SO
SO-24_5.3x15mm_P1.27mm
SO, 24 Pin (https://www.ti.com/lit/ml/msop002a/msop002a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SO SO
0
24
24
Package_SO
SOIC-4_4.55x2.6mm_P1.27mm
SOIC, 4 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12884&prodName=TLP291), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
4
4
Package_SO
SOIC-4_4.55x3.7mm_P2.54mm
SOIC, 6 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=11791&prodName=TLP185), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
4
4
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm_ThermalVias
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm
SOIC, 8 Pin (http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx#page=8), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.3mm_ThermalVias
SOIC, 8 Pin (http://www.allegromicro.com/~/media/Files/Datasheets/A4950-Datasheet.ashx#page=8), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.81mm
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.41x3.81mm_ThermalVias
SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm
SOIC, 8 Pin (https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP2303A/document_id/494#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.62x3.51mm_ThermalVias
SOIC, 8 Pin (https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP2303A/document_id/494#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm
SOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lm5017.pdf#page=31), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm_ThermalVias
SOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lm5017.pdf#page=31), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
23
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm
SOIC, 8 Pin (https://www.renesas.com/eu/en/www/doc/datasheet/hip2100.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
13
9
Package_SO
SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.514x3.2mm_ThermalVias
SOIC, 8 Pin (https://www.renesas.com/eu/en/www/doc/datasheet/hip2100.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
9
Package_SO
SOIC-8-N7_3.9x4.9mm_P1.27mm
8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC], pin 7 removed (Microchip Packaging Specification 00000049BS.pdf, http://www.onsemi.com/pub/Collateral/NCP1207B.PDF)
SOIC 1.27
0
7
7
Package_SO
SOIC-8W_5.3x5.3mm_P1.27mm
8-Lead Plastic Small Outline (SM) - 5.28 mm Body [SOIC] (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)
SOIC 1.27
0
8
8
Package_SO
SOIC-8_3.9x4.9mm_P1.27mm
SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-8_5.23x5.23mm_P1.27mm
SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-8_5.275x5.275mm_P1.27mm
SOIC, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-8_7.5x5.85mm_P1.27mm
SOIC, 8 Pin (http://www.ti.com/lit/ml/mpds382b/mpds382b.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
Package_SO
SOIC-14-16_3.9x9.9mm_P1.27mm
SOIC, 16 Pin package with pin 2 and 13 removed for voltage clearance  (UCC256301, https://www.ti.com/lit/ds/symlink/ucc256301.pdf)
SOIC SO
0
14
14
Package_SO
SOIC-14W_7.5x9mm_P1.27mm
SOIC, 14 Pin (JEDEC MS-013AF, https://www.analog.com/media/en/package-pcb-resources/package/54614177245586rw_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
14
Package_SO
SOIC-14_3.9x8.7mm_P1.27mm
SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
14
14
Package_SO
SOIC-16W-12_7.5x10.3mm_P1.27mm
SOIC-16 With 12 Pin Placed - Wide, 7.50 mm Body [SOIC] (https://docs.broadcom.com/docs/AV02-0169EN)
SOIC 1.27 16 12 Wide
0
12
12
Package_SO
SOIC-16W_5.3x10.2mm_P1.27mm
16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)
SOIC 1.27
0
16
16
Package_SO
SOIC-16W_7.5x10.3mm_P1.27mm
SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-16W_7.5x12.8mm_P1.27mm
SOIC, 16 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ri_soic_ic/ri_16_1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-16_3.9x9.9mm_P1.27mm
SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-16_4.55x10.3mm_P1.27mm
SOIC, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
16
16
Package_SO
SOIC-18W_7.5x11.6mm_P1.27mm
SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
18
18
Package_SO
SOIC-20W_7.5x12.8mm_P1.27mm
SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
20
Package_SO
SOIC-20W_7.5x15.4mm_P1.27mm
SOIC, 20 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RI_20_1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
20
20
Package_SO
SOIC-24W_7.5x15.4mm_P1.27mm
SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
24
24
Package_SO
SOIC-28W_7.5x17.9mm_P1.27mm
SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
28
28
Package_SO
SOIC-28W_7.5x18.7mm_P1.27mm
SOIC, 28 Pin (https://www.akm.com/akm/en/file/datasheet/AK5394AVS.pdf#page=23), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
28
28
Package_SO
SOJ-36_10.16x23.49mm_P1.27mm
SOJ, 36 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOJ SO
0
36
36
Package_SO
SOP-4_3.8x4.1mm_P2.54mm
SOP, 4 Pin (http://www.ixysic.com/home/pdfs.nsf/www/CPC1017N.pdf/$file/CPC1017N.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
4
4
Package_SO
SOP-4_4.4x2.6mm_P1.27mm
SOP, 4 Pin (http://www.vishay.com/docs/83510/tcmt1100.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
4
4
Package_SO
SOP-8-1EP_4.57x4.57mm_P1.27mm_EP4.57x4.45mm
SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX112.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
13
9
Package_SO
SOP-8-1EP_4.57x4.57mm_P1.27mm_EP4.57x4.45mm_ThermalVias
SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX112.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
20
9
Package_SO
SOP-8_3.9x4.9mm_P1.27mm
SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-8_3.76x4.96mm_P1.27mm
SOP, 8 Pin (https://ww2.minicircuits.com/case_style/XX211.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-8_5.28x5.23mm_P1.27mm
SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=80), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-8_6.62x9.15mm_P2.54mm
SOP, 8 Pin (http://www.ti.com/lit/ds/symlink/iso1050.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
8
8
Package_SO
SOP-16_3.9x9.9mm_P1.27mm
SOP, 16 Pin (https://www.diodes.com/assets/Datasheets/PAM8403.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
16
16
Package_SO
SOP-16_4.4x10.4mm_P1.27mm
16-Lead Plastic Small Outline http://www.vishay.com/docs/49633/sg2098.pdf
SOP 1.27
0
16
16
Package_SO
SOP-16_4.55x10.3mm_P1.27mm
SOP, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12855&prodName=TLP290-4), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
16
16
Package_SO
SOP-18_7x12.5mm_P1.27mm
SOP, 18 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=30523), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
18
18
Package_SO
SOP-20_7.5x12.8mm_P1.27mm
SOP, 20 Pin (https://www.holtek.com/documents/10179/116723/sop20-300.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
20
20
Package_SO
SOP-24_7.5x15.4mm_P1.27mm
SOP, 24 Pin (http://www.issi.com/WW/pdf/31FL3218.pdf#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOP SO
0
24
24
Package_SO
SSO-4_6.7x5.1mm_P2.54mm_Clearance8mm
4-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://www.vishay.com/docs/84299/vor1142b4.pdf
SSO Stretched SO SOIC 2.54
0
4
4
Package_SO
SSO-6_6.8x4.6mm_P1.27mm_Clearance7mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC 1.27
0
6
6
Package_SO
SSO-6_6.8x4.6mm_P1.27mm_Clearance8mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC 1.27
0
6
6
Package_SO
SSO-7-8_6.4x9.78mm_P2.54mm
SSO, 7 Pin (https://b2b-api.panasonic.eu/file_stream/pids/fileversion/2787), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSO SO
0
7
7
Package_SO
SSO-8_6.7x9.8mm_P2.54mm_Clearance8mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://www.vishay.com/docs/83831/lh1533ab.pdf
SSO Stretched SO SOIC Pitch 2.54
0
8
8
Package_SO
SSO-8_6.8x5.9mm_P1.27mm_Clearance7mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSO-8_9.6x6.3mm_P1.27mm_Clearance10.5mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSO-8_13.6x6.3mm_P1.27mm_Clearance14.2mm
8-Lead Plastic Stretched Small Outline (SSO/Stretched SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true
SSO Stretched SO SOIC Pitch 1.27
0
8
8
Package_SO
SSOP-8_2.95x2.8mm_P0.65mm
SSOP-8 2.9 x2.8mm Pitch 0.65mm
SSOP-8 2.95x2.8mm Pitch 0.65mm
0
8
8
Package_SO
SSOP-8_3.9x5.05mm_P1.27mm
SSOP, 8 Pin (http://www.fujitsu.com/downloads/MICRO/fsa/pdf/products/memory/fram/MB85RS16-DS501-00014-6v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
8
8
Package_SO
SSOP-8_3.95x5.21x3.27mm_P1.27mm
SSOP-8 3.95x5.21x3.27mm Pitch 1.27mm
SSOP-8 3.95x5.21x3.27mm 1.27mm
0
8
8
Package_SO
SSOP-8_5.25x5.24mm_P1.27mm
SSOP, 8 Pin (http://www.fujitsu.com/ca/en/Images/MB85RS2MT-DS501-00023-1v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
8
8
Package_SO
SSOP-10_3.9x4.9mm_P1.00mm
10-Lead SSOP, 3.9 x 4.9mm body, 1.00mm pitch (http://www.st.com/resource/en/datasheet/viper01.pdf)
SSOP 3.9 4.9 1.00
0
10
10
Package_SO
SSOP-14_5.3x6.2mm_P0.65mm
SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)
SSOP 0.65
0
14
14
Package_SO
SSOP-16_3.9x4.9mm_P0.635mm
SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)
SSOP 0.635
0
16
16
Package_SO
SSOP-16_4.4x5.2mm_P0.65mm
SSOP16: plastic shrink small outline package; 16 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot369-1_po.pdf)
SSOP 0.65
0
16
16
Package_SO
SSOP-16_5.3x6.2mm_P0.65mm
SSOP, 16 Pin (https://assets.nexperia.com/documents/data-sheet/74HC_HCT165.pdf#page=14), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
16
16
Package_SO
SSOP-18_4.4x6.5mm_P0.65mm
SSOP18: plastic shrink small outline package; 18 leads; body width 4.4 mm (http://toshiba.semicon-storage.com/info/docget.jsp?did=30523&prodName=TBD62783APG)
SSOP 0.65
0
18
18
Package_SO
SSOP-20_3.9x8.7mm_P0.635mm
SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf)
SSOP 0.635
0
20
20
Package_SO
SSOP-20_4.4x6.5mm_P0.65mm
SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot266-1_po.pdf)
SSOP 0.65
0
20
20
Package_SO
SSOP-20_5.3x7.2mm_P0.65mm
SSOP, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001800C.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
20
20
Package_SO
SSOP-24_3.9x8.7mm_P0.635mm
SSOP24: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot556-1_po.pdf)
SSOP 0.635
0
24
24
Package_SO
SSOP-24_5.3x8.2mm_P0.65mm
24-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
24
24
Package_SO
SSOP-28_3.9x9.9mm_P0.635mm
SSOP28: plastic shrink small outline package; 28 leads; body width 3.9 mm; lead pitch 0.635; (see http://cds.linear.com/docs/en/datasheet/38901fb.pdf)
SSOP 0.635
0
28
28
Package_SO
SSOP-28_5.3x10.2mm_P0.65mm
28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
28
28
Package_SO
SSOP-32_11.305x20.495mm_P1.27mm
SSOP, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
32
32
Package_SO
SSOP-44_5.3x12.8mm_P0.5mm
44-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (http://cds.linear.com/docs/en/datasheet/680313fa.pdf)
SSOP 0.5
0
44
44
Package_SO
SSOP-48_5.3x12.8mm_P0.5mm
SSOP, 48 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-ssop/05081887_A_G48.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SSOP SO
0
48
48
Package_SO
SSOP-48_7.5x15.9mm_P0.635mm
SSOP48: plastic shrink small outline package; 48 leads; body width 7.5 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot370-1_po.pdf)
SSOP 0.635
0
48
48
Package_SO
SSOP-56_7.5x18.5mm_P0.635mm
SSOP56: plastic shrink small outline package; 56 leads; body width 7.5 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot371-1_po.pdf)
SSOP 0.635
0
56
56
Package_SO
STC_SOP-16_3.9x9.9mm_P1.27mm
STC  SOP, 16 Pin (https://www.stcmicro.com/datasheet/STC15F2K60S2-en.pdf#page=156), generated with kicad-footprint-generator ipc_gullwing_generator.py
STC SOP SO
0
16
16
Package_SO
ST_MultiPowerSO-30
MultiPowerSO-30 3EP 16.0x17.2mm Pitch 1mm (http://www.st.com/resource/en/datasheet/vnh2sp30-e.pdf)
MultiPowerSO-30 3EP 16.0x17.2mm Pitch 1mm
0
33
33
Package_SO
ST_PowerSSO-24_SlugDown
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7266p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm
0
25
25
Package_SO
ST_PowerSSO-24_SlugDown_ThermalVias
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7266p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm
0
38
25
Package_SO
ST_PowerSSO-24_SlugUp
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7266p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-24 1EP 7.5x10.3mm Pitch 0.8mm
0
24
24
Package_SO
ST_PowerSSO-36_SlugDown
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm
0
37
37
Package_SO
ST_PowerSSO-36_SlugDown_ThermalVias
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm
0
50
37
Package_SO
ST_PowerSSO-36_SlugUp
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm [JEDEC MO-271] (http://www.st.com/resource/en/datasheet/tda7492p.pdf, http://freedatasheets.com/downloads/Technical%20Note%20Powersso24%20TN0054.pdf)
ST PowerSSO-36 1EP 7.5x10.3mm Pitch 0.8mm
0
36
36
Package_SO
TI_SO-PowerPAD-8
8-Lead Plastic PSOP, Exposed Die Pad (TI DDA0008B, see http://www.ti.com/lit/ds/symlink/lm3404.pdf)
SSOP 0.50 exposed pad
0
12
9
Package_SO
TI_SO-PowerPAD-8_ThermalVias
8-pin HTSOP package with 1.27mm pin pitch, compatible with SOIC-8, 3.9x4.9mm² body, exposed pad, thermal vias with large copper area, as proposed in http://www.ti.com/lit/ds/symlink/tps5430.pdf
HTSOP 1.27
0
19
9
Package_SO
TSOP-5_1.65x3.05mm_P0.95mm
TSOP-5 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf
Jedec MO-193C TSOP-5L
0
5
5
Package_SO
TSOP-6_1.65x3.05mm_P0.95mm
TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf
Jedec MO-193C TSOP-6L
0
6
6
Package_SO
TSOP-I-24_12.4x6mm_P0.5mm
TSOP-I, 24 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation AA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
24
24
Package_SO
TSOP-I-24_14.4x6mm_P0.5mm
TSOP-I, 24 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation AB), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
24
24
Package_SO
TSOP-I-24_16.4x6mm_P0.5mm
TSOP-I, 24 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation AC), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
24
24
Package_SO
TSOP-I-24_18.4x6mm_P0.5mm
TSOP-I, 24 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation AD), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
24
24
Package_SO
TSOP-I-28_11.8x8mm_P0.55mm
TSOP I, 28 pins, 18.8x8mm body, 0.55mm pitch, IPC-calculated pads (http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf)
TSOP I 28 pins
0
28
28
Package_SO
TSOP-I-32_11.8x8mm_P0.5mm
TSOP-I, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
32
32
Package_SO
TSOP-I-32_12.4x8mm_P0.5mm
TSOP-I, 32 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation BA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
32
32
Package_SO
TSOP-I-32_14.4x8mm_P0.5mm
TSOP-I, 32 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation BB), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
32
32
Package_SO
TSOP-I-32_16.4x8mm_P0.5mm
TSOP-I, 32 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation BC), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
32
32
Package_SO
TSOP-I-32_18.4x8mm_P0.5mm
TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf, http://www.fujitsu.com/downloads/MICRO/fma/pdfmcu/f32pm25.pdf)
TSOP I 32
0
32
32
Package_SO
TSOP-I-32_18.4x8mm_P0.5mm_Reverse
TSOP I, 32 pins, 18.4x8mm body (http://www.futurlec.com/Datasheet/Memory/628128.pdf), reverse mount
TSOP I 32 reverse
0
32
32
Package_SO
TSOP-I-40_12.4x10mm_P0.5mm
TSOP-I, 40 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation CA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
40
40
Package_SO
TSOP-I-40_14.4x10mm_P0.5mm
TSOP-I, 40 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation CB), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
40
40
Package_SO
TSOP-I-40_16.4x10mm_P0.5mm
TSOP-I, 40 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation CC), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
40
40
Package_SO
TSOP-I-40_18.4x10mm_P0.5mm
TSOP-I, 40 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation CD), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
40
40
Package_SO
TSOP-I-48_12.4x12mm_P0.5mm
TSOP-I, 48 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation DA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
48
48
Package_SO
TSOP-I-48_14.4x12mm_P0.5mm
TSOP-I, 48 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation DB), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
48
48
Package_SO
TSOP-I-48_16.4x12mm_P0.5mm
TSOP-I, 48 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation DC), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
48
48
Package_SO
TSOP-I-48_18.4x12mm_P0.5mm
TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf)
TSOP I 32
0
48
48
Package_SO
TSOP-I-56_14.4x14mm_P0.5mm
TSOP-I, 56 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation EA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
56
56
Package_SO
TSOP-I-56_16.4x14mm_P0.5mm
TSOP-I, 56 Pin (https://www.jedec.org/standards-documents/docs/mo-142-d variation EB), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-I SO
0
56
56
Package_SO
TSOP-I-56_18.4x14mm_P0.5mm
TSOP I, 32 pins, 18.4x8mm body (https://www.micron.com/~/media/documents/products/technical-note/nor-flash/tn1225_land_pad_design.pdf)
TSOP I 32
0
56
56
Package_SO
TSOP-II-32_21.0x10.2mm_P1.27mm
32-lead plastic TSOP; Type II
TSOP-II 32
0
32
32
Package_SO
TSOP-II-44_10.16x18.41mm_P0.8mm
TSOP-II, 44 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOP-II SO
0
44
44
Package_SO
TSOP-II-54_22.2x10.16mm_P0.8mm
54-lead TSOP typ II package
TSOPII TSOP2
0
54
54
Package_SO
TSSOP-4_4.4x5mm_P4mm
TSSOP, 4 Pin (https://www.onsemi.com/pub/Collateral/MDB8S-D.PDF#page=4), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
4
4
Package_SO
TSSOP-8_3x3mm_P0.65mm
TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)
SSOP 0.65
0
8
8
Package_SO
TSSOP-8_4.4x3mm_P0.65mm
TSSOP, 8 Pin (JEDEC MO-153 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
8
8
Package_SO
TSSOP-10_3x3mm_P0.5mm
TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)
SSOP 0.5
0
10
10
Package_SO
TSSOP-14-1EP_4.4x5mm_P0.65mm
14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] with exposed pad (http://cds.linear.com/docs/en/datasheet/34301fa.pdf)
SSOP 0.65 exposed pad
0
18
15
Package_SO
TSSOP-14_4.4x5mm_P0.65mm
TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
14
14
Package_SO
TSSOP-16-1EP_4.4x5mm_P0.65mm
FE Package; 16-Lead Plastic TSSOP (4.4mm); Exposed Pad Variation BB; (see Linear Technology 1956f.pdf)
SSOP 0.65
0
24
17
Package_SO
TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm
TSSOP, 16 Pin (Allegro A4954 https://www.allegromicro.com/-/media/Files/Datasheets/A4954-Datasheet.ashx), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
21
17
Package_SO
TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm_ThermalVias
TSSOP, 16 Pin (Allegro A4954 https://www.allegromicro.com/-/media/Files/Datasheets/A4954-Datasheet.ashx), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
26
17
Package_SO
TSSOP-16_4.4x5mm_P0.65mm
TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
16
16
Package_SO
TSSOP-20_4.4x5mm_P0.5mm
TSSOP, 20 Pin (JEDEC MO-153 Var BA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
20
20
Package_SO
TSSOP-20_4.4x6.5mm_P0.65mm
TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
20
20
Package_SO
TSSOP-24-1EP_4.4x7.8mm_P0.65mm_EP3.2x5mm
TSSOP, 24 Pin (https://www.st.com/resource/en/datasheet/led1642gw.pdf#page=37), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
31
25
Package_SO
TSSOP-24_4.4x5mm_P0.4mm
TSSOP, 24 Pin (JEDEC MO-153 Var CA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
24
24
Package_SO
TSSOP-24_4.4x6.5mm_P0.5mm
TSSOP, 24 Pin (JEDEC MO-153 Var BB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
24
24
Package_SO
TSSOP-24_4.4x7.8mm_P0.65mm
TSSOP, 24 Pin (JEDEC MO-153 Var AD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
24
24
Package_SO
TSSOP-24_6.1x7.8mm_P0.65mm
TSSOP, 24 Pin (JEDEC MO-153 Var DA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
24
24
Package_SO
TSSOP-28-1EP_4.4x9.7mm_P0.65mm
TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; Exposed Pad Variation; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)
SSOP 0.65
0
36
29
Package_SO
TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x6.7mm
TSSOP, 28 Pin (JEDEC MO-153 Var AET Pkg.Code U28E-4 https://pdfserv.maximintegrated.com/package_dwgs/21-0108.PDF), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
35
29
Package_SO
TSSOP-28_4.4x7.8mm_P0.5mm
TSSOP, 28 Pin (JEDEC MO-153 Var BC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
28
28
Package_SO
TSSOP-28_4.4x9.7mm_P0.65mm
TSSOP, 28 Pin (JEDEC MO-153 Var AE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
28
28
Package_SO
TSSOP-28_6.1x7.8mm_P0.5mm
TSSOP, 28 Pin (JEDEC MO-153 Var EA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
28
28
Package_SO
TSSOP-28_6.1x9.7mm_P0.65mm
TSSOP, 28 Pin (JEDEC MO-153 Var DB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
28
28
Package_SO
TSSOP-28_8x9.7mm_P0.65mm
TSSOP, 28 Pin (JEDEC MO-153 Var GA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
28
28
Package_SO
TSSOP-30_4.4x7.8mm_P0.5mm
TSSOP, 30 Pin (JEDEC MO-153 Var BC-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
30
30
Package_SO
TSSOP-30_6.1x9.7mm_P0.65mm
TSSOP, 30 Pin (JEDEC MO-153 Var DB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
30
30
Package_SO
TSSOP-32_4.4x6.5mm_P0.4mm
TSSOP, 32 Pin (JEDEC MO-153 Var CB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
32
32
Package_SO
TSSOP-32_6.1x11mm_P0.65mm
TSSOP, 32 Pin (JEDEC MO-153 Var DC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
32
32
Package_SO
TSSOP-32_8x11mm_P0.65mm
TSSOP, 32 Pin (JEDEC MO-153 Var GB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
32
32
Package_SO
TSSOP-36_4.4x7.8mm_P0.4mm
TSSOP, 36 Pin (JEDEC MO-153 Var CC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-36_4.4x9.7mm_P0.5mm
TSSOP, 36 Pin (JEDEC MO-153 Var BD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-36_6.1x7.8mm_P0.4mm
TSSOP, 36 Pin (JEDEC MO-153 Var FA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-36_6.1x9.7mm_P0.5mm
TSSOP, 36 Pin (JEDEC MO-153 Var EB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-36_6.1x12.5mm_P0.65mm
TSSOP, 36 Pin (JEDEC MO-153 Var DD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-36_8x9.7mm_P0.5mm
TSSOP, 36 Pin (JEDEC MO-153 Var HA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-36_8x12.5mm_P0.65mm
TSSOP, 36 Pin (JEDEC MO-153 Var GC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
36
36
Package_SO
TSSOP-38_4.4x9.7mm_P0.5mm
TSSOP, 38 Pin (JEDEC MO-153 Var BD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
38
38
Package_SO
TSSOP-38_6.1x12.5mm_P0.65mm
TSSOP, 38 Pin (JEDEC MO-153 Var DD-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
38
38
Package_SO
TSSOP-40_6.1x11mm_P0.5mm
TSSOP, 40 Pin (JEDEC MO-153 Var EC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
40
40
Package_SO
TSSOP-40_6.1x14mm_P0.65mm
TSSOP, 40 Pin (JEDEC MO-153 Var DE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
40
40
Package_SO
TSSOP-40_8x11mm_P0.5mm
TSSOP, 40 Pin (JEDEC MO-153 Var HB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
40
40
Package_SO
TSSOP-40_8x14mm_P0.65mm
TSSOP, 40 Pin (JEDEC MO-153 Var GD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
40
40
Package_SO
TSSOP-44_4.4x11.2mm_P0.5mm
TSSOP44: plastic thin shrink small outline package; 44 leads; body width 4.4 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot510-1_po.pdf)
SSOP 0.5
0
44
44
Package_SO
TSSOP-44_4.4x11mm_P0.5mm
TSSOP, 44 Pin (JEDEC MO-153 Var BE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
44
44
Package_SO
TSSOP-44_6.1x11mm_P0.5mm
TSSOP, 44 Pin (JEDEC MO-153 Var EC-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
44
44
Package_SO
TSSOP-48_4.4x9.7mm_P0.4mm
TSSOP, 48 Pin (JEDEC MO-153 Var CD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
48
48
Package_SO
TSSOP-48_6.1x9.7mm_P0.4mm
TSSOP, 48 Pin (JEDEC MO-153 Var FB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
48
48
Package_SO
TSSOP-48_6.1x12.5mm_P0.5mm
TSSOP, 48 Pin (JEDEC MO-153 Var ED https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
48
48
Package_SO
TSSOP-48_8x9.7mm_P0.4mm
TSSOP, 48 Pin (JEDEC MO-153 Var JA https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
48
48
Package_SO
TSSOP-48_8x12.5mm_P0.5mm
TSSOP, 48 Pin (JEDEC MO-153 Var HC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
48
48
Package_SO
TSSOP-50_4.4x12.5mm_P0.5mm
TSSOP, 50 Pin (JEDEC MO-153 Var BF https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
50
50
Package_SO
TSSOP-52_6.1x11mm_P0.4mm
TSSOP, 52 Pin (JEDEC MO-153 Var FC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
52
52
Package_SO
TSSOP-52_8x11mm_P0.4mm
TSSOP, 52 Pin (JEDEC MO-153 Var JB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
52
52
Package_SO
TSSOP-56_6.1x12.5mm_P0.4mm
TSSOP, 56 Pin (JEDEC MO-153 Var FD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
56
56
Package_SO
TSSOP-56_6.1x14mm_P0.5mm
TSSOP, 56 Pin (JEDEC MO-153 Var EE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
56
56
Package_SO
TSSOP-56_8x12.5mm_P0.4mm
TSSOP, 56 Pin (JEDEC MO-153 Var JC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
56
56
Package_SO
TSSOP-56_8x14mm_P0.5mm
TSSOP, 56 Pin (JEDEC MO-153 Var HD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
56
56
Package_SO
TSSOP-60_8x12.5mm_P0.4mm
TSSOP, 60 Pin (JEDEC MO-153 Var JC-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
60
60
Package_SO
TSSOP-64_6.1x14mm_P0.4mm
TSSOP, 64 Pin (JEDEC MO-153 Var FE https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
64
64
Package_SO
TSSOP-64_6.1x17mm_P0.5mm
TSSOP, 64 Pin (JEDEC MO-153 Var EF https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
64
64
Package_SO
TSSOP-64_8x14mm_P0.4mm
TSSOP, 64 Pin (JEDEC MO-153 Var JD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
64
64
Package_SO
TSSOP-68_8x14mm_P0.4mm
TSSOP, 68 Pin (JEDEC MO-153 Var JD-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
68
68
Package_SO
TSSOP-80_6.1x17mm_P0.4mm
TSSOP, 80 Pin (JEDEC MO-153 Var FF https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSSOP SO
0
80
80
Package_SO
Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm
Texas Instruments HSOP 9, 1.27mm pitch, 3.9x4.9mm body, exposed pad, DDA0008J (http://www.ti.com/lit/ds/symlink/tps5430.pdf)
HSOP 1.27
0
11
9
Package_SO
Texas_HSOP-8-1EP_3.9x4.9mm_P1.27mm_ThermalVias
Texas Instruments HSOP 9, 1.27mm pitch, 3.9x4.9mm body, exposed pad, thermal vias, DDA0008J (http://www.ti.com/lit/ds/symlink/tps5430.pdf)
HSOP 1.27
0
20
9
Package_SO
Texas_HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias
8-pin HTSOP package with 1.27mm pin pitch, compatible with SOIC-8, 3.9x4.9mm body, exposed pad, thermal vias, http://www.ti.com/lit/ds/symlink/drv8870.pdf
HTSOP 1.27
0
18
9
Package_SO
Texas_PWP0020A
20-Pin Thermally Enhanced Thin Shrink Small-Outline Package, Body 4.4x6.5x1.1mm, Pad 3.0x4.2mm, Texas Instruments (see http://www.ti.com/lit/ds/symlink/lm5118.pdf)
PWP HTSSOP 0.65mm
0
25
21
Package_SO
Texas_R-PDSO-G8_EP2.95x4.9mm_Mask2.4x3.1mm
HSOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lmr14030.pdf#page=28, http://www.ti.com/lit/ml/msoi002j/msoi002j.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOIC SO
0
16
9
Package_SO
Texas_R-PDSO-G8_EP2.95x4.9mm_Mask2.4x3.1mm_ThermalVias
HSOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lmr14030.pdf#page=28, http://www.ti.com/lit/ml/msoi002j/msoi002j.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
HSOIC SO
0
23
9
Package_SO
Texas_R-PDSO-N5
Plastic Small outline http://www.ti.com/lit/ml/mpds158c/mpds158c.pdf
SOT23 R-PDSO-N5
0
5
5
Package_SO
VSO-40_7.6x15.4mm_P0.762mm
VSO40: plastic very small outline package; 40 leads (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot158-1_po.pdf)
SSOP 0.762
0
40
40
Package_SO
VSO-56_11.1x21.5mm_P0.75mm
VSO56: plastic very small outline package; 56 leads (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot190-1_po.pdf)
SSOP 0.75
0
56
56
Package_SO
VSSOP-8_2.3x2mm_P0.5mm
VSSOP-8 2.3x2mm Pitch 0.5mm
VSSOP-8 2.3x2mm Pitch 0.5mm
0
8
8
Package_SO
VSSOP-8_2.4x2.1mm_P0.5mm
http://www.ti.com/lit/ml/mpds050d/mpds050d.pdf
VSSOP DCU R-PDSO-G8 Pitch0.5mm
0
8
8
Package_SO
VSSOP-8_3.0x3.0mm_P0.65mm
VSSOP-8 3.0 x 3.0, http://www.ti.com/lit/ds/symlink/lm75b.pdf
VSSOP-8 3.0 x 3.0
0
8
8
Package_SO
VSSOP-10_3x3mm_P0.5mm
VSSOP, 10 Pin (http://www.ti.com/lit/ds/symlink/ads1115.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
VSSOP SO
0
10
10
Package_SO
Vishay_PowerPAK_1212-8_Dual
PowerPAK 1212-8 Dual (https://www.vishay.com/docs/71656/ppak12128.pdf, https://www.vishay.com/docs/72598/72598.pdf)
Vishay_PowerPAK_1212-8_Dual
0
6
6
Package_SO
Vishay_PowerPAK_1212-8_Single
PowerPAK 1212-8 Single (https://www.vishay.com/docs/71656/ppak12128.pdf, https://www.vishay.com/docs/72597/72597.pdf)
Vishay PowerPAK 1212-8 Single
0
5
5
Package_SO
Zetex_SM8
Zetex,  SMD, 8 pin package (http://datasheet.octopart.com/ZDT6758TA-Zetex-datasheet-68057.pdf)
Zetex SM8
0
8
8
Package_TO_SOT_SMD
ATPAK-2
ATPAK SMD package, http://www.onsemi.com/pub/Collateral/ENA2192-D.PDF
ATPAK 
0
7
3
Package_TO_SOT_SMD
Analog_KS-4
Analog Devices KS-4, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sc70ks/ks_4.pdf
Analog Devices KS-4 (like EIAJ SC-82)
0
4
4
Package_TO_SOT_SMD
Diodes_SOT-553
Diodes SOT-553, https://www.diodes.com/assets/Package-Files/SOT553.pdf
SOT-553
0
5
5
Package_TO_SOT_SMD
HVSOF5
HVSOF5, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hvsof5_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/sensor/hall/bu52001gul-e.pdf
HVSOF5
0
5
5
Package_TO_SOT_SMD
HVSOF6
HVSOF6, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hvsof6_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/audio_video/video_amplifier/bh76106hfv-e.pdf
HVSOF6
0
7
7
Package_TO_SOT_SMD
Infineon_PG-HDSOP-10-1
Infineon PG-HDSOP-10-1 (DDPAK), 20.96x6.5x2.3mm, slug up (https://www.infineon.com/cms/en/product/packages/PG-HDSOP/PG-HDSOP-10-1/)
hdsop 10 ddpak
0
10
10
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-1
HSOF-8-1 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-1/)
mosfet hsof toll
0
53
3
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-1_ThermalVias
HSOF-8-1 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-1/)
mosfet hsof toll thermal vias
0
96
3
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-2
HSOF-8-2 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-2/)
mosfet hsof toll
0
12
4
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-2_ThermalVias
HSOF-8-2 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-2/)
mosfet hsof toll thermal vias
0
97
4
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-2_ThermalVias2
HSOF-8-2 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-2/, https://www.infineon.com/dgdl/Infineon-ApplicationNote_600V_CoolMOS_C7_Gold_TOLL-AN-v01_00-EN.pdf?fileId=5546d4625b10283a015b144a1af70df6)
mosfet hsof toll thermal vias
0
159
4
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-3
HSOF-8-3 power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-3/)
mosfet hsof
0
25
4
Package_TO_SOT_SMD
Infineon_PG-HSOF-8-3_ThermalVias
HSOF-8-3 power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-3/)
mosfet hsof
0
64
4
Package_TO_SOT_SMD
Infineon_PG-TO-220-7Lead_TabPin8
Infineon PG-TO-220-7, Tab as Pin 8, see e.g. https://www.infineon.com/dgdl/Infineon-BTS50055-1TMC-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa9b0007235e9
Infineon PG-TO-220-7
0
12
8
Package_TO_SOT_SMD
LFPAK33
LFPAK33 SOT-1210 https://assets.nexperia.com/documents/outline-drawing/SOT1210.pdf
LFPAK33 SOT-1210
0
17
5
Package_TO_SOT_SMD
LFPAK56
LFPAK56 https://assets.nexperia.com/documents/outline-drawing/SOT669.pdf
LFPAK56 SOT-669 Power-SO8
0
18
5
Package_TO_SOT_SMD
Nexperia_CFP15_SOT-1289
Nexperia CFP15 (SOT-1289), https://assets.nexperia.com/documents/outline-drawing/SOT1289.pdf
SOT-1289 CFP15
0
8
3
Package_TO_SOT_SMD
OnSemi_ECH8
On Semiconductor ECH8, https://www.onsemi.com/pub/Collateral/318BF.PDF
ECH8 SOT28-FL SOT-28-FL
0
8
8
Package_TO_SOT_SMD
PQFN_8x8
Low Profile 8x8mm PQFN, Dual Cool 88, https://www.onsemi.com/pub/Collateral/FDMT80080DC-D.pdf
pqfn vdfn mosfet
0
9
3
Package_TO_SOT_SMD
PowerMacro_M234_NoHole
TO-50-4 Power Macro Package Style M234
TO-50-4 Power Macro Package Style M234
0
4
4
Package_TO_SOT_SMD
PowerMacro_M234_WithHole
TO-50-4 Power Macro Package Style M234
TO-50-4 Power Macro Package Style M234
0
4
4
Package_TO_SOT_SMD
Rohm_HRP7
Rohm HRP7 SMD package, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hrp7_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/motor/dc/bd621x-e.pdf
Rohm HRP7 SMD
0
69
7
Package_TO_SOT_SMD
SC-59
SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg
SC-59
0
3
3
Package_TO_SOT_SMD
SC-59_Handsoldering
SC-59, hand-soldering varaint, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg
SC-59 hand-soldering
0
3
3
Package_TO_SOT_SMD
SC-70-8
SC70-8
SC70-8
0
8
8
Package_TO_SOT_SMD
SC-70-8_Handsoldering
SC70-8, Handsoldering
SC70-8 Handsoldering
0
8
8
Package_TO_SOT_SMD
SC-82AA
SC-82AA
SC-82AA
0
4
4
Package_TO_SOT_SMD
SC-82AA_Handsoldering
SC-82AA
SC-82AA
0
4
4
Package_TO_SOT_SMD
SC-82AB
SC-82AB
SC-82AB
0
4
4
Package_TO_SOT_SMD
SC-82AB_Handsoldering
SC-82AB
SC-82AB
0
4
4
Package_TO_SOT_SMD
SOT-23
SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOT TO_SOT_SMD
0
3
3
Package_TO_SOT_SMD
SOT-23-5
SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOT TO_SOT_SMD
0
5
5
Package_TO_SOT_SMD
SOT-23-5_HandSoldering
5-pin SOT23 package
SOT-23-5 hand-soldering
0
5
5
Package_TO_SOT_SMD
SOT-23-6
SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOT TO_SOT_SMD
0
6
6
Package_TO_SOT_SMD
SOT-23-6_Handsoldering
6-pin SOT-23 package, Handsoldering
SOT-23-6 Handsoldering
0
6
6
Package_TO_SOT_SMD
SOT-23-8
SOT, 8 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOT TO_SOT_SMD
0
8
8
Package_TO_SOT_SMD
SOT-23-8_Handsoldering
8-pin SOT-23 package, Handsoldering, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sot-23rj/rj_8.pdf
SOT-23-8 Handsoldering
0
8
8
Package_TO_SOT_SMD
SOT-23W
SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3
SOT-23W
0
3
3
Package_TO_SOT_SMD
SOT-23W_Handsoldering
SOT-23W http://www.allegromicro.com/~/media/Files/Datasheets/A112x-Datasheet.ashx?la=en&hash=7BC461E058CC246E0BAB62433B2F1ECA104CA9D3
SOT-23W for handsoldering
0
3
3
Package_TO_SOT_SMD
SOT-23_Handsoldering
SOT-23, Handsoldering
SOT-23
0
3
3
Package_TO_SOT_SMD
SOT-89-3
SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf
SOT-89-3
0
3
3
Package_TO_SOT_SMD
SOT-89-3_Handsoldering
SOT-89-3 Handsoldering
SOT-89-3 Handsoldering
0
3
3
Package_TO_SOT_SMD
SOT-89-5
SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf
SOT-89-5
0
5
5
Package_TO_SOT_SMD
SOT-89-5_Handsoldering
SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf
SOT-89-5
0
5
5
Package_TO_SOT_SMD
SOT-143
SOT-143 https://www.nxp.com/docs/en/package-information/SOT143B.pdf
SOT-143
0
4
4
Package_TO_SOT_SMD
SOT-143R
SOT-143R, reverse pinning, https://www.nxp.com/docs/en/package-information/SOT143R.pdf
SOT-143R Reverse
0
4
4
Package_TO_SOT_SMD
SOT-143R_Handsoldering
SOT-143R, reverse pinning, Handsoldering, https://www.nxp.com/docs/en/package-information/SOT143R.pdf
SOT-143 Reverse Handsoldering
0
4
4
Package_TO_SOT_SMD
SOT-143_Handsoldering
SOT-143 Handsoldering https://www.nxp.com/docs/en/package-information/SOT143B.pdf
SOT-143 Handsoldering
0
4
4
Package_TO_SOT_SMD
SOT-223
module CMS SOT223 4 pins
CMS SOT
0
4
4
Package_TO_SOT_SMD
SOT-223-3_TabPin2
module CMS SOT223 4 pins
CMS SOT
0
4
3
Package_TO_SOT_SMD
SOT-223-5
module CMS SOT223 5 pins, http://ww1.microchip.com/downloads/en/DeviceDoc/51751a.pdf
CMS SOT
0
5
5
Package_TO_SOT_SMD
SOT-223-6
module CMS SOT223 6 pins, http://www.ti.com/lit/ds/symlink/tps737.pdf
CMS SOT
0
6
6
Package_TO_SOT_SMD
SOT-223-6_TabPin3
module CMS SOT223 6 pins, http://www.ti.com/lit/ds/symlink/tps737.pdf
CMS SOT
0
6
5
Package_TO_SOT_SMD
SOT-223-8
module CMS SOT223 8 pins, https://www.diodes.com/assets/Datasheets/ZXSBMR16PT8.pdf
CMS SOT
0
8
8
Package_TO_SOT_SMD
SOT-323_SC-70
SOT-323, SC-70
SOT-323 SC-70
0
3
3
Package_TO_SOT_SMD
SOT-323_SC-70_Handsoldering
SOT-323, SC-70 Handsoldering
SOT-323 SC-70 Handsoldering
0
3
3
Package_TO_SOT_SMD
SOT-343_SC-70-4
SOT-343, SC-70-4
SOT-343 SC-70-4
0
4
4
Package_TO_SOT_SMD
SOT-343_SC-70-4_Handsoldering
SOT-343, SC-70-4, Handsoldering
SOT-343 SC-70-4 Handsoldering
0
4
4
Package_TO_SOT_SMD
SOT-353_SC-70-5
SOT-353, SC-70-5
SOT-353 SC-70-5
0
5
5
Package_TO_SOT_SMD
SOT-353_SC-70-5_Handsoldering
SOT-353, SC-70-5, Handsoldering
SOT-353 SC-70-5 Handsoldering
0
5
5
Package_TO_SOT_SMD
SOT-363_SC-70-6
SOT-363, SC-70-6
SOT-363 SC-70-6
0
6
6
Package_TO_SOT_SMD
SOT-363_SC-70-6_Handsoldering
SOT-363, SC-70-6, Handsoldering
SOT-363 SC-70-6 Handsoldering
0
6
6
Package_TO_SOT_SMD
SOT-383F
8-pin SOT-383F, http://www.mouser.com/ds/2/80/CPDVR085V0C-HF-RevB-10783.pdf
SOT-383F
0
9
9
Package_TO_SOT_SMD
SOT-383FL
8-pin SOT-383FL package, http://www.onsemi.com/pub_link/Collateral/ENA2267-D.PDF
SOT-383FL
0
8
8
Package_TO_SOT_SMD
SOT-416
SOT-416, https://www.nxp.com/docs/en/package-information/SOT416.pdf
SOT-416
0
3
3
Package_TO_SOT_SMD
SOT-523
SOT523, https://www.diodes.com/assets/Package-Files/SOT523.pdf
SOT-523
0
3
3
Package_TO_SOT_SMD
SOT-543
SOT-543 4 lead surface package
SOT-543 SC-107A EMD4
0
4
4
Package_TO_SOT_SMD
SOT-553
SOT553
SOT-553
0
5
5
Package_TO_SOT_SMD
SOT-563
SOT563
SOT-563
0
6
6
Package_TO_SOT_SMD
SOT-665
SOT665
SOT-665
0
5
5
Package_TO_SOT_SMD
SOT-666
SOT666
SOT-666
0
6
6
Package_TO_SOT_SMD
SOT-723
http://toshiba.semicon-storage.com/info/docget.jsp?did=5879&prodName=RN1104MFV
sot 723
0
3
3
Package_TO_SOT_SMD
SOT-883
SOT-883, https://assets.nexperia.com/documents/outline-drawing/SOT883.pdf
SOT-883
0
3
3
Package_TO_SOT_SMD
SOT-886
SOT-886
SOT-886
0
6
6
Package_TO_SOT_SMD
SOT-963
SOT 963 6 pins package 1x0.8mm pitch 0.35mm
SOT 963 6 pins package 1x0.8mm pitch 0.35mm
0
6
6
Package_TO_SOT_SMD
SOT-1123
SOT-1123 small outline transistor (see http://www.onsemi.com/pub/Collateral/NST3906F3-D.PDF)
SOT-1123 transistor
0
3
3
Package_TO_SOT_SMD
SOT-1333-1
SOT-1333-1 
SOT-1333-1 
0
9
9
Package_TO_SOT_SMD
SOT-1334-1
SOT-1334-1
SOT-1334-1
0
14
14
Package_TO_SOT_SMD
SuperSOT-3
3-pin SuperSOT package https://www.fairchildsemi.com/package-drawings/MA/MA03B.pdf
SuperSOT-3 SSOT-3
0
3
3
Package_TO_SOT_SMD
SuperSOT-6
6-pin SuperSOT package http://www.mouser.com/ds/2/149/FMB5551-889214.pdf
SuperSOT-6 SSOT-6
0
6
6
Package_TO_SOT_SMD
SuperSOT-8
8-pin SuperSOT package, http://www.icbank.com/icbank_data/semi_package/ssot8_dim.pdf
SuperSOT-8 SSOT-8
0
8
8
Package_TO_SOT_SMD
TDSON-8-1
Power MOSFET package, TDSON-8-1, 5.15x5.9mm (https://www.infineon.com/cms/en/product/packages/PG-TDSON/PG-TDSON-8-1/)
tdson 
0
14
5
Package_TO_SOT_SMD
TO-50-3_LongPad-NoHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
Package_TO_SOT_SMD
TO-50-3_LongPad-WithHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
Package_TO_SOT_SMD
TO-50-3_ShortPad-NoHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
Package_TO_SOT_SMD
TO-50-3_ShortPad-WithHole_Housing
TO-50-3 Macro T Package Style M236
TO-50-3 Macro T Package Style M236
0
3
3
Package_TO_SOT_SMD
TO-50-4_LongPad-NoHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
Package_TO_SOT_SMD
TO-50-4_LongPad-WithHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
Package_TO_SOT_SMD
TO-50-4_ShortPad-NoHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
Package_TO_SOT_SMD
TO-50-4_ShortPad-WithHole_Housing
TO-50-4 Macro X Package Style M238
TO-50-4 Macro X Package Style M238
0
4
4
Package_TO_SOT_SMD
TO-252-2
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/
DPAK TO-252 DPAK-3 TO-252-3 SOT-428
0
7
3
Package_TO_SOT_SMD
TO-252-2_TabPin1
TO-252-2, tab to pin 1 https://www.wolfspeed.com/media/downloads/87/CSD01060.pdf
TO-252-2 diode
0
7
2
Package_TO_SOT_SMD
TO-252-3_TabPin2
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/
DPAK TO-252 DPAK-3 TO-252-3 SOT-428
0
8
3
Package_TO_SOT_SMD
TO-252-3_TabPin4
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/
DPAK TO-252 DPAK-3 TO-252-3 SOT-428
0
8
4
Package_TO_SOT_SMD
TO-252-4
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-5-11/
DPAK TO-252 DPAK-5 TO-252-5
0
9
5
Package_TO_SOT_SMD
TO-252-5_TabPin3
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-5-11/
DPAK TO-252 DPAK-5 TO-252-5
0
10
5
Package_TO_SOT_SMD
TO-252-5_TabPin6
TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-5-11/
DPAK TO-252 DPAK-5 TO-252-5
0
10
6
Package_TO_SOT_SMD
TO-263-2
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
7
3
Package_TO_SOT_SMD
TO-263-2_TabPin1
TO-263 / D2PAK / DDPAK SMD package, tab to pin 1, https://www.wolfspeed.com/media/downloads/137/C3D06060G.pdf
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404 diode
0
7
2
Package_TO_SOT_SMD
TO-263-3_TabPin2
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
8
3
Package_TO_SOT_SMD
TO-263-3_TabPin4
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
8
4
Package_TO_SOT_SMD
TO-263-4
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
9
5
Package_TO_SOT_SMD
TO-263-5_TabPin3
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
10
5
Package_TO_SOT_SMD
TO-263-5_TabPin6
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-5-1/
D2PAK DDPAK TO-263 D2PAK-5 TO-263-5 SOT-426
0
10
6
Package_TO_SOT_SMD
TO-263-6
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/
D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427
0
11
7
Package_TO_SOT_SMD
TO-263-7_TabPin4
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/
D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427
0
12
7
Package_TO_SOT_SMD
TO-263-7_TabPin8
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-7-1/
D2PAK DDPAK TO-263 D2PAK-7 TO-263-7 SOT-427
0
12
8
Package_TO_SOT_SMD
TO-263-9_TabPin5
TO-263 / D2PAK / DDPAK SMD package, http://www.ti.com/lit/ds/symlink/lm4755.pdf
D2PAK DDPAK TO-263 D2PAK-9 TO-263-9
0
14
9
Package_TO_SOT_SMD
TO-263-9_TabPin10
TO-263 / D2PAK / DDPAK SMD package, http://www.ti.com/lit/ds/symlink/lm4755.pdf
D2PAK DDPAK TO-263 D2PAK-9 TO-263-9
0
14
10
Package_TO_SOT_SMD
TO-268-2
TO-268/D3PAK SMD package, http://www.icbank.com/icbank_data/semi_package/to268aa_dim.pdf
D3PAK TO-268 D3PAK-3 TO-268-3
0
7
3
Package_TO_SOT_SMD
TO-269AA
SMD package TO-269AA (e.g. diode bridge), see http://www.vishay.com/docs/88854/padlayouts.pdf
TO-269AA MBS diode bridge
0
4
4
Package_TO_SOT_SMD
TO-277A
Thermal enhanced ultra thin SMD package; 3 leads; body: 4.3x6.1x0.43mm, https://www.vishay.com/docs/95570/to-277asmpc.pdf
TO-277A SMPC
0
12
3
Package_TO_SOT_SMD
TO-277B
TO-227B https://media.digikey.com/pdf/Data%20Sheets/Littelfuse%20PDFs/DST2050S.pdf
TO-277B
0
9
3
Package_TO_SOT_SMD
TSOT-23
3-pin TSOT23 package, http://www.analog.com.tw/pdf/All_In_One.pdf
TSOT-23
0
3
3
Package_TO_SOT_SMD
TSOT-23-5
TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOT TO_SOT_SMD
0
5
5
Package_TO_SOT_SMD
TSOT-23-5_HandSoldering
5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf
TSOT-23-5 Hand-soldering
0
5
5
Package_TO_SOT_SMD
TSOT-23-6
TSOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOT TO_SOT_SMD
0
6
6
Package_TO_SOT_SMD
TSOT-23-6_HandSoldering
6-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_6_05-08-1636.pdf
TSOT-23-6 MK06A TSOT-6 Hand-soldering
0
6
6
Package_TO_SOT_SMD
TSOT-23-8
TSOT, 8 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant BA), generated with kicad-footprint-generator ipc_gullwing_generator.py
TSOT TO_SOT_SMD
0
8
8
Package_TO_SOT_SMD
TSOT-23-8_HandSoldering
8-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_8_05-08-1637.pdf
TSOT-23-8 Hand-soldering
0
8
8
Package_TO_SOT_SMD
TSOT-23_HandSoldering
5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf
TSOT-23 Hand-soldering
0
3
3
Package_TO_SOT_SMD
Texas_DRT-3
Texas Instrument DRT-3 1x0.8mm Pitch 0.7mm http://www.ti.com/lit/ds/symlink/tpd2eusb30.pdf
DRT-3 1x0.8mm Pitch 0.7mm
0
3
3
Package_TO_SOT_SMD
Texas_NDQ
Texas Instruments, NDQ, 5 pin (https://www.ti.com/lit/ml/mmsf022/mmsf022.pdf)
ti pfm dap
0
6
6
Package_TO_SOT_SMD
Texas_NDY0011A
TO-PMOD-11 11-pin switching regulator package, http://www.ti.com/lit/ml/mmsf025/mmsf025.pdf
Texas TO-PMOD NDY00011A
0
12
12
Package_TO_SOT_SMD
Texas_R-PDSO-G6
R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf
R-PDSO-G6 SC-70-6
0
6
6
Package_TO_SOT_SMD
VSOF5
VSOF5
VSOF5
0
5
5
Package_TO_SOT_SMD
Vishay_PowerPAK_SC70-6L_Dual
Vishay PowerPAK SC70 dual transistor package http://www.vishay.com/docs/70487/70487.pdf
powerpak sc70 sc-70 dual
0
8
6
Package_TO_SOT_SMD
Vishay_PowerPAK_SC70-6L_Single
Vishay PowerPAK SC70 single transistor package http://www.vishay.com/docs/70486/70486.pdf
powerpak sc70 sc-70
0
6
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-3-5.08_1x03_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-3-5.08, 3 pins, pitch 5.08mm, size 15.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-3-5.08 pitch 5.08mm size 15.2x9.8mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-3_1x03_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-3, 3 pins, pitch 5mm, size 15x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-3 pitch 5mm size 15x9.8mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-4-5.08_1x04_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-4-5.08, 4 pins, pitch 5.08mm, size 20.3x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-4-5.08 pitch 5.08mm size 20.3x9.8mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-4_1x04_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-4, 4 pins, pitch 5mm, size 20x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-4 pitch 5mm size 20x9.8mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-5-5.08_1x05_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-5-5.08, 5 pins, pitch 5.08mm, size 25.4x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-5-5.08 pitch 5.08mm size 25.4x9.8mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-5_1x05_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-5, 5 pins, pitch 5mm, size 25x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-5 pitch 5mm size 25x9.8mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-6-5.08_1x06_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-6-5.08, 6 pins, pitch 5.08mm, size 30.5x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-6-5.08 pitch 5.08mm size 30.5x9.8mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-6_1x06_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-6, 6 pins, pitch 5mm, size 30x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-6 pitch 5mm size 30x9.8mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-7-5.08_1x07_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-7-5.08, 7 pins, pitch 5.08mm, size 35.6x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-7-5.08 pitch 5.08mm size 35.6x9.8mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-7_1x07_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-7, 7 pins, pitch 5mm, size 35x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-7 pitch 5mm size 35x9.8mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-8-5.08_1x08_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-8-5.08, 8 pins, pitch 5.08mm, size 40.6x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-8-5.08 pitch 5.08mm size 40.6x9.8mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-8_1x08_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-8, 8 pins, pitch 5mm, size 40x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-8 pitch 5mm size 40x9.8mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-9-5.08_1x09_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-9-5.08, 9 pins, pitch 5.08mm, size 45.7x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-9-5.08 pitch 5.08mm size 45.7x9.8mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-9_1x09_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-9, 9 pins, pitch 5mm, size 45x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-9 pitch 5mm size 45x9.8mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-10-5.08, 10 pins, pitch 5.08mm, size 50.8x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-10-5.08 pitch 5.08mm size 50.8x9.8mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-10_1x10_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-10, 10 pins, pitch 5mm, size 50x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-10 pitch 5mm size 50x9.8mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-11-5.08_1x11_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-11-5.08, 11 pins, pitch 5.08mm, size 55.9x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-11-5.08 pitch 5.08mm size 55.9x9.8mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-11_1x11_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-11, 11 pins, pitch 5mm, size 55x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-11 pitch 5mm size 55x9.8mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-12-5.08_1x12_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-12-5.08, 12 pins, pitch 5.08mm, size 61x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-12-5.08 pitch 5.08mm size 61x9.8mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-12_1x12_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-12, 12 pins, pitch 5mm, size 60x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-12 pitch 5mm size 60x9.8mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-13-5.08_1x13_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-13-5.08, 13 pins, pitch 5.08mm, size 66x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-13-5.08 pitch 5.08mm size 66x9.8mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-13_1x13_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-13, 13 pins, pitch 5mm, size 65x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-13 pitch 5mm size 65x9.8mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-14-5.08_1x14_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-14-5.08, 14 pins, pitch 5.08mm, size 71.1x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-14-5.08 pitch 5.08mm size 71.1x9.8mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-14_1x14_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-14, 14 pins, pitch 5mm, size 70x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-14 pitch 5mm size 70x9.8mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-15-5.08_1x15_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-15-5.08, 15 pins, pitch 5.08mm, size 76.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-15-5.08 pitch 5.08mm size 76.2x9.8mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-15_1x15_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-15, 15 pins, pitch 5mm, size 75x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-15 pitch 5mm size 75x9.8mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-16-5.08_1x16_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-1,5-16-5.08, 16 pins, pitch 5.08mm, size 81.3x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-16-5.08 pitch 5.08mm size 81.3x9.8mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-1,5-16_1x16_P5.00mm_Horizontal
Terminal Block Phoenix MKDS-1,5-16, 16 pins, pitch 5mm, size 80x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-1,5-16 pitch 5mm size 80x9.8mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-3-5.08_1x03_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-3-5.08, 3 pins, pitch 5.08mm, size 15.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-3-5.08 pitch 5.08mm size 15.2x11.2mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-4-5.08_1x04_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-4-5.08, 4 pins, pitch 5.08mm, size 20.3x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-4-5.08 pitch 5.08mm size 20.3x11.2mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-5-5.08_1x05_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-5-5.08, 5 pins, pitch 5.08mm, size 25.4x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-5-5.08 pitch 5.08mm size 25.4x11.2mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-6-5.08_1x06_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-6-5.08, 6 pins, pitch 5.08mm, size 30.5x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-6-5.08 pitch 5.08mm size 30.5x11.2mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-7-5.08_1x07_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-7-5.08, 7 pins, pitch 5.08mm, size 35.6x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-7-5.08 pitch 5.08mm size 35.6x11.2mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-8-5.08_1x08_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-8-5.08, 8 pins, pitch 5.08mm, size 40.6x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-8-5.08 pitch 5.08mm size 40.6x11.2mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-9-5.08_1x09_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-9-5.08, 9 pins, pitch 5.08mm, size 45.7x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-9-5.08 pitch 5.08mm size 45.7x11.2mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-10-5.08_1x10_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-10-5.08, 10 pins, pitch 5.08mm, size 50.8x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-10-5.08 pitch 5.08mm size 50.8x11.2mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-11-5.08_1x11_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-11-5.08, 11 pins, pitch 5.08mm, size 55.9x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-11-5.08 pitch 5.08mm size 55.9x11.2mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-12-5.08_1x12_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-12-5.08, 12 pins, pitch 5.08mm, size 61x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-12-5.08 pitch 5.08mm size 61x11.2mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-13-5.08_1x13_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-13-5.08, 13 pins, pitch 5.08mm, size 66x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-13-5.08 pitch 5.08mm size 66x11.2mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-14-5.08_1x14_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-14-5.08, 14 pins, pitch 5.08mm, size 71.1x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-14-5.08 pitch 5.08mm size 71.1x11.2mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-15-5.08_1x15_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-15-5.08, 15 pins, pitch 5.08mm, size 76.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-15-5.08 pitch 5.08mm size 76.2x11.2mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MKDS-3-16-5.08_1x16_P5.08mm_Horizontal
Terminal Block Phoenix MKDS-3-16-5.08, 16 pins, pitch 5.08mm, size 81.3x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MKDS-3-16-5.08 pitch 5.08mm size 81.3x11.2mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-2-2.54_1x02_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-2-2.54, 2 pins, pitch 2.54mm, size 5.54x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-2-2.54 pitch 2.54mm size 5.54x6.2mm^2 drill 1.1mm pad 2.2mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-3-2.54_1x03_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-3-2.54, 3 pins, pitch 2.54mm, size 8.08x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725656-920552.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-3-2.54 pitch 2.54mm size 8.08x6.2mm^2 drill 1.1mm pad 2.2mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-4-2.54_1x04_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-4-2.54, 4 pins, pitch 2.54mm, size 10.6x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-4-2.54 pitch 2.54mm size 10.6x6.2mm^2 drill 1.1mm pad 2.2mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-5-2.54_1x05_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-5-2.54, 5 pins, pitch 2.54mm, size 13.2x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-5-2.54 pitch 2.54mm size 13.2x6.2mm^2 drill 1.1mm pad 2.2mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-6-2.54_1x06_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-6-2.54, 6 pins, pitch 2.54mm, size 15.7x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-6-2.54 pitch 2.54mm size 15.7x6.2mm^2 drill 1.1mm pad 2.2mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-7-2.54_1x07_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-7-2.54, 7 pins, pitch 2.54mm, size 18.2x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-7-2.54 pitch 2.54mm size 18.2x6.2mm^2 drill 1.1mm pad 2.2mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-8-2.54_1x08_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-8-2.54, 8 pins, pitch 2.54mm, size 20.8x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-8-2.54 pitch 2.54mm size 20.8x6.2mm^2 drill 1.1mm pad 2.2mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-9-2.54_1x09_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-9-2.54, 9 pins, pitch 2.54mm, size 23.3x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-9-2.54 pitch 2.54mm size 23.3x6.2mm^2 drill 1.1mm pad 2.2mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-10-2.54_1x10_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-10-2.54, 10 pins, pitch 2.54mm, size 25.9x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-10-2.54 pitch 2.54mm size 25.9x6.2mm^2 drill 1.1mm pad 2.2mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-11-2.54_1x11_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-11-2.54, 11 pins, pitch 2.54mm, size 28.4x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-11-2.54 pitch 2.54mm size 28.4x6.2mm^2 drill 1.1mm pad 2.2mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_MPT-0,5-12-2.54_1x12_P2.54mm_Horizontal
Terminal Block Phoenix MPT-0,5-12-2.54, 12 pins, pitch 2.54mm, size 30.9x6.2mm^2, drill diamater 1.1mm, pad diameter 2.2mm, see http://www.mouser.com/ds/2/324/ItemDetail_1725672-916605.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix MPT-0,5-12-2.54 pitch 2.54mm size 30.9x6.2mm^2 drill 1.1mm pad 2.2mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-2-3.5-H_1x02_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-2-3.5-H, 2 pins, pitch 3.5mm, size 7x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-2-3.5-H pitch 3.5mm size 7x7.6mm^2 drill 1.2mm pad 2.4mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-2-5.0-H_1x02_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-2-5.0-H, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-2-5.0-H pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.6mm
0
2
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-3-5.0-H_1x03_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-3-5.0-H, 3 pins, pitch 5mm, size 15x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-3-5.0-H pitch 5mm size 15x9mm^2 drill 1.3mm pad 2.6mm
0
3
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-4-3.5-H_1x04_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-4-3.5-H, 4 pins, pitch 3.5mm, size 14x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-4-3.5-H pitch 3.5mm size 14x7.6mm^2 drill 1.2mm pad 2.4mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-4-5.0-H_1x04_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-4-5.0-H, 4 pins, pitch 5mm, size 20x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-4-5.0-H pitch 5mm size 20x9mm^2 drill 1.3mm pad 2.6mm
0
4
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-5-3.5-H_1x05_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-5-3.5-H, 5 pins, pitch 3.5mm, size 17.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-5-3.5-H pitch 3.5mm size 17.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-5-5.0-H_1x05_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-5-5.0-H, 5 pins, pitch 5mm, size 25x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-5-5.0-H pitch 5mm size 25x9mm^2 drill 1.3mm pad 2.6mm
0
5
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-6-3.5-H_1x06_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-6-3.5-H, 6 pins, pitch 3.5mm, size 21x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-6-3.5-H pitch 3.5mm size 21x7.6mm^2 drill 1.2mm pad 2.4mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-6-5.0-H_1x06_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-6-5.0-H, 6 pins, pitch 5mm, size 30x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-6-5.0-H pitch 5mm size 30x9mm^2 drill 1.3mm pad 2.6mm
0
6
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-7-3.5-H_1x07_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-7-3.5-H, 7 pins, pitch 3.5mm, size 24.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-7-3.5-H pitch 3.5mm size 24.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-7-5.0-H, 7 pins, pitch 5mm, size 35x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-7-5.0-H pitch 5mm size 35x9mm^2 drill 1.3mm pad 2.6mm
0
7
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-8-3.5-H_1x08_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-8-3.5-H, 8 pins, pitch 3.5mm, size 28x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-8-3.5-H pitch 3.5mm size 28x7.6mm^2 drill 1.2mm pad 2.4mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-8-5.0-H_1x08_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-8-5.0-H, 8 pins, pitch 5mm, size 40x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-8-5.0-H pitch 5mm size 40x9mm^2 drill 1.3mm pad 2.6mm
0
8
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-9-3.5-H_1x09_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-9-3.5-H, 9 pins, pitch 3.5mm, size 31.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-9-3.5-H pitch 3.5mm size 31.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-9-5.0-H_1x09_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-9-5.0-H, 9 pins, pitch 5mm, size 45x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-9-5.0-H pitch 5mm size 45x9mm^2 drill 1.3mm pad 2.6mm
0
9
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-10-3.5-H_1x10_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-10-3.5-H, 10 pins, pitch 3.5mm, size 35x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-10-3.5-H pitch 3.5mm size 35x7.6mm^2 drill 1.2mm pad 2.4mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-10-5.0-H_1x10_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-10-5.0-H, 10 pins, pitch 5mm, size 50x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-10-5.0-H pitch 5mm size 50x9mm^2 drill 1.3mm pad 2.6mm
0
10
10
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-11-3.5-H_1x11_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-11-3.5-H, 11 pins, pitch 3.5mm, size 38.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-11-3.5-H pitch 3.5mm size 38.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-11-5.0-H_1x11_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-11-5.0-H, 11 pins, pitch 5mm, size 55x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-11-5.0-H pitch 5mm size 55x9mm^2 drill 1.3mm pad 2.6mm
0
11
11
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-12-3.5-H_1x12_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-12-3.5-H, 12 pins, pitch 3.5mm, size 42x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-12-3.5-H pitch 3.5mm size 42x7.6mm^2 drill 1.2mm pad 2.4mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-12-5.0-H_1x12_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-12-5.0-H, 12 pins, pitch 5mm, size 60x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-12-5.0-H pitch 5mm size 60x9mm^2 drill 1.3mm pad 2.6mm
0
12
12
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-13-3.5-H_1x13_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-13-3.5-H, 13 pins, pitch 3.5mm, size 45.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-13-3.5-H pitch 3.5mm size 45.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-13-5.0-H_1x13_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-13-5.0-H, 13 pins, pitch 5mm, size 65x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-13-5.0-H pitch 5mm size 65x9mm^2 drill 1.3mm pad 2.6mm
0
13
13
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-14-3.5-H_1x14_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-14-3.5-H, 14 pins, pitch 3.5mm, size 49x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-14-3.5-H pitch 3.5mm size 49x7.6mm^2 drill 1.2mm pad 2.4mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-14-5.0-H_1x14_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-14-5.0-H, 14 pins, pitch 5mm, size 70x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-14-5.0-H pitch 5mm size 70x9mm^2 drill 1.3mm pad 2.6mm
0
14
14
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-15-3.5-H_1x15_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-15-3.5-H, 15 pins, pitch 3.5mm, size 52.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-15-3.5-H pitch 3.5mm size 52.5x7.6mm^2 drill 1.2mm pad 2.4mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-15-5.0-H_1x15_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-15-5.0-H, 15 pins, pitch 5mm, size 75x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-15-5.0-H pitch 5mm size 75x9mm^2 drill 1.3mm pad 2.6mm
0
15
15
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-16-3.5-H_1x16_P3.50mm_Horizontal
Terminal Block Phoenix PT-1,5-16-3.5-H, 16 pins, pitch 3.5mm, size 56x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-16-3.5-H pitch 3.5mm size 56x7.6mm^2 drill 1.2mm pad 2.4mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PT-1,5-16-5.0-H_1x16_P5.00mm_Horizontal
Terminal Block Phoenix PT-1,5-16-5.0-H, 16 pins, pitch 5mm, size 80x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PT-1,5-16-5.0-H pitch 5mm size 80x9mm^2 drill 1.3mm pad 2.6mm
0
16
16
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-2,5-V-SMD_1x02-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 2 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814702/pdf
PhoenixContact PTSM0.5 2 2.5mm vertical SMD spring clamp terminal block connector 
0
4
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-2.5-H-THR_1x02_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-2-2.5-H-THR, 2 pins, pitch 2.5mm, size 7.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-2-2.5-H-THR pitch 2.5mm size 7.2x10mm^2 drill 1.2mm pad 3mm
0
4
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-2.5-V-THR_1x02_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-2-2.5-V-THR, vertical (cable from top), 2 pins, pitch 2.5mm, size 5.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-2-2.5-V-THR vertical pitch 2.5mm size 5.5x5mm^2 drill 1.2mm pad 2mm
0
4
2
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-2-HV-2.5-SMD_1x02-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 2 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778696/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
4
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-2,5-V-SMD_1x03-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 3 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814715/pdf
PhoenixContact PTSM0.5 3 2.5mm vertical SMD spring clamp terminal block connector 
0
5
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-2.5-H-THR_1x03_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-3-2.5-H-THR, 3 pins, pitch 2.5mm, size 9.7x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-3-2.5-H-THR pitch 2.5mm size 9.7x10mm^2 drill 1.2mm pad 3mm
0
6
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-2.5-V-THR_1x03_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-3-2.5-V-THR, vertical (cable from top), 3 pins, pitch 2.5mm, size 8x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-3-2.5-V-THR vertical pitch 2.5mm size 8x5mm^2 drill 1.2mm pad 2mm
0
6
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-3-HV-2.5-SMD_1x03-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 3 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778706/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
5
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-2,5-V-SMD_1x04-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 4 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814728/pdf
PhoenixContact PTSM0.5 4 2.5mm vertical SMD spring clamp terminal block connector 
0
6
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-2.5-H-THR_1x04_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-4-2.5-H-THR, 4 pins, pitch 2.5mm, size 12.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-4-2.5-H-THR pitch 2.5mm size 12.2x10mm^2 drill 1.2mm pad 3mm
0
8
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-2.5-V-THR_1x04_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-4-2.5-V-THR, vertical (cable from top), 4 pins, pitch 2.5mm, size 10.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-4-2.5-V-THR vertical pitch 2.5mm size 10.5x5mm^2 drill 1.2mm pad 2mm
0
8
4
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-4-HV-2.5-SMD_1x04-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 4 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778719/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
4
3
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-2,5-V-SMD_1x05-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 5 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814731/pdf
PhoenixContact PTSM0.5 5 2.5mm vertical SMD spring clamp terminal block connector 
0
7
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-2.5-H-THR_1x05_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-5-2.5-H-THR, 5 pins, pitch 2.5mm, size 14.7x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-5-2.5-H-THR pitch 2.5mm size 14.7x10mm^2 drill 1.2mm pad 3mm
0
10
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-2.5-V-THR_1x05_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-5-2.5-V-THR, vertical (cable from top), 5 pins, pitch 2.5mm, size 13x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-5-2.5-V-THR vertical pitch 2.5mm size 13x5mm^2 drill 1.2mm pad 2mm
0
10
5
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-5-HV-2.5-SMD_1x05-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 5 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778722/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
7
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-2,5-V-SMD_1x06-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 6 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814744/pdf
PhoenixContact PTSM0.5 6 2.5mm vertical SMD spring clamp terminal block connector 
0
8
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-2.5-H-THR_1x06_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-6-2.5-H-THR, 6 pins, pitch 2.5mm, size 17.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-6-2.5-H-THR pitch 2.5mm size 17.2x10mm^2 drill 1.2mm pad 3mm
0
12
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-2.5-V-THR_1x06_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-6-2.5-V-THR, vertical (cable from top), 6 pins, pitch 2.5mm, size 15.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-6-2.5-V-THR vertical pitch 2.5mm size 15.5x5mm^2 drill 1.2mm pad 2mm
0
12
6
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-6-HV-2.5-SMD_1x06-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 6 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778735/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
8
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-2,5-V-SMD_1x07-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 7 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814757/pdf
PhoenixContact PTSM0.5 7 2.5mm vertical SMD spring clamp terminal block connector 
0
9
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-2.5-H-THR_1x07_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-7-2.5-H-THR, 7 pins, pitch 2.5mm, size 19.7x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-7-2.5-H-THR pitch 2.5mm size 19.7x10mm^2 drill 1.2mm pad 3mm
0
14
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-2.5-V-THR_1x07_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-7-2.5-V-THR, vertical (cable from top), 7 pins, pitch 2.5mm, size 18x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-7-2.5-V-THR vertical pitch 2.5mm size 18x5mm^2 drill 1.2mm pad 2mm
0
14
7
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-7-HV-2.5-SMD_1x07-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 7 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778748/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
9
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-2,5-V-SMD_1x08-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 8 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1814760/pdf
PhoenixContact PTSM0.5 8 2.5mm vertical SMD spring clamp terminal block connector 
0
10
9
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-2.5-H-THR_1x08_P2.50mm_Horizontal
Terminal Block Phoenix PTSM-0,5-8-2.5-H-THR, 8 pins, pitch 2.5mm, size 22.2x10mm^2, drill diamater 1.2mm, pad diameter 3mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556441-da-01-de-LEITERPLATTENKL__PTSM_0_5__8_2_5_H_THR.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-8-2.5-H-THR pitch 2.5mm size 22.2x10mm^2 drill 1.2mm pad 3mm
0
16
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-2.5-V-THR_1x08_P2.50mm_Vertical
Terminal Block Phoenix PTSM-0,5-8-2.5-V-THR, vertical (cable from top), 8 pins, pitch 2.5mm, size 20.5x5mm^2, drill diamater 1.2mm, pad diameter 2mm, see http://www.produktinfo.conrad.com/datenblaetter/550000-574999/556444-da-01-de-LEITERPLATTENKL__PTSM_0_5__4_2_5_V_THR.pdf, script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix
THT Terminal Block Phoenix PTSM-0,5-8-2.5-V-THR vertical pitch 2.5mm size 20.5x5mm^2 drill 1.2mm pad 2mm
0
16
8
TerminalBlock_Phoenix
TerminalBlock_Phoenix_PTSM-0,5-8-HV-2.5-SMD_1x08-1MP_P2.50mm_Vertical
PhoenixContact PTSM0,5 8 HV 2,5mm vertical SMD spring clamp terminal block connector http://www.phoenixcontact.com/us/products/1778751/pdf
2.5mm vertical SMD spring clamp terminal block connector 
0
10
9
VL_Capacitors
C0402


0
2
2
VL_Capacitors
C0603


0
2
2
VL_Capacitors
C0805
Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
capacitor
0
2
2
VL_Capacitors
C1206
Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
VL_Capacitors
C1210
Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
VL_Capacitors
C1812
Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
VL_Capacitors
C2010
Capacitor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
VL_Capacitors
C2512
Capacitor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
capacitor
0
2
2
VL_Connectors
Barrel_Jack_SMT


0
4
2
VL_Connectors
GMX-SMT2-N-44


0
4
4
VL_Connectors
Header_1x02_P2.54mm


0
2
2
VL_Connectors
Header_1x03_P2.54mm
Through hole straight pin header, 1x03, 2.54mm pitch, single row
Through hole pin header THT 1x03 2.54mm single row
0
3
3
VL_Connectors
Header_1x04_P2.54mm


0
4
4
VL_Connectors
Hirose_DF1BZ-4DP-2.5DS


0
4
4
VL_Connectors
JST_ZH_5PIN_B5B-ZR-SM4-TF


0
7
6
VL_Connectors
JST_ZH_5PIN_S5B-ZR-SM4A-TF


0
7
6
VL_Connectors
PROGTEST_PROBE_EDGE_CONNECTOR


0
36
36
VL_Connectors
PROGTEST_TESTER_EDGE_SOCKET


0
36
36
VL_Connectors
PinHeader_1x04_P2.00mm_Vertical
Through hole straight pin header, 1x04, 2.00mm pitch, single row
Through hole pin header THT 1x04 2.00mm single row
0
4
4
VL_Connectors
PinHeader_1x04_P2.54mm_Vertical
Through hole straight pin header, 1x04, 2.54mm pitch, single row
Through hole pin header THT 1x04 2.54mm single row
0
4
4
VL_Connectors
PinHeader_1x05_P2.00mm_Vertical
Through hole straight pin header, 1x05, 2.00mm pitch, single row
Through hole pin header THT 1x05 2.00mm single row
0
5
5
VL_Connectors
PinHeader_1x05_P2.54mm_Vertical
Through hole straight pin header, 1x05, 2.54mm pitch, single row
Through hole pin header THT 1x05 2.54mm single row
0
5
5
VL_Connectors
PinHeader_1x06_P2.00mm_Vertical
Through hole straight pin header, 1x06, 2.00mm pitch, single row
Through hole pin header THT 1x06 2.00mm single row
0
6
6
VL_Connectors
PinHeader_1x06_P2.54mm_Vertical
Through hole straight pin header, 1x06, 2.54mm pitch, single row
Through hole pin header THT 1x06 2.54mm single row
0
6
6
VL_Connectors
PinHeader_1x36_P2.54mm_Vertical
Through hole straight pin header, 1x36, 2.54mm pitch, single row
Through hole pin header THT 1x36 2.54mm single row
0
36
36
VL_Connectors
PinHeader_1x36_P2.54mm_Vertical_CENTERED
Through hole straight pin header, 1x36, 2.54mm pitch, single row
Through hole pin header THT 1x36 2.54mm single row
0
36
36
VL_Connectors
PinHeader_2x07_P1.27mm_Vertical_SMD
surface-mounted straight pin header, 2x07, 1.27mm pitch, double rows
Surface mounted pin header SMD 2x07 1.27mm double row
0
14
14
VL_Connectors
PinSocket_1x05_P2.54mm_Horizontal
Through hole angled socket strip, 1x05, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated
Through hole angled socket strip THT 1x05 2.54mm single row
0
5
5
VL_Connectors
RPi_Connector


0
40
40
VL_Connectors
SWD_Connector_THT


0
5
5
VL_Connectors
SWD_Connector_for_PogoHeader


0
5
5
VL_Connectors
Solder_Pads_Thin_1x2


0
2
2
VL_Connectors
Sullins_SWR204-NRTN-D02-RA-GA


0
4
4
VL_Connectors
TerminalBlock_1x2_PhoenixContact_P3.5mm


0
2
2
VL_Connectors
TerminalBlock_1x4_PhoenixContact_P3.5mm


0
4
4
VL_Connectors
Testing_Probe_Socket


0
1
1
VL_Connectors
U.FL_TE_1909763-1


0
3
2
VL_Connectors
USB_C_Receptacle_GCT_USB4085
USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf
USB Type-C Receptacle Through-hole Right angle
0
20
17
VL_Connectors
WAGO_2060-452


0
4
2
VL_DFN_QFN
4-VDFN_2x2mm


0
4
4
VL_DFN_QFN
QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm
QFN, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf#page=34), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
25
21
VL_DFN_QFN
QFN-28_4x4mm_P0.5mm
QFN, 28 Pin (http://www.st.com/resource/en/datasheet/stm32f031k6.pdf#page=90), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
28
28
VL_DFN_QFN
QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm_ThermalVias
QFN, 36 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/36L_QFN_6x6_with_3_7x3_7_EP_Punch_Dimpled_4E_C04-0241A.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py
QFN DFN_QFN
0
63
37
VL_DFN_QFN
QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm


0
65
49
VL_DFN_QFN
ST_UFQFPN-20_3x3mm_P0.5mm
UFQFPN 20-lead, 3 x 3 mm, 0.5 mm pitch, ultra thin fine pitch quad flat package (http://www.st.com/resource/en/datasheet/stm8s003f3.pdf)
UFQFPN 0.5
0
20
20
VL_DFN_QFN
TDFN-8-1EP_2x2mm_P0.5mm


0
8
8
VL_DFN_QFN
TDFN-8-1EP_2x2mm_P0.5mm_EP0.8x1.2mm
TDFN, 8 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0168.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py
TDFN NoLead
0
13
9
VL_DFN_QFN
TDFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.4mm
TDFN, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/MCP6V66-Family-Data-Sheet-DS20006266A.pdf#page=35), generated with kicad-footprint-generator ipc_noLead_generator.py
TDFN NoLead
0
13
9
VL_DFN_QFN
Texas_S-PWQFN-N24_EP2.7x2.7mm
QFN, 24 Pin (http://www.ti.com/lit/ds/symlink/bq25601.pdf#page=54), generated with kicad-footprint-generator ipc_noLead_generator.py
QFN NoLead
0
29
25
VL_Diodes
D_SOD-323
SOD-323
SOD-323
0
2
2
VL_Diodes
D_SOD-323F
SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf
SOD-323F
0
2
2
VL_Diodes
D_SOD-923
https://www.onsemi.com/pub/Collateral/ESD9B-D.PDF#page=4
Diode SOD923
0
2
2
VL_Diodes
LED_0603


0
2
2
VL_Diodes
LED_ASMB-KTF0-0A306


0
4
4
VL_Diodes
LED_QLS6B-FKW-CNSNSF043


0
6
6
VL_Diodes
LED_UV275nm_Osram-SU-CULDN1.VC


0
9
3
VL_Diodes
LED_UV365nm_Wuerth-15335337AA350


0
7
3
VL_Diodes
RF-W2SA50TS-A39R


0
6
6
VL_Inductors
Coilcraft_XAL5050-153MEC


0
2
2
VL_Inductors
L0402
Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
VL_Inductors
L0603
Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
inductor
0
2
2
VL_Inductors
L0805
Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator
inductor
0
2
2
VL_Inductors
L_EPL2014


0
2
2
VL_Inductors
L_NR40xx


0
2
2
VL_LGA
LGA-12_2x2mm_P0.5mm
LGA12
lga land grid array
0
12
12
VL_LGA
LGA-16_3x3mm_P0.5mm_LayoutBorder3x5y
LGA, 16 Pin (http://www.st.com/resource/en/datasheet/lis331hh.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py
LGA NoLead
0
16
16
VL_Logos
OSHW-Logo2_7.3x6mm_SilkScreen
Open Source Hardware Symbol
Logo Symbol OSHW
0
0
0
VL_Logos
OSHW-Logo2_7.3x6mm_SilkScreen_no_text


0
0
0
VL_Logos
OSHW-Logo2_9.8x8mm_SilkScreen
Open Source Hardware Symbol
Logo Symbol OSHW
0
0
0
VL_Logos
OSHW-Logo_5.7x6mm_SilkScreen
Open Source Hardware Logo
Logo OSHW
0
0
0
VL_Logos
OSHW-Logo_7.5x8mm_SilkScreen
Open Source Hardware Logo
Logo OSHW
0
0
0
VL_Logos
OSHW-Logo_11.4x12mm_SilkScreen
Open Source Hardware Logo
Logo OSHW
0
0
0
VL_Logos
VL_Logo_12x10mm


0
0
0
VL_Other
0900FM15D0039


0
10
10
VL_Other
ANT_W3012_3


0
3
2
VL_Other
Breakaway_tab_holes


0
0
0
VL_Other
CMT-7525S-SMT-TR


0
4
4
VL_Other
EMI_Gasket_16.51x16.51mm


0
16
1
VL_Other
EMI_Gasket_20x20mm


0
20
1
VL_Other
F0603


0
2
2
VL_Other
F1206


0
2
2
VL_Other
Fiducial_0.5mm_Mask1.5mm
Circular Fiducial, 0.5mm bare copper, 1.5mm soldermask opening
fiducial
0
1
0
VL_Other
Fiducial_0.5mm_Mask1mm
Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)
fiducial
0
1
0
VL_Other
Fiducial_1.5mm_Mask3mm
Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening
fiducial
0
1
0
VL_Other
Fiducial_1.5mm_Mask4.5mm
Circular Fiducial, 1.5mm bare copper, 4.5mm soldermask opening
fiducial
0
1
0
VL_Other
Fiducial_1mm_Mask2mm
Circular Fiducial, 1mm bare copper, 2mm soldermask opening (Level A)
fiducial
0
1
0
VL_Other
Fiducial_1mm_Mask3mm
Circular Fiducial, 1mm bare copper, 3mm soldermask opening (recommended)
fiducial
0
1
0
VL_Other
LFB182G45CGFD436


0
3
3
VL_Other
MLPF-WB55-01E3


0
6
6
VL_Other
MODULE_STLINK-V3MODS


0
32
32
VL_Other
Meander_PCB_Antenna_2.4GHz


0
1
1
VL_Other
ProgTest_Tester_Module


0
14
14
VL_Other
PushButton_Omron-B3SE-1002P


0
4
4
VL_Other
RF_FORK


0
3
3
VL_Other
SB0603


0
2
2
VL_Other
SB0603_dual


0
4
3
VL_Other
SERIAL_NUMBER_SPACE


0
0
0
VL_Other
SIMCom_SIM800L


0
11
11
VL_Other
SW_KMS221GLFS


0
5
2
VL_Other
SW_KMS233GLFG


0
5
2
VL_Other
TEST_CHECKMARKS


0
0
0
VL_Other
TSNP-6-2


0
6
6
VL_Other
Tactile_Switch_6x6_SMT


0
4
2
VL_Other
Testpoint_SMD_1mm


0
1
1
VL_Other
Testpoint_SMD_2mm


0
1
1
VL_Other
VL_STLINK_MODULE


0
10
10
VL_Other
VL_TESTER_MODULE


0
10
10
VL_Other
soil_moisture_sensor_electrode


0
3
2
VL_QFP
LQFP-32_7x7mm_P0.8mm
LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
32
32
VL_QFP
LQFP-48_7x7mm_P0.5mm
LQFP, 48 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ltc2358-16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
LQFP QFP
0
48
48
VL_QFP
LQFP-64_10x10mm_P0.5mm
64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)
QFP 0.5
0
64
64
VL_QFP
LQFP-100_14x14mm_P0.5mm
LQFP100: plastic low profile quad flat package; 100 leads; body 14 x 14 x 1.4 mm (see NXP sot407-1_po.pdf and sot407-1_fr.pdf)
QFP 0.5
0
100
100
VL_QFP
LQFP-144_20x20mm_P0.5mm
144-Lead Plastic Low Profile Quad Flatpack (PL) - 20x20x1.40 mm Body [LQFP], 2.00 mm Footprint (see Microchip Packaging Specification 00000049BS.pdf)
QFP 0.5
0
144
144
VL_Resistors
R0402
Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
VL_Resistors
R0603


0
2
2
VL_Resistors
R0805


0
2
2
VL_Resistors
R1206
Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator
resistor
0
2
2
VL_Resistors
TRIMMER_10k_Bourns-PVG3K103C01R00


0
3
3
VL_SO
MSOP-10-1EP_3x3mm_P0.5mm_EP1.68x1.88mm
MSOP, 10 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3805fg.pdf#page=18), generated with kicad-footprint-generator ipc_gullwing_generator.py
MSOP SO
0
15
11
VL_SO
SOIC-8_3.9x4.9mm_P1.27mm
SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py
SOIC SO
0
8
8
VL_SO
SOT-223-3(TAB-pin-2)
module CMS SOT223 4 pins
CMS SOT
0
4
3
VL_SO
SSOP-28_5.3x10.2mm_P0.65mm
28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)
SSOP 0.65
0
28
28
VL_SON
Texas_VSON8


0
9
9
VL_SOT
SOT-23
3-pin SOT-23 package

0
3
3
VL_SOT
SOT-23-5
5-pin SOT-23 package
SOT-23-6
0
5
5
VL_SOT
SOT-26-6
6-pin SOT-23 package

0
6
6
VL_SOT
SOT-223-3(TAB-pin-2)
module CMS SOT223 4 pins
CMS SOT
0
4
3
VL_SOT
SOT-363_SC-70-6
SOT-363, SC-70-6
SOT-363 SC-70-6
0
6
6
VL_SOT
SOT−563-6


0
6
6
VL_Sensors
SCD4x


0
21
21
VL_Sensors
SGP4x


0
7
7
VL_Sensors
SHT3x


0
9
9
VL_Sensors
SHT4x


0
4
4
VL_Sensors
VL53L3CX


0
12
12
VL_Sensors
VL53L5CXV0GC


0
17
17
VL_Sensors
VL6180


0
12
12
VL_TO_SMD
TO-252-2(DPAK)


0
3
3
VL_TO_SMD
TO-263-2
TO-263 / D2PAK / DDPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO263/PG-TO263-3-1/
D2PAK DDPAK TO-263 D2PAK-3 TO-263-3 SOT-404
0
7
3
VL_TO_SMD
TO-263-2(D2PAK)


0
3
3
VL_XTALs
ABM8G


0
4
4
VL_XTALs
ECX-32


0
4
4
VL_XTALs
NX2012SA


0
2
2
VL_XTALs
NX2016SA


0
4
4
footprints
VL53L5CXV0GC&slash_1


0
17
17
